Altium Designer Pick and Place Locations
C:\Users\Public\Documents\Altium\UB66_SSCB_PB_DGTOLL_2P\Project Outputs for UB66_SSCB_PB_DGTOLL_2P_V1\Pick Place\Pick Place for SSCB_Combo JFET V1.1(Combo-FET).txt

========================================================================================================================
File Design Information:

Date:       21/07/25
Time:       06:31
Revision:   Not in VersionControl
Variant:    Combo-FET
Units used: mil

Designator Comment               Layer       Footprint              Center-X(mil) Center-Y(mil) Rotation Description                                                                                                                                        
R160       CRCW06030000Z0ED      TopLayer    RESC1608X50N           315.000       -3430.000     90       "0 Ohms Jumper Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200, Pulse Withstanding Thick Film"                                                
P1         5034800600            TopLayer    5034800600             324.599       -3574.597     0        "CONN, FLAT FLEX, R/A, 6-POS, 0.5mm, SMD"                                                                                                          
R164       CRCW06030000Z0ED      BottomLayer RESC1608X50N           -345.000      -3010.000     90       "0 Ohms Jumper Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200, Pulse Withstanding Thick Film"                                                
F5_2       FIDUCIAL              TopLayer    FID1                   -1990.000     -1665.440     270      "Fiducial 1mm"                                                                                                                                     
F4_1       FIDUCIAL              TopLayer    FID1                   2004.560      -190.000      270      "Fiducial 1mm"                                                                                                                                     
F5_1       FIDUCIAL              TopLayer    FID1                   1925.000      -190.000      270      "Fiducial 1mm"                                                                                                                                     
F5         FIDUCIAL              TopLayer    FID1                   -1774.560     -3600.000     0        "Fiducial 1mm"                                                                                                                                     
F4         FIDUCIAL              TopLayer    FID1                   -1695.000     -3620.000     0        "Fiducial 1mm"                                                                                                                                     
F3         FIDUCIAL              TopLayer    FID1                   1040.000      -3290.000     0        "Fiducial 1mm"                                                                                                                                     
F2         FIDUCIAL              TopLayer    FID1                   405.000       -3030.000     0        "Fiducial 1mm"                                                                                                                                     
C139       C0603C101F1GAC7867    TopLayer    CAPC1608X90N           790.000       -2265.000     0        "100 pF ±1% 100V Ceramic Capacitor C0G, NP0 0603 (1608 Metric)"                                                                                    
TP14       5001                  TopLayer    5000                   1615.000      -2644.084     0        "Black PC Test Point, Miniature Phosphor Bronze Silver Plating Through Hole Mounting Type"                                                         
S3         PTS636_SK25F_SMTR_LFS TopLayer    PTS636SK25FSMTRLFS     1298.289      -3252.146     180      "Tactile Switch SPST-NO Top Actuated Surface Mount"                                                                                                
R158       CRCW0603107RFKEA      BottomLayer RESC1608X50N           925.000       -2965.000     180      "107 Ohms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                         
R157       CRCW0603107RFKEA      BottomLayer RESC1608X50N           1110.000      -2830.000     0        "107 Ohms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                         
R153       CRCW0603107RFKEA      BottomLayer RESC1608X50N           690.000       -2915.000     270      "107 Ohms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                         
R152       CRCW0603107RFKEA      BottomLayer RESC1608X50N           1110.207      -2895.000     0        "107 Ohms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                         
TP12       5001                  TopLayer    5000                   1555.000      -2915.000     0        "Black PC Test Point, Miniature Phosphor Bronze Silver Plating Through Hole Mounting Type"                                                         
TP9        5001                  TopLayer    5000                   1555.000      -2790.000     0        "Black PC Test Point, Miniature Phosphor Bronze Silver Plating Through Hole Mounting Type"                                                         
S2         JS102011JCQN          TopLayer    JS102011JCQN           662.619       -2531.575     90       "Slide Switch SPDT Surface Mount"                                                                                                                  
S1         JS102011JCQN          TopLayer    JS102011JCQN           471.152       -2533.425     90       "Slide Switch SPDT Surface Mount"                                                                                                                  
U19        SN74LVC1G08DBVR       TopLayer    SOT95P280X145-5N       -70.000       -2730.000     270      "AND Gate IC 1 Channel SOT-23-5"                                                                                                                   
C128       CL10B104KB8NNNC       TopLayer    CAPC1608X90N           75.000        -2615.187     0        "0.1 µF ±10% 50V Ceramic Capacitor X7R 0603 (1608 Metric)"                                                                                         
U11        SN74LVC1G08DBVR       TopLayer    SOT95P280X145-5N       50.000        -2521.870     0        "AND Gate IC 1 Channel SOT-23-5"                                                                                                                   
R149       CRCW060310K0DHEAP     BottomLayer RESC1608X50N           1915.000      -2932.185     180      "10 kOhms ±0.5% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                       
R148       CRCW08054K70FKEA      TopLayer    RESC2012X50N           271.624       -2750.000     90       "4.7 kOhms ±1% 0.125W, 1/8W Chip Resistor 0805 (2012 Metric) Automotive AEC-Q200 Thick Film"                                                       
D18        LTST-C171GKT          TopLayer    LEDC2012X90N           185.000       -2750.000     270      "Green 569nm LED Indication - Discrete 2.1V 0805 (2012 Metric)"                                                                                    
C111       CL10B105KA8NNNC       BottomLayer CAPC1608X90N           1915.000      -2880.797     180      "1 µF ±10% 25V Ceramic Capacitor X7R 0603 (1608 Metric)"                                                                                           
C52        CL10B104KB8NNNC       TopLayer    CAPC1608X90N           75.000        -2404.734     270      "0.1 µF ±10% 50V Ceramic Capacitor X7R 0603 (1608 Metric)"                                                                                         
T40        ""                    TopLayer    TP_5002                565.000       -3209.657     180      Testpoint                                                                                                                                          
T39        ""                    TopLayer    TP_5002                590.764       -3248.666     180      Testpoint                                                                                                                                          
R24        CRCW06031K00FKEA      TopLayer    RESC1608X50N           580.000       -2995.000     90       "1 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                          
D17        LTST-C171GKT          TopLayer    LEDC2012X90N           507.746       -2980.000     90       "Green 569nm LED Indication - Discrete 2.1V 0805 (2012 Metric)"                                                                                    
R151       SMA-A0207FTDT10R      BottomLayer SMAA0207FTDT10R        140.000       -305.000      180      "10 Ohms ±1% 1W Chip Resistor MELF, 0207 Automotive AEC-Q200 Metal Film"                                                                           
R150       SMA-A0207FTDT10R      BottomLayer SMAA0207FTDT10R        140.000       -420.000      180      "10 Ohms ±1% 1W Chip Resistor MELF, 0207 Automotive AEC-Q200 Metal Film"                                                                           
C125       C2220C663KDGLCAUTO    BottomLayer CAPC5950X155N          -175.000      -365.000      180      "0.066 µF ±10% 1000V (1kV) Ceramic Capacitor C0G, NP0 2220 (5750 Metric)"                                                                          
T76        PROG_EN               BottomLayer TP_5002                -296.805      -3048.195     180      Testpoint                                                                                                                                          
T75        PROG_EN               BottomLayer TP_5002                -270.000      -2975.000     180      Testpoint                                                                                                                                          
T14        PROG_EN               TopLayer    TP_5002                -400.000      -3095.000     0        Testpoint                                                                                                                                          
L6         MU2029-301Y           BottomLayer IND_BOURNS_2029        -115.000      -2991.010     0        "300 Ohms @ 100 MHz 1 Power, Signal Line Ferrite Bead 0805 (2012 Metric) 500mA 300mOhm"                                                            
R147       CRCW0603107RFKEA      BottomLayer RESC1608X50N           793.957       -2915.000     270      "107 Ohms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                         
R146       CRCW0603107RFKEA      BottomLayer RESC1608X50N           741.979       -2915.000     270      "107 Ohms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                         
R144       CRCW0603107RFKEA      BottomLayer RESC1608X50N           90.000        -3185.936     0        "107 Ohms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                         
R143       CRCW0603107RFKEA      BottomLayer RESC1608X50N           90.000        -3030.000     0        "107 Ohms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                         
R142       CRCW0603107RFKEA      BottomLayer RESC1608X50N           90.000        -3133.957     0        "107 Ohms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                         
R141       CRCW0603107RFKEA      BottomLayer RESC1608X50N           90.000        -3081.979     0        "107 Ohms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                         
R138       CRCW0603107RFKEA      TopLayer    RESC1608X50N           1110.000      -2641.979     180      "107 Ohms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                         
R137       CRCW0603107RFKEA      TopLayer    RESC1608X50N           1110.000      -2590.000     180      "107 Ohms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                         
R135       CRCW0603107RFKEA      BottomLayer RESC1608X50N           845.935       -2915.000     270      "107 Ohms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                         
R134       CRCW0603107RFKEA      BottomLayer RESC1608X50N           950.000       -3065.000     180      "107 Ohms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                         
JP1        CRCW08050000Z0EAHP    TopLayer    RESC2012X60N           -935.000      -3230.000     90       "0 Ohms Jumper Chip Resistor 0805 (2012 Metric) Automotive AEC-Q200, Pulse Withstanding Thick Film"                                                
TP11       5001                  TopLayer    5000                   -1280.000     -3535.000     0        "Black PC Test Point, Miniature Phosphor Bronze Silver Plating Through Hole Mounting Type"                                                         
T74        PROG_EN               TopLayer    TP_5002                -1310.000     -3404.077     0        Testpoint                                                                                                                                          
T73        PROG_EN               BottomLayer TP_5002                -1190.000     -3175.000     180      Testpoint                                                                                                                                          
U1         TPSM863253RDXR        TopLayer    VREG_TPSM863253RDXR    -1265.000     -3280.532     0        "Non-Isolated PoL Module DC DC Converter 1 Output 3.3V 3A 3V - 17V Input"                                                                          
R110       CRCW06030000Z0ED      TopLayer    RESC1608X50N           -1110.000     -3238.504     90       "0 Ohms Jumper Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200, Pulse Withstanding Thick Film"                                                
R107       CRCW060362K0FKEA      TopLayer    RESC1608X50N           -1109.468     -3125.472     270      "62 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                         
C151       GRM31CR70J226KE19K    TopLayer    GRM31X                 -932.106      -3390.000     90       "22 µF ±10% 6.3V Ceramic Capacitor X7R 1206 (3216 Metric)"                                                                                         
C150       GRM31CR70J226KE19K    TopLayer    GRM31X                 -1100.000     -3390.000     90       "22 µF ±10% 6.3V Ceramic Capacitor X7R 1206 (3216 Metric)"                                                                                         
C33        06035A100C4T2A        TopLayer    CAPC1608X90N           -1054.084     -3235.000     90       "10 pF ±0.25pF 50V Ceramic Capacitor C0G, NP0 0603 (1608 Metric)"                                                                                  
C32        GRM31CR70J226KE19K    TopLayer    GRM31X                 -1016.053     -3390.000     270      "22 µF ±10% 6.3V Ceramic Capacitor X7R 1206 (3216 Metric)"                                                                                         
C29        GRM31CR70J226KE19K    BottomLayer GRM31X                 -1055.000     -3390.000     270      "22 µF ±10% 6.3V Ceramic Capacitor X7R 1206 (3216 Metric)"                                                                                         
C28        CL10B104KB8NNNC       TopLayer    CAPC1608X90N           -1460.000     -3170.000     0        "0.1 µF ±10% 50V Ceramic Capacitor X7R 0603 (1608 Metric)"                                                                                         
C23        CL31B106KAHNFNE       TopLayer    CAPC3216X180N          -1475.000     -3239.557     0        "10 µF ±10% 25V Ceramic Capacitor X7R 1206 (3216 Metric)"                                                                                          
C14        CL31B106KAHNFNE       TopLayer    CAPC3216X180N          -1475.000     -3325.000     0        "10 µF ±10% 25V Ceramic Capacitor X7R 1206 (3216 Metric)"                                                                                          
C5         GRM31CR70J226KE19K    BottomLayer GRM31X                 -971.053      -3390.000     270      "22 µF ±10% 6.3V Ceramic Capacitor X7R 1206 (3216 Metric)"                                                                                         
C4         06035A102GAT2A        BottomLayer CAPC1608X90N           70.207        -2880.000     180      "1000 pF ±2% 50V Ceramic Capacitor C0G, NP0 0603 (1608 Metric)"                                                                                    
Z5_Q4      TZM5225B-GS08         TopLayer    DIOMELF3515N           1632.136      -1170.000     90       "Zener Diode 3 V 500 mW ±5% Surface Mount SOD-80 MiniMELF"                                                                                         
Z5_Q3      TZM5225B-GS08         TopLayer    DIOMELF3515N           955.955       -1170.000     90       "Zener Diode 3 V 500 mW ±5% Surface Mount SOD-80 MiniMELF"                                                                                         
Z5_Q2      TZM5225B-GS08         TopLayer    DIOMELF3515N           -344.045      -1170.000     90       "Zener Diode 3 V 500 mW ±5% Surface Mount SOD-80 MiniMELF"                                                                                         
Z5_Q1      TZM5225B-GS08         TopLayer    DIOMELF3515N           -1019.045     -1170.000     90       "Zener Diode 3 V 500 mW ±5% Surface Mount SOD-80 MiniMELF"                                                                                         
RV7        SV275K10BL1           TopLayer    SV300K10BL1            1366.142      -68.898       90       "430 V 3.5 kA Varistor 1 Circuit Through Hole Radial"                                                                                              
RV6        SV275K10BL1           TopLayer    SV300K10BL1            1051.181      -68.898       90       "430 V 3.5 kA Varistor 1 Circuit Through Hole Radial"                                                                                              
RV5        SV275K10BL1           TopLayer    SV300K10BL1            736.220       -68.898       90       "430 V 3.5 kA Varistor 1 Circuit Through Hole Radial"                                                                                              
RV3        SV275K10BL1           TopLayer    SV300K10BL1            -736.221      -68.898       270      "430 V 3.5 kA Varistor 1 Circuit Through Hole Radial"                                                                                              
RV2        SV275K10BL1           TopLayer    SV300K10BL1            -1051.181     -68.898       270      "430 V 3.5 kA Varistor 1 Circuit Through Hole Radial"                                                                                              
RV1        SV275K10BL1           TopLayer    SV300K10BL1            -1366.142     -68.898       270      "430 V 3.5 kA Varistor 1 Circuit Through Hole Radial"                                                                                              
R82        SMA-A0207FTDT10R      TopLayer    SMAA0207FTDT10R        137.795       -708.661      180      "10 Ohms ±1% 1W Chip Resistor MELF, 0207 Automotive AEC-Q200 Metal Film"                                                                           
D42        SD0603S040S0R2        TopLayer    SD0603                 1125.000      -1610.000     0        "Diode 40 V 200mA Surface Mount 0603 (1608 Metric)"                                                                                                
D41        SD0603S040S0R2        TopLayer    SD0603                 -792.682      -1610.000     0        "Diode 40 V 200mA Surface Mount 0603 (1608 Metric)"                                                                                                
R77        SMA-A0207FTDT10R      TopLayer    SMAA0207FTDT10R        137.795       -590.551      180      "10 Ohms ±1% 1W Chip Resistor MELF, 0207 Automotive AEC-Q200 Metal Film"                                                                           
C147       C2220C663KDGLCAUTO    TopLayer    CAPC5950X155N          -177.165      -531.496      180      "0.066 µF ±10% 1000V (1kV) Ceramic Capacitor C0G, NP0 2220 (5750 Metric)"                                                                          
TP10       5001                  TopLayer    5000                   -842.667      -3160.000     0        "Black PC Test Point, Miniature Phosphor Bronze Silver Plating Through Hole Mounting Type"                                                         
T72        PROG_EN               BottomLayer TP_5002                1652.852      -2316.110     180      Testpoint                                                                                                                                          
T71        PROG_EN               BottomLayer TP_5002                1647.852      -2530.000     180      Testpoint                                                                                                                                          
T70        PROG_EN               TopLayer    TP_5002                1335.000      -2045.000     0        Testpoint                                                                                                                                          
T69        PROG_EN               BottomLayer TP_5002                1577.022      -1840.451     180      Testpoint                                                                                                                                          
T68        PROG_EN               BottomLayer TP_5002                -1585.000     -2065.000     180      Testpoint                                                                                                                                          
T67        PROG_EN               TopLayer    TP_5002                -1385.000     -2010.000     0        Testpoint                                                                                                                                          
T66        PROG_EN               BottomLayer TP_5002                1199.506      -1575.000     180      Testpoint                                                                                                                                          
T65        PROG_EN               BottomLayer TP_5002                446.253       -2668.747     180      Testpoint                                                                                                                                          
T64        PROG_EN               BottomLayer TP_5002                1330.000      -1535.000     180      Testpoint                                                                                                                                          
T63        PROG_EN               BottomLayer TP_5002                1110.000      -2129.904     90       Testpoint                                                                                                                                          
T62        PROG_EN               BottomLayer TP_5002                400.000       -2415.000     90       Testpoint                                                                                                                                          
T61        PROG_EN               BottomLayer TP_5002                957.500       -2197.500     90       Testpoint                                                                                                                                          
T60        PROG_EN               BottomLayer TP_5002                670.000       -2050.000     90       Testpoint                                                                                                                                          
T59        PROG_EN               BottomLayer TP_5002                800.494       -1580.000     90       Testpoint                                                                                                                                          
T58        PROG_EN               BottomLayer TP_5002                -340.000      -2820.000     90       Testpoint                                                                                                                                          
T57        PROG_EN               BottomLayer TP_5002                310.000       -2625.000     90       Testpoint                                                                                                                                          
T56        PROG_EN               BottomLayer TP_5002                -295.000      -2820.000     90       Testpoint                                                                                                                                          
T55        PROG_EN               TopLayer    TP_5002                -255.000      -2805.000     90       Testpoint                                                                                                                                          
T54        PROG_EN               BottomLayer TP_5002                -645.494      -1580.000     90       Testpoint                                                                                                                                          
T53        PROG_EN               BottomLayer TP_5002                -495.000      -1580.000     90       Testpoint                                                                                                                                          
T52        PROG_EN               BottomLayer TP_5002                -755.000      -2115.000     90       Testpoint                                                                                                                                          
T51        PROG_EN               BottomLayer TP_5002                -685.494      -2430.000     90       Testpoint                                                                                                                                          
T50        PROG_EN               BottomLayer TP_5002                -870.000      -2235.000     90       Testpoint                                                                                                                                          
T49        PROG_EN               BottomLayer TP_5002                -1120.000     -2105.000     90       Testpoint                                                                                                                                          
T48        PROG_EN               BottomLayer TP_5002                -1089.506     -1580.000     90       Testpoint                                                                                                                                          
T47        PROG_EN               TopLayer    TP_5002                -465.000      -2905.000     90       Testpoint                                                                                                                                          
T44        PROG_EN               BottomLayer TP_5002                125.000       -2480.000     180      Testpoint                                                                                                                                          
T43        PROG_EN               TopLayer    TP_5002                -5.000        -2400.000     0        Testpoint                                                                                                                                          
T42        PROG_EN               TopLayer    TP_5002                340.000       -2600.000     0        Testpoint                                                                                                                                          
T41        PROG_EN               BottomLayer TP_5002                -295.494      -2200.000     180      Testpoint                                                                                                                                          
T38        PROG_EN               BottomLayer TP_5002                291.125       -1863.087     180      Testpoint                                                                                                                                          
T37        PROG_EN               BottomLayer TP_5002                -226.256      -1831.256     180      Testpoint                                                                                                                                          
T36        PROG_EN               TopLayer    TP_5002                343.723       -2477.000     0        Testpoint                                                                                                                                          
T35        PROG_EN               BottomLayer TP_5002                335.000       -2150.000     180      Testpoint                                                                                                                                          
T34        PROG_EN               BottomLayer TP_5002                480.888       -2140.000     180      Testpoint                                                                                                                                          
T33_Q4     PROG_EN               TopLayer    TP_5002                1307.269      -1067.151     90       Testpoint                                                                                                                                          
T33_Q3     PROG_EN               TopLayer    TP_5002                631.088       -1067.151     90       Testpoint                                                                                                                                          
T33_Q2     PROG_EN               TopLayer    TP_5002                -668.912      -1067.151     90       Testpoint                                                                                                                                          
T33_Q1     PROG_EN               TopLayer    TP_5002                -1343.912     -1067.151     90       Testpoint                                                                                                                                          
T32_Q4     PROG_EN               TopLayer    TP_5002                1452.069      -1077.844     90       Testpoint                                                                                                                                          
T32_Q3     PROG_EN               TopLayer    TP_5002                775.888       -1077.844     90       Testpoint                                                                                                                                          
T32_Q2     PROG_EN               TopLayer    TP_5002                -524.112      -1077.844     90       Testpoint                                                                                                                                          
T32_Q1     PROG_EN               TopLayer    TP_5002                -1199.112     -1077.844     90       Testpoint                                                                                                                                          
T31_Q4     PROG_EN               TopLayer    TP_5002                1461.081      -1037.844     90       Testpoint                                                                                                                                          
T31_Q3     PROG_EN               TopLayer    TP_5002                784.899       -1037.844     90       Testpoint                                                                                                                                          
T31_Q2     PROG_EN               TopLayer    TP_5002                -515.101      -1037.844     90       Testpoint                                                                                                                                          
T31_Q1     PROG_EN               TopLayer    TP_5002                -1190.101     -1037.844     90       Testpoint                                                                                                                                          
T30        PROG_EN               TopLayer    TP_5002                -425.000      -2990.000     0        Testpoint                                                                                                                                          
T29        PROG_EN               TopLayer    TP_5002                -420.000      -3155.000     90       Testpoint                                                                                                                                          
T28        PROG_EN               TopLayer    TP_5002                820.000       -2345.000     90       Testpoint                                                                                                                                          
T27        PROG_EN               TopLayer    TP_5002                741.597       -1685.000     90       Testpoint                                                                                                                                          
T26        PROG_EN               TopLayer    TP_5002                -381.124      -1588.403     90       Testpoint                                                                                                                                          
T25        PROG_EN               TopLayer    TP_5002                1550.000      -1490.136     90       Testpoint                                                                                                                                          
T24        PROG_EN               TopLayer    TP_5002                -1485.000     -1495.000     90       Testpoint                                                                                                                                          
T23        PROG_EN               TopLayer    TP_5002                -1675.000     -1640.000     0        Testpoint                                                                                                                                          
T22        PROG_EN               TopLayer    TP_5002                1745.000      -1630.000     0        Testpoint                                                                                                                                          
T21        PROG_EN               TopLayer    TP_5002                -740.000      -1470.000     0        Testpoint                                                                                                                                          
T20        PROG_EN               TopLayer    TP_5002                1167.100      -1482.900     90       Testpoint                                                                                                                                          
T19        PROG_EN               TopLayer    TP_5002                -405.000      -1791.597     0        Testpoint                                                                                                                                          
T18        PROG_EN               TopLayer    TP_5002                2040.000      -1385.000     90       Testpoint                                                                                                                                          
T17        PROG_EN               TopLayer    TP_5002                -1980.612     -1390.000     90       Testpoint                                                                                                                                          
D40        BAV99-7-F             TopLayer    SOT96P240X110-3N       1275.000      -2210.000     0        "Diode Array 1 Pair Series Connection 75 V 300mA (DC) Surface Mount TO-236-3, SC-59, SOT-23-3"                                                     
D39        BAV99-7-F             TopLayer    SOT96P240X110-3N       -1490.000     -2090.000     90       "Diode Array 1 Pair Series Connection 75 V 300mA (DC) Surface Mount TO-236-3, SC-59, SOT-23-3"                                                     
U27        SN74LVC1G32DBVR       TopLayer    SOT95P280X145-5N       215.364       -2570.000     180      "OR Gate IC 1 Channel SOT-23-5"                                                                                                                    
D38        LTST-C171GKT          TopLayer    LEDC2012X90N           -140.000      -2492.254     180      "Green 569nm LED Indication - Discrete 2.1V 0805 (2012 Metric)"                                                                                    
C146       CL10B104KB8NNNC       TopLayer    CAPC1608X90N           25.000        -2750.000     270      "0.1 µF ±10% 50V Ceramic Capacitor X7R 0603 (1608 Metric)"                                                                                         
R131       CRCW08054K70FKEA      TopLayer    RESC2012X50N           -282.726      -2525.000     180      "4.7 kOhms ±1% 0.125W, 1/8W Chip Resistor 0805 (2012 Metric) Automotive AEC-Q200 Thick Film"                                                       
R128       CRCW0603107RFKEA      TopLayer    RESC1608X50N           1100.000      -3111.978     180      "107 Ohms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                         
R127       CRCW060310K0DHEAP     TopLayer    RESC1608X50N           1095.000      -3060.000     0        "10 kOhms ±0.5% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                       
C92        CL10B105KA8NNNC       BottomLayer CAPC1608X90N           583.612       -3000.000     270      "1 µF ±10% 25V Ceramic Capacitor X7R 0603 (1608 Metric)"                                                                                           
U18        AD8034ARZ             BottomLayer R_8_ADI-M              1425.000      -1845.000     270      "High bandwidth (50MHz) Low offset (200µV) Rail-to-rail 5V Op am"                                                                                  
U17        AD8034ARZ             BottomLayer R_8_ADI-M              -1410.000     -1845.000     270      "High bandwidth (50MHz) Low offset (200µV) Rail-to-rail 5V Op am"                                                                                  
U16        TSV792IYST            BottomLayer MINISO8_STM-M          -550.000      -2739.527     180      "High bandwidth (50MHz) Low offset (200µV) Rail-to-rail 5V Op am"                                                                                  
U15        TSV792IYST            BottomLayer MINISO8_STM-M          -120.500      -2695.000     180      "High bandwidth (50MHz) Low offset (200µV) Rail-to-rail 5V Op am"                                                                                  
U14        TSV792IYST            BottomLayer MINISO8_STM-M          630.000       -2445.000     270      "High bandwidth (50MHz) Low offset (200µV) Rail-to-rail 5V Op am"                                                                                  
U13        TSV792IYST            BottomLayer MINISO8_STM-M          -520.000      -2445.000     270      "High bandwidth (50MHz) Low offset (200µV) Rail-to-rail 5V Op am"                                                                                  
U12        TSV792IYST            BottomLayer MINISO8_STM-M          955.000       -1955.000     0        "High bandwidth (50MHz) Low offset (200µV) Rail-to-rail 5V Op am"                                                                                  
U10        TSV792IYST            BottomLayer MINISO8_STM-M          -910.000      -1955.000     0        "High bandwidth (50MHz) Low offset (200µV) Rail-to-rail 5V Op am"                                                                                  
U9         OPA837IDCKT           BottomLayer DCK5_TEX-M             -200.000      -2070.000     0        "Voltage Feedback Amplifier 1 Circuit Rail-to-Rail SC-70-5"                                                                                        
U7         TSV792IYST            BottomLayer MINISO8_STM-M          10.000        -2055.000     270      "High bandwidth (50MHz) Low offset (200µV) Rail-to-rail 5V Op am"                                                                                  
U6         TSV792IYST            BottomLayer MINISO8_STM-M          0.000         -1792.870     0        "High bandwidth (50MHz) Low offset (200µV) Rail-to-rail 5V Op am"                                                                                  
R35        CRCW08051K00JNEA      TopLayer    RESC2012X50N           1590.000      -1550.000     0        "1 kOhms ±5% 0.125W, 1/8W Chip Resistor 0805 (2012 Metric) Automotive AEC-Q200 Thick Film"                                                         
R34        CRCW08051K00JNEA      TopLayer    RESC2012X50N           -1525.000     -1555.000     180      "1 kOhms ±5% 0.125W, 1/8W Chip Resistor 0805 (2012 Metric) Automotive AEC-Q200 Thick Film"                                                         
TP8        5001                  TopLayer    5000                   -1020.000     -2830.000     0        "Black PC Test Point, Miniature Phosphor Bronze Silver Plating Through Hole Mounting Type"                                                         
TP7        5001                  TopLayer    5000                   1850.000      -2110.000     0        "Black PC Test Point, Miniature Phosphor Bronze Silver Plating Through Hole Mounting Type"                                                         
TP6        5001                  TopLayer    5000                   1965.000      -2110.000     0        "Black PC Test Point, Miniature Phosphor Bronze Silver Plating Through Hole Mounting Type"                                                         
TP5        5001                  TopLayer    5000                   -1975.000     -2495.000     0        "Black PC Test Point, Miniature Phosphor Bronze Silver Plating Through Hole Mounting Type"                                                         
TP4        5001                  TopLayer    5000                   -835.000      -3440.000     0        "Black PC Test Point, Miniature Phosphor Bronze Silver Plating Through Hole Mounting Type"                                                         
TP3        5001                  TopLayer    5000                   -1765.000     -2495.000     0        "Black PC Test Point, Miniature Phosphor Bronze Silver Plating Through Hole Mounting Type"                                                         
TP2        5001                  TopLayer    5000                   -1030.000     -2995.000     0        "Black PC Test Point, Miniature Phosphor Bronze Silver Plating Through Hole Mounting Type"                                                         
TP1        5001                  TopLayer    5000                   -729.825      -2845.634     0        "Black PC Test Point, Miniature Phosphor Bronze Silver Plating Through Hole Mounting Type"                                                         
GT1        CRCW12060000Z0EAHP    TopLayer    RESC3116X65N           0.000         -1160.000     90       "0 Ohms Jumper Chip Resistor 1206 (3216 Metric) Automotive AEC-Q200, Pulse Withstanding Thick Film"                                                
R6         CRCW060322K0FKEA      TopLayer    RESC1608X50N           110.000       -2805.000     90       "22 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                         
D16        BAV99-7-F             TopLayer    SOT96P240X110-3N       1447.274      -1544.715     0        "Diode Array 1 Pair Series Connection 75 V 300mA (DC) Surface Mount TO-236-3, SC-59, SOT-23-3"                                                     
D15        BAV99-7-F             TopLayer    SOT96P240X110-3N       -1375.000     -1555.000     180      "Diode Array 1 Pair Series Connection 75 V 300mA (DC) Surface Mount TO-236-3, SC-59, SOT-23-3"                                                     
D34        BAV99-7-F             TopLayer    SOT96P240X110-3N       1375.000      -1780.000     90       "Diode Array 1 Pair Series Connection 75 V 300mA (DC) Surface Mount TO-236-3, SC-59, SOT-23-3"                                                     
D32        BAV99-7-F             TopLayer    SOT96P240X110-3N       1515.000      -1780.000     90       "Diode Array 1 Pair Series Connection 75 V 300mA (DC) Surface Mount TO-236-3, SC-59, SOT-23-3"                                                     
D30        BAV99-7-F             TopLayer    SOT96P240X110-3N       -1519.774     -1790.000     90       "Diode Array 1 Pair Series Connection 75 V 300mA (DC) Surface Mount TO-236-3, SC-59, SOT-23-3"                                                     
D29        BAV99-7-F             TopLayer    SOT96P240X110-3N       -1380.000     -1790.000     90       "Diode Array 1 Pair Series Connection 75 V 300mA (DC) Surface Mount TO-236-3, SC-59, SOT-23-3"                                                     
D25        BAV99-7-F             TopLayer    SOT96P240X110-3N       1232.293      -2025.000     90       "Diode Array 1 Pair Series Connection 75 V 300mA (DC) Surface Mount TO-236-3, SC-59, SOT-23-3"                                                     
D24        BAV99-7-F             TopLayer    SOT96P240X110-3N       -610.000      -2025.000     90       "Diode Array 1 Pair Series Connection 75 V 300mA (DC) Surface Mount TO-236-3, SC-59, SOT-23-3"                                                     
D23        BAV99-7-F             TopLayer    SOT96P240X110-3N       657.205       -2043.661     90       "Diode Array 1 Pair Series Connection 75 V 300mA (DC) Surface Mount TO-236-3, SC-59, SOT-23-3"                                                     
D22        BAV99-7-F             TopLayer    SOT96P240X110-3N       -1200.000     -2045.000     90       "Diode Array 1 Pair Series Connection 75 V 300mA (DC) Surface Mount TO-236-3, SC-59, SOT-23-3"                                                     
D7         BAV99-7-F             BottomLayer SOT96P240X110-3N       435.000       -1941.958     270      "Diode Array 1 Pair Series Connection 75 V 300mA (DC) Surface Mount TO-236-3, SC-59, SOT-23-3"                                                     
R99        CRCW040227R0FKEDC     BottomLayer RESC1005X35N           1655.000      -2485.227     180      "27 Ohms ±1% 0.063W, 1/16W Chip Resistor 0402 (1005 Metric) Thick Film"                                                                            
R98        CRCW040227R0FKEDC     BottomLayer RESC1005X35N           1650.000      -2358.258     180      "27 Ohms ±1% 0.063W, 1/16W Chip Resistor 0402 (1005 Metric) Thick Film"                                                                            
L3         0402DC-1N2XJRW        TopLayer    0402DC1N2XJRW          865.000       -3366.988     180      "1.2 nH Unshielded Wirewound Inductor 980 mA 125mOhm Max 0402 (1005 Metric)"                                                                       
C113       GJM1555C1H120JB01D    TopLayer    CAPC1005X55N           935.000       -3030.000     180      "12 pF ±5% 50V Ceramic Capacitor C0G, NP0 0402 (1005 Metric)"                                                                                      
C112       GJM1555C1H120JB01D    TopLayer    CAPC1005X55N           1000.000      -3115.000     90       "12 pF ±5% 50V Ceramic Capacitor C0G, NP0 0402 (1005 Metric)"                                                                                      
C41        C0603C101F1GAC7867    TopLayer    CAPC1608X90N           -1060.000     -2250.000     0        "100 pF ±1% 100V Ceramic Capacitor C0G, NP0 0603 (1608 Metric)"                                                                                    
C38        C0603C101F1GAC7867    TopLayer    CAPC1608X90N           -960.000      -2250.000     180      "100 pF ±1% 100V Ceramic Capacitor C0G, NP0 0603 (1608 Metric)"                                                                                    
C37        C0603C101F1GAC7867    TopLayer    CAPC1608X90N           890.000       -2265.000     0        "100 pF ±1% 100V Ceramic Capacitor C0G, NP0 0603 (1608 Metric)"                                                                                    
C36        C0603C101F1GAC7867    TopLayer    CAPC1608X90N           -850.000      -2250.000     0        "100 pF ±1% 100V Ceramic Capacitor C0G, NP0 0603 (1608 Metric)"                                                                                    
C35        C0603C101F1GAC7867    TopLayer    CAPC1608X90N           1005.000      -2265.000     180      "100 pF ±1% 100V Ceramic Capacitor C0G, NP0 0603 (1608 Metric)"                                                                                    
C34        CL31B475KBHNFNE       TopLayer    CAPC3216X180N          -455.138      -2195.000     90       "4.7 µF ±10% 50V Ceramic Capacitor X7R 1206 (3216 Metric)"                                                                                         
C31        CL31B475KBHNFNE       BottomLayer CAPC3216X180N          960.000       -1710.000     270      "4.7 µF ±10% 50V Ceramic Capacitor X7R 1206 (3216 Metric)"                                                                                         
C30        CL31B475KBHNFNE       BottomLayer CAPC3216X180N          1045.443      -1710.000     270      "4.7 µF ±10% 50V Ceramic Capacitor X7R 1206 (3216 Metric)"                                                                                         
C27        CL31B475KBHNFNE       BottomLayer CAPC3216X180N          -825.000      -1710.000     270      "4.7 µF ±10% 50V Ceramic Capacitor X7R 1206 (3216 Metric)"                                                                                         
C26        CL31B475KBHNFNE       BottomLayer CAPC3216X180N          -910.443      -1710.000     270      "4.7 µF ±10% 50V Ceramic Capacitor X7R 1206 (3216 Metric)"                                                                                         
C17        CL31B475KBHNFNE       TopLayer    CAPC3216X180N          443.711       -1645.000     180      "4.7 µF ±10% 50V Ceramic Capacitor X7R 1206 (3216 Metric)"                                                                                         
C16        CL31B475KBHNFNE       TopLayer    CAPC3216X180N          -405.000      -1690.000     270      "4.7 µF ±10% 50V Ceramic Capacitor X7R 1206 (3216 Metric)"                                                                                         
C12        CL31B475KBHNFNE       TopLayer    CAPC3216X180N          640.000       -1705.000     0        "4.7 µF ±10% 50V Ceramic Capacitor X7R 1206 (3216 Metric)"                                                                                         
C11        CL31B475KBHNFNE       TopLayer    CAPC3216X180N          640.000       -1790.443     0        "4.7 µF ±10% 50V Ceramic Capacitor X7R 1206 (3216 Metric)"                                                                                         
C10        CL31B475KBHNFNE       TopLayer    CAPC3216X180N          -1214.813     -1875.886     180      "4.7 µF ±10% 50V Ceramic Capacitor X7R 1206 (3216 Metric)"                                                                                         
C9         CL31B475KBHNFNE       TopLayer    CAPC3216X180N          -1215.000     -1790.443     180      "4.7 µF ±10% 50V Ceramic Capacitor X7R 1206 (3216 Metric)"                                                                                         
C8         CL31B475KBHNFNE       TopLayer    CAPC3216X180N          -1215.000     -1705.000     180      "4.7 µF ±10% 50V Ceramic Capacitor X7R 1206 (3216 Metric)"                                                                                         
C7         CL10B104KB8NNNC       BottomLayer CAPC1608X90N           865.000       -1729.203     0        "0.1 µF ±10% 50V Ceramic Capacitor X7R 0603 (1608 Metric)"                                                                                         
C6         CL10B104KB8NNNC       BottomLayer CAPC1608X90N           -1002.382     -1770.797     0        "0.1 µF ±10% 50V Ceramic Capacitor X7R 0603 (1608 Metric)"                                                                                         
C2         CL10B104KB8NNNC       BottomLayer CAPC1608X90N           865.000       -1780.000     0        "0.1 µF ±10% 50V Ceramic Capacitor X7R 0603 (1608 Metric)"                                                                                         
C1         CL10B104KB8NNNC       BottomLayer CAPC1608X90N           -1002.382     -1720.000     0        "0.1 µF ±10% 50V Ceramic Capacitor X7R 0603 (1608 Metric)"                                                                                         
X2         ABS06-32.768KHZ-9-T   TopLayer    2012                   705.000       -3280.000     180      "32.768 kHz ±20ppm Crystal 9pF 90 kOhms 2-SMD, No Lead"                                                                                            
X1         E1SB32E001501E        TopLayer    BT-XTAL_2016           935.000       -3105.000     90       "XTAL, 32MHz, ±10PPM, 9pF, 60 OHM, 4-SMD"                                                                                                          
USB1       USB4110-GF-A          TopLayer    USB_TYPEC-SMD          1879.291      -2425.000     90       "CONN, USB2.0, TYP C, R/A, 24 POS, SMD"                                                                                                            
U26        FT230XS-R             TopLayer    FT230XS                1600.000      -2420.000     90       "IC USB SERIAL BASIC UART 16SSOP"                                                                                                                  
U25        ISO7220MDR            TopLayer    SOIC127P600X175-8N     1325.000      -2865.000     180      "General Purpose Digital Isolator 2500Vrms 2 Channel 150Mbps 25kV/µs CMTI 8-SOIC (0.154", 3.90mm Width)"                                           
U22        ISO7221MDR            TopLayer    SOIC127P600X175-8N     1325.000      -2615.000     0        "General Purpose Digital Isolator 2500Vrms 2 Channel 150Mbps 25kV/µs CMTI 8-SOIC (0.154", 3.90mm Width)"                                           
U21        QPG6105               TopLayer    QPG6105_QFN32          720.000       -3130.000     180      "LOW POWER COMM CONTROLLER"                                                                                                                        
U8         TLV1702AIDGKR         BottomLayer DGK0008A_M             -160.000      -2385.181     180      "Comparator General Purpose Open-Collector 8-VSSOP"                                                                                                
U5         TLV3201AIDBVR         BottomLayer SOT95P280X145-5N       250.000       -2325.787     90       "Comparator General Purpose Push-Pull SOT-23-5"                                                                                                    
U4         MCP6V76UT-E/OT        BottomLayer SOT95P280X145-5N       233.415       -2075.000     270      "IC OPAMP ZER-DRIFT 1CIRC SOT23-5"                                                                                                                 
U3         UCC21750QDWQ1         TopLayer    SOIC127P1030X265-16N   -905.512      -1968.504     270      "10A Gate Driver Capacitive Coupling 5700Vrms 1 Channel 16-SOIC"                                                                                   
U2         UCC21750QDWQ1         TopLayer    SOIC127P1030X265-16N   944.882       -1968.504     270      "10A Gate Driver Capacitive Coupling 5700Vrms 1 Channel 16-SOIC"                                                                                   
T16        SSN/SWIO              TopLayer    TP_5002                1080.000      -2775.000     0        Testpoint                                                                                                                                          
T15        SSN/SWIO              TopLayer    TP_5002                1115.000      -2960.000     0        Testpoint                                                                                                                                          
T10        GND_HV                TopLayer    TP_5002                1135.000      -2745.000     90       Testpoint                                                                                                                                          
T9         ""                    TopLayer    TP_5002                1064.274      -2970.000     0        Testpoint                                                                                                                                          
T8         SSN/SWIO              TopLayer    TP_5002                1120.000      -2695.000     0        Testpoint                                                                                                                                          
T7         RESETN                TopLayer    TP_5002                850.000       -2675.000     90       Testpoint                                                                                                                                          
T6         MISO/UART-TX          TopLayer    TP_5002                1025.000      -2645.000     0        Testpoint                                                                                                                                          
T5         MOSI/UART-RX          TopLayer    TP_5002                1027.736      -2590.000     90       Testpoint                                                                                                                                          
T4         SCLK/SWCLK            TopLayer    TP_5002                720.000       -2850.000     0        Testpoint                                                                                                                                          
T3         SSN/SWIO              TopLayer    TP_5002                675.000       -2990.000     0        Testpoint                                                                                                                                          
T2         PROG_EN               TopLayer    TP_5002                1035.000      -2740.000     90       Testpoint                                                                                                                                          
T1         SSN/SWIO              TopLayer    TP_5002                1120.000      -2535.000     0        Testpoint                                                                                                                                          
SW2        GT11MSABETR           TopLayer    GT11MSABETR            1833.160      -2850.000     180      "Toggle Switch SPDT Surface Mount, Right Angle"                                                                                                    
SW1_Q4     UG4SC075005L8S        BottomLayer UJ4SC075005L8S_MD      1330.906      -874.409      180      "Dual gate TOLL package"                                                                                                                           
SW1_Q3     UG4SC075005L8S        BottomLayer UJ4SC075005L8S_MD      654.724       -874.409      180      "Dual gate TOLL package"                                                                                                                           
SW1_Q2     UG4SC075005L8S        BottomLayer UJ4SC075005L8S_MD      -645.276      -874.409      180      "Dual gate TOLL package"                                                                                                                           
SW1_Q1     UG4SC075005L8S        BottomLayer UJ4SC075005L8S_MD      -1320.276     -874.409      180      "Dual gate TOLL package"                                                                                                                           
R126       CRCW060310K0DHEAP     BottomLayer RESC1608X50N           1915.000      -2778.612     180      "10 kOhms ±0.5% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                       
R125       CRCW0603120RFKEA      BottomLayer RESC1608X50N           1810.000      -2780.000     0        "120 Ohms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                         
R124       CRCW060310K0DHEAP     TopLayer    RESC1608X50N           1110.000      -2890.000     0        "10 kOhms ±0.5% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                       
R123       CRCW0603120RFKEA      BottomLayer RESC1608X50N           1810.000      -2930.000     0        "120 Ohms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                         
R122       CRCW060310K0DHEAP     TopLayer    RESC1608X50N           1110.000      -2835.000     180      "10 kOhms ±0.5% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                       
R121       CRCW060330K0FKEA      TopLayer    RESC1608X50N           -1057.490     -3125.000     90       "30 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                         
R120       CRCW06031K00FKEA      BottomLayer RESC1608X50N           -1460.000     -2590.000     180      "1 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                          
R119       CRCW06033K30FKEA      BottomLayer RESC1608X50N           -1400.000     -2675.000     270      "3.3 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                        
R118       CRCW080510K0FKEA      TopLayer    RESC2012X50N           -1540.626     -2995.000     270      "10 kOhms ±1% 0.125W, 1/8W Chip Resistor 0805 (2012 Metric) Automotive AEC-Q200 Thick Film"                                                        
R117       CRCW08054K70FKEA      TopLayer    RESC2012X50N           -1415.000     -3430.000     0        "4.7 kOhms ±1% 0.125W, 1/8W Chip Resistor 0805 (2012 Metric) Automotive AEC-Q200 Thick Film"                                                       
R115       CRCW08054K70FKEA      TopLayer    RESC2012X50N           -662.726      -3040.000     180      "4.7 kOhms ±1% 0.125W, 1/8W Chip Resistor 0805 (2012 Metric) Automotive AEC-Q200 Thick Film"                                                       
R114       CRCW060310K0DHEAP     BottomLayer RESC1608X50N           -595.000      -3045.000     180      "10 kOhms ±0.5% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                       
R113       CRCW060310K0DHEAP     BottomLayer RESC1608X50N           -600.000      -3130.000     180      "10 kOhms ±0.5% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                       
R112       CRCW060310K0FKEAC     BottomLayer RESC1608X55N           1380.000      -2080.000     270      "10 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Thick Film"                                                                             
R111       CRCW06031K00FKEA      BottomLayer RESC1608X50N           1449.442      -2062.994     90       "1 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                          
R109       CRCW060310K0FKEAC     BottomLayer RESC1608X55N           -1455.000     -2090.000     270      "10 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Thick Film"                                                                             
R108       CRCW06031K00FKEA      BottomLayer RESC1608X50N           -1386.388     -2090.000     90       "1 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                          
R106       CRCW06032K00FKEA      BottomLayer RESC1608X50N           1296.978      -1615.000     270      "2 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                          
R104       CRCW06032K00FKEA      BottomLayer RESC1608X50N           700.000       -1615.000     270      "2 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                          
R102       CRCW06032K00FKEA      BottomLayer RESC1608X50N           -545.000      -1615.000     270      "2 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                          
R100       CRCW04025K10FKED      BottomLayer RESC1005X40N           1690.000      -2555.118     90       "5.1 kOhms ±1% 0.063W, 1/16W Chip Resistor 0402 (1005 Metric) Automotive AEC-Q200 Thick Film"                                                      
R97        CRCW04025K10FKED      BottomLayer RESC1005X40N           1695.000      -2288.366     90       "5.1 kOhms ±1% 0.063W, 1/16W Chip Resistor 0402 (1005 Metric) Automotive AEC-Q200 Thick Film"                                                      
R96        CRCW06032K00FKEA      BottomLayer RESC1608X50N           -1190.000     -1615.000     270      "2 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                          
R94        CRCW06030000Z0ED      BottomLayer RESC1608X50N           1130.000      -2025.000     270      "0 Ohms Jumper Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200, Pulse Withstanding Thick Film"                                                
R93        CRCW0603107RFKEA      BottomLayer RESC1608X50N           605.000       -2617.494     180      "107 Ohms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                         
R92        CRCW06032K00FKEA      BottomLayer RESC1608X50N           507.967       -2455.000     270      "2 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                          
R91        CRCW06032K00FKEA      BottomLayer RESC1608X50N           1245.000      -1615.000     270      "2 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                          
R90        CRCW060310K0DHEAP     TopLayer    RESC1608X50N           -325.000      -2756.979     0        "10 kOhms ±0.5% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                       
R89        CRCW06031K00FKEA      BottomLayer RESC1608X50N           507.967       -2345.000     270      "1 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                          
R88        CRCW06030000Z0ED      BottomLayer RESC1608X50N           770.000       -2025.000     270      "0 Ohms Jumper Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200, Pulse Withstanding Thick Film"                                                
R87        CRCW06032K00FKEA      BottomLayer RESC1608X50N           1020.000      -2130.000     180      "2 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                          
R86        CRCW06032K00FKEA      BottomLayer RESC1608X50N           455.988       -2455.000     270      "2 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                          
R85        CRCW06032K00FKEA      BottomLayer RESC1608X50N           895.000       -2135.000     0        "2 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                          
R84        CRCW06032K00FKEA      BottomLayer RESC1608X50N           755.000       -1615.000     270      "2 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                          
R83        CRCW060310K0FKEAC     BottomLayer RESC1608X55N           1577.022      -1735.000     270      "10 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Thick Film"                                                                             
R81        CRCW060310K0FKEAC     BottomLayer RESC1608X55N           1630.000      -1626.034     180      "10 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Thick Film"                                                                             
R80        CRCW0603107RFKEA      TopLayer    RESC1608X50N           1385.000      -2085.000     270      "107 Ohms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                         
R79        CRCW060310K0FKEAC     BottomLayer RESC1608X55N           1577.022      -1920.000     270      "10 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Thick Film"                                                                             
R78        CRCW060310K0FKEAC     BottomLayer RESC1608X55N           1630.000      -1565.000     180      "10 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Thick Film"                                                                             
R76        CRCW0603107RFKEA      TopLayer    RESC1608X50N           -1485.000     -1955.000     90       "107 Ohms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                         
R75        CRCW060310K0FKEAC     TopLayer    RESC1608X55N           -1395.000     -1950.000     0        "10 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Thick Film"                                                                             
R74        CRCW060310K0FKEAC     BottomLayer RESC1608X55N           -1577.175     -1740.000     270      "10 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Thick Film"                                                                             
R73        CRCW060310K0FKEAC     BottomLayer RESC1608X55N           -1570.000     -1646.034     0        "10 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Thick Film"                                                                             
R72        CRCW060310K0FKEAC     BottomLayer RESC1608X55N           -1570.000     -1585.000     0        "10 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Thick Film"                                                                             
R71        CRCW060310K0DHEAP     BottomLayer RESC1608X50N           -320.000      -2720.000     0        "10 kOhms ±0.5% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                       
R70        CRCW06033K30FKEA      BottomLayer RESC1608X50N           -119.528      -2806.994     180      "3.3 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                        
R69        CRCW06032K00FKEA      BottomLayer RESC1608X50N           -830.000      -2130.000     180      "2 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                          
R68        CRCW0603107RFKEA      BottomLayer RESC1608X50N           -325.000      -2771.979     0        "107 Ohms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                         
R67        CRCW06033K30FKEA      TopLayer    RESC1608X50N           -325.000      -2705.000     0        "3.3 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                        
R66        CRCW0603107RFKEA      BottomLayer RESC1608X50N           -30.000       -2880.000     180      "107 Ohms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                         
R65        CRCW06032K00FKEA      BottomLayer RESC1608X50N           -408.006      -2470.000     270      "2 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                          
R64        CRCW06032K00FKEA      BottomLayer RESC1608X50N           -970.000      -2130.000     0        "2 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                          
R63        CRCW06032K00FKEA      BottomLayer RESC1608X50N           -600.000      -1615.000     270      "2 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                          
R62        CRCW06031K00FKEA      BottomLayer RESC1608X50N           -642.033      -2350.000     270      "1 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                          
R61        CRCW06030000Z0ED      BottomLayer RESC1608X50N           -720.000      -2030.000     270      "0 Ohms Jumper Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200, Pulse Withstanding Thick Film"                                                
R60        CRCW0603107RFKEA      BottomLayer RESC1608X50N           -490.000      -2617.494     0        "107 Ohms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                         
R59        CRCW06032K00FKEA      BottomLayer RESC1608X50N           -640.000      -2455.000     270      "2 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                          
R58        CRCW06030000Z0ED      BottomLayer RESC1608X50N           -1088.612     -2025.000     270      "0 Ohms Jumper Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200, Pulse Withstanding Thick Film"                                                
R57        CRCW060310K0DHEAP     TopLayer    RESC1608X50N           -510.000      -2751.979     0        "10 kOhms ±0.5% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                       
R56        CRCW06033K30FKEA      TopLayer    RESC1608X50N           -560.000      -2700.000     0        "3.3 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                        
R55        CRCW06032K00FKEA      BottomLayer RESC1608X50N           -1135.000     -1615.000     270      "2 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                          
R54        CRCW06031K00FKEA      BottomLayer RESC1608X50N           -80.000       -2505.000     180      "1 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                          
R53        CRCW060310K0DHEAP     BottomLayer RESC1608X50N           -220.000      -2175.000     0        "10 kOhms ±0.5% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                       
R52        CRCW06032K00FKEA      BottomLayer RESC1608X50N           -120.000      -1945.000     90       "2 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                          
R51        CRCW06038K06FKEA      BottomLayer RESC1608X50N           -215.000      -2505.000     180      "8.06 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                       
R50        CRCW06031M00FKEA      BottomLayer RESC1608X50N           -321.978      -2505.000     0        "1 MOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                          
R49        CRCW06031K00FKEA      BottomLayer RESC1608X50N           -326.978      -2277.494     180      "1 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                          
R48        CRCW0603120RFKEA      BottomLayer RESC1608X50N           -250.000      -2251.978     270      "120 Ohms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                         
R47        CRCW06032K00FKEA      BottomLayer RESC1608X50N           -281.978      -1945.000     90       "2 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                          
R46        CRCW060310K0DHEAP     TopLayer    RESC1608X50N           -260.000      -2420.000     180      "10 kOhms ±0.5% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                       
R45        CRCW060310K0DHEAP     BottomLayer RESC1608X50N           43.612        -2252.494     90       "10 kOhms ±0.5% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                       
R44        CRCW06031K00FKEA      BottomLayer RESC1608X50N           50.000        -2465.000     180      "1 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                          
R43        CRCW060310K0DHEAP     BottomLayer RESC1608X50N           -230.000      -1945.000     90       "10 kOhms ±0.5% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                       
R42        CRCW060310K0DHEAP     BottomLayer RESC1608X50N           -20.000       -2252.494     90       "10 kOhms ±0.5% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                       
R41        CRCW06030000Z0ED      TopLayer    RESC1608X50N           -1041.162     -1605.000     90       "0 Ohms Jumper Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200, Pulse Withstanding Thick Film"                                                
R40        CRCW08056R80FKEAHP    TopLayer    RESC2012X60N           -976.782      -1610.000     90       "6.8 Ohms ±1% 0.5W, 1/2W Chip Resistor 0805 (2012 Metric) Automotive AEC-Q200, Pulse Withstanding Thick Film"                                      
R39        CRCW08056R80FKEAHP    TopLayer    RESC2012X60N           -900.000      -1610.000     90       "6.8 Ohms ±1% 0.5W, 1/2W Chip Resistor 0805 (2012 Metric) Automotive AEC-Q200, Pulse Withstanding Thick Film"                                      
R38        CRCW08056R80FKEAHP    TopLayer    RESC2012X60N           1014.360      -1610.000     90       "6.8 Ohms ±1% 0.5W, 1/2W Chip Resistor 0805 (2012 Metric) Automotive AEC-Q200, Pulse Withstanding Thick Film"                                      
R37        CRCW08056R80FKEAHP    TopLayer    RESC2012X60N           937.578       -1610.000     90       "6.8 Ohms ±1% 0.5W, 1/2W Chip Resistor 0805 (2012 Metric) Automotive AEC-Q200, Pulse Withstanding Thick Film"                                      
R36        CRCW06030000Z0ED      TopLayer    RESC1608X50N           873.198       -1605.000     90       "0 Ohms Jumper Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200, Pulse Withstanding Thick Film"                                                
R33        CRCW08052K21FKEA      TopLayer    RESC2012X50N           1130.000      -1545.000     180      "2.21 kOhms ±1% 0.125W, 1/8W Chip Resistor 0805 (2012 Metric) Automotive AEC-Q200 Thick Film"                                                      
R32        CRCW08052K21FKEA      TopLayer    RESC2012X50N           -790.000      -1545.000     180      "2.21 kOhms ±1% 0.125W, 1/8W Chip Resistor 0805 (2012 Metric) Automotive AEC-Q200 Thick Film"                                                      
R31        CRCW06031M00FKEA      BottomLayer RESC1608X50N           50.000        -2350.000     180      "1 MOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                          
R30        SMA-A0207FTDT10R      TopLayer    SMAA0207FTDT10R        137.795       -472.441      180      "10 Ohms ±1% 1W Chip Resistor MELF, 0207 Automotive AEC-Q200 Metal Film"                                                                           
R29        CRCW06031K00FKEA      BottomLayer RESC1608X50N           -328.711      -2425.000     90       "1 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                          
R28_Q4     CRCW060310K0FKEA      TopLayer    RESC1608X50N           1381.575      -1041.457     0        "10 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                         
R28_Q3     CRCW060310K0FKEA      TopLayer    RESC1608X50N           705.394       -1041.457     0        "10 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                         
R28_Q2     CRCW060310K0FKEA      TopLayer    RESC1608X50N           -594.606      -1041.457     0        "10 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                         
R28_Q1     CRCW060310K0FKEA      TopLayer    RESC1608X50N           -1269.606     -1041.457     0        "10 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                         
R27_Q4     CRCW060310K0FKEA      TopLayer    RESC1608X50N           1531.575      -1041.457     180      "10 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                         
R27_Q3     CRCW060310K0FKEA      TopLayer    RESC1608X50N           855.394       -1041.457     180      "10 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                         
R27_Q2     CRCW060310K0FKEA      TopLayer    RESC1608X50N           -444.606      -1041.457     180      "10 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                         
R27_Q1     CRCW060310K0FKEA      TopLayer    RESC1608X50N           -1119.606     -1041.457     180      "10 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                         
R26_Q4     CRCW08054R70FKEA      TopLayer    RESC2012X50N           1353.012      -1187.844     90       "4.7 Ohms ±1% 0.125W, 1/8W Chip Resistor 0805 (2012 Metric) Automotive AEC-Q200 Thick Film"                                                        
R26_Q3     CRCW08054R70FKEA      TopLayer    RESC2012X50N           676.831       -1187.844     90       "4.7 Ohms ±1% 0.125W, 1/8W Chip Resistor 0805 (2012 Metric) Automotive AEC-Q200 Thick Film"                                                        
R26_Q2     CRCW08054R70FKEA      TopLayer    RESC2012X50N           -623.169      -1187.844     90       "4.7 Ohms ±1% 0.125W, 1/8W Chip Resistor 0805 (2012 Metric) Automotive AEC-Q200 Thick Film"                                                        
R26_Q1     CRCW08054R70FKEA      TopLayer    RESC2012X50N           -1298.169     -1187.844     90       "4.7 Ohms ±1% 0.125W, 1/8W Chip Resistor 0805 (2012 Metric) Automotive AEC-Q200 Thick Film"                                                        
R25_Q4     CRCW080550R0FKTA      TopLayer    RESC2012X50N           1541.575      -1187.215     90       "50 Ohms ±1% 0.125W, 1/8W Chip Resistor 0805 (2012 Metric) Automotive AEC-Q200 Thick Film"                                                         
R25_Q3     CRCW080550R0FKTA      TopLayer    RESC2012X50N           865.394       -1187.215     90       "50 Ohms ±1% 0.125W, 1/8W Chip Resistor 0805 (2012 Metric) Automotive AEC-Q200 Thick Film"                                                         
R25_Q2     CRCW080550R0FKTA      TopLayer    RESC2012X50N           -434.606      -1187.215     90       "50 Ohms ±1% 0.125W, 1/8W Chip Resistor 0805 (2012 Metric) Automotive AEC-Q200 Thick Film"                                                         
R25_Q1     CRCW080550R0FKTA      TopLayer    RESC2012X50N           -1109.606     -1187.215     90       "50 Ohms ±1% 0.125W, 1/8W Chip Resistor 0805 (2012 Metric) Automotive AEC-Q200 Thick Film"                                                         
R23        CRCW06032K00FKEA      BottomLayer RESC1608X50N           26.979        -1550.000     270      "2 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                          
R22        CRCW06032K00FKEA      BottomLayer RESC1608X50N           110.000       -1680.876     180      "2 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                          
R21        CRCW06032K00FKEA      BottomLayer RESC1608X50N           -110.000      -1680.876     0        "2 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                          
R20        CRCW06032K00FKEA      BottomLayer RESC1608X50N           -25.000       -1550.000     270      "2 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                          
R19        CRCW0603100KFKEA      TopLayer    RESC1608X50N           250.000       -2393.612     0        "100 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                        
R18        CRCW06032K00FKEA      BottomLayer RESC1608X50N           156.092       -2340.000     270      "2 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                          
R17        CRCW06030000Z0ED      TopLayer    RESC1608X50N           360.000       -2406.506     270      "0 Ohms Jumper Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200, Pulse Withstanding Thick Film"                                                
R16        CRCW06032K00FKEA      BottomLayer RESC1608X50N           240.000       -2205.000     180      "2 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                          
R15        CRCW06031K00FKEA      BottomLayer RESC1608X50N           193.415       -1940.000     270      "1 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                          
R14        CRCW060362K0FKEA      BottomLayer RESC1608X50N           138.415       -2045.000     90       "62 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                         
R13        CRCW06031K00FKEA      BottomLayer RESC1608X50N           333.415       -1940.000     270      "1 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                          
R12        CRCW0603107RFKEA      BottomLayer RESC1608X50N           410.393       -2140.207     0        "107 Ohms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                         
R11        CRCW060362K0FKEA      BottomLayer RESC1608X50N           333.415       -2065.000     90       "62 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"                                                         
R10        SMA-A0207FTDT10R      TopLayer    SMAA0207FTDT10R        137.795       -826.772      180      "10 Ohms ±1% 1W Chip Resistor MELF, 0207 Automotive AEC-Q200 Metal Film"                                                                           
R9_Q4      CRCW08051R00FKEA      TopLayer    RESC2012X50N           1191.575      -1187.844     90       "1 Ohms ±1% 0.125W, 1/8W Chip Resistor 0805 (2012 Metric) Automotive AEC-Q200 Thick Film"                                                          
R9_Q3      CRCW08051R00FKEA      TopLayer    RESC2012X50N           515.394       -1187.844     90       "1 Ohms ±1% 0.125W, 1/8W Chip Resistor 0805 (2012 Metric) Automotive AEC-Q200 Thick Film"                                                          
R9_Q2      CRCW08051R00FKEA      TopLayer    RESC2012X50N           -784.606      -1187.844     90       "1 Ohms ±1% 0.125W, 1/8W Chip Resistor 0805 (2012 Metric) Automotive AEC-Q200 Thick Film"                                                          
R9_Q1      CRCW08051R00FKEA      TopLayer    RESC2012X50N           -1459.606     -1187.844     90       "1 Ohms ±1% 0.125W, 1/8W Chip Resistor 0805 (2012 Metric) Automotive AEC-Q200 Thick Film"                                                          
R8         WSLP3921L1000FEA      BottomLayer RESC10052X50N          137.795       -984.252      270      "0.1 mOhms ±1% 9W Chip Resistor Nonstandard Anti-Sulfur, Automotive AEC-Q200, Current Sense, Moisture Resistant, Pulse Withstanding Metal Element" 
R7         WSLP3921L1000FEA      BottomLayer RESC10052X50N          -137.795      -984.252      90       "0.1 mOhms ±1% 9W Chip Resistor Nonstandard Anti-Sulfur, Automotive AEC-Q200, Current Sense, Moisture Resistant, Pulse Withstanding Metal Element" 
R5         RMCF0603FT560R        TopLayer    RESC1608X05N           -168.436      -2804.999     270      "RES 560 OHM 1% 1/10W 0603"                                                                                                                        
R4         CRCW08054K70FKEA      TopLayer    RESC2012X50N           -662.726      -3135.000     180      "4.7 kOhms ±1% 0.125W, 1/8W Chip Resistor 0805 (2012 Metric) Automotive AEC-Q200 Thick Film"                                                       
R2         RMCF0603FT560R        TopLayer    RESC1608X05N           -657.470      -1772.058     90       "RES 560 OHM 1% 1/10W 0603"                                                                                                                        
R1         RMCF0603FT560R        TopLayer    RESC1608X05N           1192.924      -1764.499     90       "RES 560 OHM 1% 1/10W 0603"                                                                                                                        
Q1         PXP015-30QLJ          TopLayer    PXP01530QLJ            -1477.303     -2655.000     90       "P-Channel 30 V 8A (Ta), 24.7A (Tc) 1.7W (Ta), 16W (Tc) Surface Mount MLPAK33"                                                                     
PS1        MGJ2D121505MPC-R7     TopLayer    MGJ2D121505MPCR7       0.000         -1956.693     90       "Isolated Module DC DC Converter 2 Output 15V -5V 100mA, 100mA 10.8V - 13.2V Input"                                                                
L8         744787220             TopLayer    744787220              -1304.754     -2940.443     270      "22 µH Shielded Drum Core, Wirewound Inductor 1.83 A 103mOhm Max 2-SMD"                                                                            
L5         MU2029-301Y           TopLayer    IND_BOURNS_2029        1020.000      -1445.000     270      "300 Ohms @ 100 MHz 1 Power, Signal Line Ferrite Bead 0805 (2012 Metric) 500mA 300mOhm"                                                            
L4         MU2029-301Y           TopLayer    IND_BOURNS_2029        -910.000      -1445.000     90       "300 Ohms @ 100 MHz 1 Power, Signal Line Ferrite Bead 0805 (2012 Metric) 500mA 300mOhm"                                                            
L2         MU2029-301Y           BottomLayer IND_BOURNS_2029        95.000        -1584.382     90       "300 Ohms @ 100 MHz 1 Power, Signal Line Ferrite Bead 0805 (2012 Metric) 500mA 300mOhm"                                                            
L1         MU2029-301Y           BottomLayer IND_BOURNS_2029        -91.494       -1584.382     90       "300 Ohms @ 100 MHz 1 Power, Signal Line Ferrite Bead 0805 (2012 Metric) 500mA 300mOhm"                                                            
HV+_P2     8191-5                TopLayer    81915                  1811.024      -472.441      0        "4 Pin Screw Terminal, Power Tap 6-32 Through Hole"                                                                                                
HV+_P1     8191-5                TopLayer    81915                  -1811.024     -472.441      0        "4 Pin Screw Terminal, Power Tap 6-32 Through Hole"                                                                                                
J1         105313-1204           TopLayer    105313-1104            -1808.941     -2775.000     270      "Connector Header Through Hole, Right Angle 4 position 0.098" (2.50mm)"                                                                            
IC1        ADS7066IRTER          TopLayer    QFN50P300X300X80-17N-D -179.055      -3059.528     180      "16 Bit Analog to Digital Converter 8 Input 1 SAR 16-WQFN (3x3)"                                                                                   
H1         FTSH-105-01-L-DV-K-TR TopLayer    HDR2X5_1.27SMD         880.000       -2836.506     180      "CONN, HDR, 10 POS, 0.050", SMD"                                                                                                                   
H2         M50-3611242           TopLayer    M503611242             -196.850      -3464.567     0        "Connector Header Surface Mount 24 position 0.050" (1.27mm)"                                                                                       
FB1        BLM15BA330SN1D        TopLayer    0402                   1680.000      -2225.000     180      "FER, BEAD, 33 OHM, 750mA, 0201"                                                                                                                   
D35        LTST-C171GKT          TopLayer    LEDC2012X90N           -1557.726     -3430.000     0        "Green 569nm LED Indication - Discrete 2.1V 0805 (2012 Metric)"                                                                                    
D28        STTH1R06AF            TopLayer    SODFL4724X103N         1785.000      -1395.000     0        "Diode Standard 600 V 1A Surface Mount SOD128Flat"                                                                                                 
D27        STTH1R06AF            TopLayer    SODFL4724X103N         -1735.000     -1415.000     180      "Diode Standard 600 V 1A Surface Mount SOD128Flat"                                                                                                 
D26        LTST-C171GKT          TopLayer    LEDC2012X90N           -1550.000     -2840.000     270      "Green 569nm LED Indication - Discrete 2.1V 0805 (2012 Metric)"                                                                                    
D14        STTH1R06AF            TopLayer    SODFL4724X103N         1960.000      -1240.000     270      "Diode Standard 600 V 1A Surface Mount SOD128Flat"                                                                                                 
D13        STTH1R06AF            TopLayer    SODFL4724X103N         -1905.000     -1240.000     270      "Diode Standard 600 V 1A Surface Mount SOD128Flat"                                                                                                 
D12        STTH1R06AF            TopLayer    SODFL4724X103N         1960.000      -1005.000     270      "Diode Standard 600 V 1A Surface Mount SOD128Flat"                                                                                                 
D11        STTH1R06AF            TopLayer    SODFL4724X103N         -1905.000     -1005.000     270      "Diode Standard 600 V 1A Surface Mount SOD128Flat"                                                                                                 
D10        AK3-430C              TopLayer    AK3430C                -10.000       -189.554      0        "625V Clamp 3000A (3kA) (8/20µs) Ipp Tvs Diode Through Hole Axial"                                                                                 
D9         BAV99-7-F             BottomLayer SOT96P240X110-3N       215.000       -1585.000     180      "Diode Array 1 Pair Series Connection 75 V 300mA (DC) Surface Mount TO-236-3, SC-59, SOT-23-3"                                                     
D8         BAV99-7-F             BottomLayer SOT96P240X110-3N       -210.000      -1580.000     0        "Diode Array 1 Pair Series Connection 75 V 300mA (DC) Surface Mount TO-236-3, SC-59, SOT-23-3"                                                     
D6         STTH1R06AF            TopLayer    SODFL4724X103N         -1735.000     -1545.000     0        "Diode Standard 600 V 1A Surface Mount SOD128Flat"                                                                                                 
D5         STTH1R06AF            TopLayer    SODFL4724X103N         1790.000      -1545.000     180      "Diode Standard 600 V 1A Surface Mount SOD128Flat"                                                                                                 
D4         STTH1R06AF            TopLayer    SODFL4724X103N         -1905.000     -1470.000     270      "Diode Standard 600 V 1A Surface Mount SOD128Flat"                                                                                                 
D3         STTH1R06AF            TopLayer    SODFL4724X103N         1960.000      -1475.000     270      "Diode Standard 600 V 1A Surface Mount SOD128Flat"                                                                                                 
D2         LTST-C171GKT          TopLayer    LEDC2012X90N           -520.000      -3037.470     180      "Green 569nm LED Indication - Discrete 2.1V 0805 (2012 Metric)"                                                                                    
D1         LTST-C171GKT          TopLayer    LEDC2012X90N           -520.000      -3130.000     180      "Green 569nm LED Indication - Discrete 2.1V 0805 (2012 Metric)"                                                                                    
C143       CL10B105KA8NNNC       BottomLayer CAPC1608X90N           1915.000      -2830.000     180      "1 µF ±10% 25V Ceramic Capacitor X7R 0603 (1608 Metric)"                                                                                           
C142       CL10B104KB8NNNC       TopLayer    CAPC1608X90N           1451.841      -2997.687     180      "0.1 µF ±10% 50V Ceramic Capacitor X7R 0603 (1608 Metric)"                                                                                         
C141       CL10B104KB8NNNC       TopLayer    CAPC1608X90N           1190.000      -3000.000     180      "0.1 µF ±10% 50V Ceramic Capacitor X7R 0603 (1608 Metric)"                                                                                         
C138       CL31B475KBHNFNE       BottomLayer CAPC3216X180N          -1205.000     -2701.279     0        "4.7 µF ±10% 50V Ceramic Capacitor X7R 1206 (3216 Metric)"                                                                                         
C137       T495X107K020ATE150    BottomLayer CAPPM7343X310N         -1182.234     -2923.140     90       "100 µF Molded Tantalum Capacitors 20 V 2917 (7343 Metric) 150mOhm"                                                                                
C136       T495X107K020ATE150    BottomLayer CAPPM7343X310N         -1385.000     -2925.000     90       "100 µF Molded Tantalum Capacitors 20 V 2917 (7343 Metric) 150mOhm"                                                                                
C135       CL31B475KBHNFNE       BottomLayer CAPC3216X180N          -1510.000     -3146.860     180      "4.7 µF ±10% 50V Ceramic Capacitor X7R 1206 (3216 Metric)"                                                                                         
C134       CL31B475KBHNFNE       BottomLayer CAPC3216X180N          -1600.000     -2500.000     0        "4.7 µF ±10% 50V Ceramic Capacitor X7R 1206 (3216 Metric)"                                                                                         
C133       06035C103JAZ2A        BottomLayer CAPC1608X90N           -1348.612     -2675.000     270      "10000 pF ±5% 50V Ceramic Capacitor X7R 0603 (1608 Metric)"                                                                                        
C132       GRM21BC71E106KE11L    TopLayer    CAPC2012X145N          -935.000      -3104.399     90       "10 µF ±10% 25V Ceramic Capacitor X7S 0805 (2012 Metric)"                                                                                          
C127       CL10B104KB8NNNC       TopLayer    CAPC1608X90N           1440.000      -2455.000     270      "0.1 µF ±10% 50V Ceramic Capacitor X7R 0603 (1608 Metric)"                                                                                         
C126       C0402C223K4RECAUTO    BottomLayer C0402                  630.000       -2990.000     90       "0.022 µF ±10% 16V Ceramic Capacitor X7R 0402 (1005 Metric)"                                                                                       
C124       CL10B105KA8NNNC       BottomLayer CAPC1608X90N           -305.000      -2925.000     0        "1 µF ±10% 25V Ceramic Capacitor X7R 0603 (1608 Metric)"                                                                                           
C123       CL10B105KA8NNNC       BottomLayer CAPC1608X90N           -120.000      -3080.733     90       "1 µF ±10% 25V Ceramic Capacitor X7R 0603 (1608 Metric)"                                                                                           
C122       CL10B104KB8NNNC       BottomLayer CAPC1608X90N           -245.000      -3080.000     90       "0.1 µF ±10% 50V Ceramic Capacitor X7R 0603 (1608 Metric)"                                                                                         
C120       CL10B105KA8NNNC       BottomLayer CAPC1608X90N           760.797       -3305.000     90       "1 µF ±10% 25V Ceramic Capacitor X7R 0603 (1608 Metric)"                                                                                           
C118       CL10B105KA8NNNC       TopLayer    CAPC1608X90N           -330.000      -3100.797     0        "1 µF ±10% 25V Ceramic Capacitor X7R 0603 (1608 Metric)"                                                                                           
C116       GJM1555C1HR50WB01D    TopLayer    CAPC1005X55N           845.000       -3310.916     180      "0.5 pF ±0.05pF 50V Ceramic Capacitor C0G, NP0 0402 (1005 Metric)"                                                                                 
C114       C0402C270J3GACTU      TopLayer    CAPC1005X55N           865.000       -3255.000     270      "27 pF ±5% 25V Ceramic Capacitor C0G, NP0 0402 (1005 Metric)"                                                                                      
C110       06035A102GAT2A        BottomLayer CAPC1608X90N           1324.084      -2075.000     270      "1000 pF ±2% 50V Ceramic Capacitor C0G, NP0 0603 (1608 Metric)"                                                                                    
C109       06035A102GAT2A        TopLayer    CAPC1608X90N           1380.000      -1640.000     0        "1000 pF ±2% 50V Ceramic Capacitor C0G, NP0 0603 (1608 Metric)"                                                                                    
C108       06035A102GAT2A        BottomLayer CAPC1608X90N           1520.000      -1610.000     270      "1000 pF ±2% 50V Ceramic Capacitor C0G, NP0 0603 (1608 Metric)"                                                                                    
C107       06035A102GAT2A        BottomLayer CAPC1608X90N           -1510.916     -2090.000     270      "1000 pF ±2% 50V Ceramic Capacitor C0G, NP0 0603 (1608 Metric)"                                                                                    
C106       06035A102GAT2A        TopLayer    CAPC1608X90N           -1550.000     -1680.000     180      "1000 pF ±2% 50V Ceramic Capacitor C0G, NP0 0603 (1608 Metric)"                                                                                    
C105       CL10B104KB8NNNC       TopLayer    CAPC1608X90N           1190.000      -2482.313     180      "0.1 µF ±10% 50V Ceramic Capacitor X7R 0603 (1608 Metric)"                                                                                         
C104       CL10B104KB8NNNC       BottomLayer CAPC1608X90N           -745.723      -2660.000     0        "0.1 µF ±10% 50V Ceramic Capacitor X7R 0603 (1608 Metric)"                                                                                         
C103       06031C681K4T2A        TopLayer    CAPC1608X90N           -10.000       -3065.000     180      "680 pF ±5% 100V Ceramic Capacitor X7R 0603 (1608 Metric)"                                                                                         
C102       06035A102GAT2A        BottomLayer CAPC1608X90N           1181.388      -2025.000     90       "1000 pF ±2% 50V Ceramic Capacitor C0G, NP0 0603 (1608 Metric)"                                                                                    
C101       06035A102GAT2A        BottomLayer CAPC1608X90N           1130.000      -1885.000     90       "1000 pF ±2% 50V Ceramic Capacitor C0G, NP0 0603 (1608 Metric)"                                                                                    
C100       GRM1555C1H101JA01D    TopLayer    CAPC1005X55N           711.289       -2928.199     0        "100 pF ±5% 50V Ceramic Capacitor C0G, NP0 0402 (1005 Metric)"                                                                                     
C99        GRM1555C1H101JA01D    TopLayer    CAPC1005X55N           711.289       -2890.000     0        "100 pF ±5% 50V Ceramic Capacitor C0G, NP0 0402 (1005 Metric)"                                                                                     
C98        CL10B104KB8NNNC       BottomLayer CAPC1608X90N           1573.966      -2437.185     180      "0.1 µF ±10% 50V Ceramic Capacitor X7R 0603 (1608 Metric)"                                                                                         
C97        GRM1555C1H101JA01D    BottomLayer CAPC1005X55N           1660.000      -2443.484     0        "100 pF ±5% 50V Ceramic Capacitor C0G, NP0 0402 (1005 Metric)"                                                                                     
C96        GRM1555C1H101JA01D    BottomLayer CAPC1005X55N           1660.000      -2400.000     0        "100 pF ±5% 50V Ceramic Capacitor C0G, NP0 0402 (1005 Metric)"                                                                                     
C95        CL10B104KB8NNNC       BottomLayer CAPC1608X90N           1508.445      -2325.000     270      "0.1 µF ±10% 50V Ceramic Capacitor X7R 0603 (1608 Metric)"                                                                                         
C94        CL21B106KQQNNNE       BottomLayer CAPC2012X95N           1568.297      -2325.000     90       "10 µF ±10% 6.3V Ceramic Capacitor X7R 0805 (2012 Metric)"                                                                                         
C93        CL10B104KB8NNNC       TopLayer    CAPC1608X90N           -330.000      -3050.000     0        "0.1 µF ±10% 50V Ceramic Capacitor X7R 0603 (1608 Metric)"                                                                                         
C91        CL10B104KB8NNNC       BottomLayer CAPC1608X90N           508.557       -2560.000     90       "0.1 µF ±10% 50V Ceramic Capacitor X7R 0603 (1608 Metric)"                                                                                         
C90        06035C103JAZ2A        BottomLayer CAPC1608X90N           456.579       -2345.000     90       "10000 pF ±5% 50V Ceramic Capacitor X7R 0603 (1608 Metric)"                                                                                        
C89        CL10B104KB8NNNC       BottomLayer CAPC1608X90N           -320.000      -2655.000     0        "0.1 µF ±10% 50V Ceramic Capacitor X7R 0603 (1608 Metric)"                                                                                         
C88        CL10B104KB8NNNC       BottomLayer CAPC1608X90N           -641.443      -2562.047     90       "0.1 µF ±10% 50V Ceramic Capacitor X7R 0603 (1608 Metric)"                                                                                         
C87        CL10B104KB8NNNC       BottomLayer CAPC1608X90N           1020.000      -2075.000     0        "0.1 µF ±10% 50V Ceramic Capacitor X7R 0603 (1608 Metric)"                                                                                         
C86        CL10B104KB8NNNC       BottomLayer CAPC1608X90N           -1560.000     -1945.000     270      "0.1 µF ±10% 50V Ceramic Capacitor X7R 0603 (1608 Metric)"                                                                                         
C85        CL10B104KB8NNNC       BottomLayer CAPC1608X90N           1275.000      -1945.000     270      "0.1 µF ±10% 50V Ceramic Capacitor X7R 0603 (1608 Metric)"                                                                                         
C84        06031C681K4T2A        TopLayer    CAPC1608X90N           -10.000       -3125.000     180      "680 pF ±5% 100V Ceramic Capacitor X7R 0603 (1608 Metric)"                                                                                         
C83        06035A102GAT2A        BottomLayer CAPC1608X90N           1500.830      -2061.222     90       "1000 pF ±2% 50V Ceramic Capacitor C0G, NP0 0603 (1608 Metric)"                                                                                    
C82        06031C681K4T2A        TopLayer    CAPC1608X90N           -312.923      -2955.797     0        "680 pF ±5% 100V Ceramic Capacitor X7R 0603 (1608 Metric)"                                                                                         
C81        06035A102GAT2A        BottomLayer CAPC1608X90N           -1335.000     -2090.000     90       "1000 pF ±2% 50V Ceramic Capacitor C0G, NP0 0603 (1608 Metric)"                                                                                    
C80        CL10B104KB8NNNC       BottomLayer CAPC1608X90N           -830.000      -2076.443     0        "0.1 µF ±10% 50V Ceramic Capacitor X7R 0603 (1608 Metric)"                                                                                         
C79        06035C103JAZ2A        BottomLayer CAPC1608X90N           670.000       -2273.096     180      "10000 pF ±5% 50V Ceramic Capacitor X7R 0603 (1608 Metric)"                                                                                        
C78        06035A102GAT2A        BottomLayer CAPC1608X90N           718.612       -2025.000     90       "1000 pF ±2% 50V Ceramic Capacitor C0G, NP0 0603 (1608 Metric)"                                                                                    
C77        06035C103JAZ2A        BottomLayer CAPC1608X90N           55.000        -2730.000     90       "10000 pF ±5% 50V Ceramic Capacitor X7R 0603 (1608 Metric)"                                                                                        
C76        06035A102GAT2A        BottomLayer CAPC1608X90N           783.096       -1885.000     90       "1000 pF ±2% 50V Ceramic Capacitor C0G, NP0 0603 (1608 Metric)"                                                                                    
C75        06035A102GAT2A        BottomLayer CAPC1608X90N           -665.000      -2030.000     90       "1000 pF ±2% 50V Ceramic Capacitor C0G, NP0 0603 (1608 Metric)"                                                                                    
C74        06035C103JAZ2A        TopLayer    CAPC1608X90N           -510.000      -2805.000     0        "10000 pF ±5% 50V Ceramic Capacitor X7R 0603 (1608 Metric)"                                                                                        
C73        06035C103JAZ2A        BottomLayer CAPC1608X90N           -495.000      -2265.000     180      "10000 pF ±5% 50V Ceramic Capacitor X7R 0603 (1608 Metric)"                                                                                        
C72        06031C681K4T2A        TopLayer    CAPC1608X90N           -80.000       -2949.478     180      "680 pF ±5% 100V Ceramic Capacitor X7R 0603 (1608 Metric)"                                                                                         
C71        06035C103JAZ2A        BottomLayer CAPC1608X90N           -693.421      -2350.000     90       "10000 pF ±5% 50V Ceramic Capacitor X7R 0603 (1608 Metric)"                                                                                        
C70        06035A102GAT2A        BottomLayer CAPC1608X90N           -720.000      -1890.000     90       "1000 pF ±2% 50V Ceramic Capacitor C0G, NP0 0603 (1608 Metric)"                                                                                    
C69        06035A102GAT2A        BottomLayer CAPC1608X90N           -1140.000     -2025.000     90       "1000 pF ±2% 50V Ceramic Capacitor C0G, NP0 0603 (1608 Metric)"                                                                                    
C68        06031C681K4T2A        TopLayer    CAPC1608X90N           -315.000      -2905.000     0        "680 pF ±5% 100V Ceramic Capacitor X7R 0603 (1608 Metric)"                                                                                         
C67        06035A102GAT2A        BottomLayer CAPC1608X90N           -1083.612     -1880.000     90       "1000 pF ±2% 50V Ceramic Capacitor C0G, NP0 0603 (1608 Metric)"                                                                                    
C66        CL10B104KB8NNNC       BottomLayer CAPC1608X90N           -71.388       -2250.723     90       "0.1 µF ±10% 50V Ceramic Capacitor X7R 0603 (1608 Metric)"                                                                                         
C65        CL10B104KB8NNNC       BottomLayer CAPC1608X90N           -351.939      -2345.000     0        "0.1 µF ±10% 50V Ceramic Capacitor X7R 0603 (1608 Metric)"                                                                                         
C64        CL10B104KB8NNNC       BottomLayer CAPC1608X90N           -140.000      -2196.466     90       "0.1 µF ±10% 50V Ceramic Capacitor X7R 0603 (1608 Metric)"                                                                                         
C63        06035A102GAT2A        BottomLayer CAPC1608X90N           -1460.738     -1588.132     180      "1000 pF ±2% 50V Ceramic Capacitor C0G, NP0 0603 (1608 Metric)"                                                                                    
C62        CL10B104KB8NNNC       BottomLayer CAPC1608X90N           205.000       -1820.000     180      "0.1 µF ±10% 50V Ceramic Capacitor X7R 0603 (1608 Metric)"                                                                                         
C61        06031A220F4T2A        BottomLayer CAPC1608X90N           -322.953      -2560.000     180      "10 pF ±2% 50V Ceramic Capacitor C0G, NP0 0603 (1608 Metric)"                                                                                      
C60        C0603C101F1GAC7867    BottomLayer CAPC1608X90N           -195.000      -2250.722     270      "100 pF ±1% 100V Ceramic Capacitor C0G, NP0 0603 (1608 Metric)"                                                                                    
C59        C0603C101F1GAC7867    TopLayer    CAPC1608X90N           -145.000      -2420.000     180      "100 pF ±1% 100V Ceramic Capacitor C0G, NP0 0603 (1608 Metric)"                                                                                    
C58        06035C103JAZ2A        BottomLayer CAPC1608X90N           -215.000      -2560.000     0        "10000 pF ±5% 50V Ceramic Capacitor X7R 0603 (1608 Metric)"                                                                                        
C57        06035A100GAT2A        BottomLayer CAPC1608X90N           -171.388      -1945.000     90       "10 pF ±2% 50V Ceramic Capacitor C0G, NP0 0603 (1608 Metric)"                                                                                      
C56        06031A220F4T2A        BottomLayer CAPC1608X90N           50.000        -2401.388     0        "10 pF ±2% 50V Ceramic Capacitor C0G, NP0 0603 (1608 Metric)"                                                                                      
C55        06035C103JAZ2A        BottomLayer CAPC1608X90N           95.000        -2250.723     90       "10000 pF ±5% 50V Ceramic Capacitor X7R 0603 (1608 Metric)"                                                                                        
C54        06035A102GAT2A        TopLayer    CAPC1608X90N           165.000       -2404.734     90       "1000 pF ±2% 50V Ceramic Capacitor C0G, NP0 0603 (1608 Metric)"                                                                                    
C53        CL10B104KB8NNNC       BottomLayer CAPC1608X90N           138.415       -2145.207     90       "0.1 µF ±10% 50V Ceramic Capacitor X7R 0603 (1608 Metric)"                                                                                         
C51        06035A100GAT2A        BottomLayer CAPC1608X90N           0.000         -1677.185     180      "10 pF ±2% 50V Ceramic Capacitor C0G, NP0 0603 (1608 Metric)"                                                                                      
C50        06035A102GAT2A        BottomLayer CAPC1608X90N           0.000         -1626.388     180      "1000 pF ±2% 50V Ceramic Capacitor C0G, NP0 0603 (1608 Metric)"                                                                                    
C49        06035C103JAZ2A        BottomLayer CAPC1608X90N           248.524       -2438.071     0        "10000 pF ±5% 50V Ceramic Capacitor X7R 0603 (1608 Metric)"                                                                                        
C48        06035C103JAZ2A        TopLayer    CAPC1608X90N           275.000       -2445.000     180      "10000 pF ±5% 50V Ceramic Capacitor X7R 0603 (1608 Metric)"                                                                                        
C47        CL10B104KB8NNNC       BottomLayer CAPC1608X90N           350.000       -2305.000     90       "0.1 µF ±10% 50V Ceramic Capacitor X7R 0603 (1608 Metric)"                                                                                         
C46        06035C103JAZ2A        BottomLayer CAPC1608X90N           345.000       -2217.706     180      "10000 pF ±5% 50V Ceramic Capacitor X7R 0603 (1608 Metric)"                                                                                        
C45        06035A102GAT2A        BottomLayer CAPC1608X90N           138.415       -1940.000     270      "1000 pF ±2% 50V Ceramic Capacitor C0G, NP0 0603 (1608 Metric)"                                                                                    
C44        06031C681K4T2A        TopLayer    CAPC1608X90N           -10.000       -3000.276     180      "680 pF ±5% 100V Ceramic Capacitor X7R 0603 (1608 Metric)"                                                                                         
C43        06035A100C4T2A        BottomLayer CAPC1608X90N           282.027       -1940.000     270      "10 pF ±0.25pF 50V Ceramic Capacitor C0G, NP0 0603 (1608 Metric)"                                                                                  
C42        06035A102GAT2A        BottomLayer CAPC1608X90N           384.803       -2065.000     90       "1000 pF ±2% 50V Ceramic Capacitor C0G, NP0 0603 (1608 Metric)"                                                                                    
C40        CL10B104KB8NNNC       TopLayer    CAPC1608X90N           1135.000      -2235.000     180      "0.1 µF ±10% 50V Ceramic Capacitor X7R 0603 (1608 Metric)"                                                                                         
C39        CL10B104KB8NNNC       TopLayer    CAPC1608X90N           -710.000      -2229.144     180      "0.1 µF ±10% 50V Ceramic Capacitor X7R 0603 (1608 Metric)"                                                                                         
C25        CC0603KPX7R9BB101     TopLayer    CAPC1608X09N           1130.000      -1670.000     0        "100 pF ±10% 50V Ceramic Capacitor X7R 0603 (1608 Metric)"                                                                                         
C24        CC0603KPX7R9BB101     TopLayer    CAPC1608X09N           -705.000      -1650.000     90       "100 pF ±10% 50V Ceramic Capacitor X7R 0603 (1608 Metric)"                                                                                         
C20        CL10B104KB8NNNC       TopLayer    CAPC1608X90N           -387.018      -2225.000     270      "0.1 µF ±10% 50V Ceramic Capacitor X7R 0603 (1608 Metric)"                                                                                         
C19        CL10B104KB8NNNC       BottomLayer CAPC1608X90N           710.000       -3305.000     90       "0.1 µF ±10% 50V Ceramic Capacitor X7R 0603 (1608 Metric)"                                                                                         
C15        CL31B475KBHNFNE       TopLayer    CAPC3216X180N          443.711       -1740.000     180      "4.7 µF ±10% 50V Ceramic Capacitor X7R 1206 (3216 Metric)"                                                                                         
C13        CL31B475KBHNFNE       TopLayer    CAPC3216X180N          640.000       -1875.886     0        "4.7 µF ±10% 50V Ceramic Capacitor X7R 1206 (3216 Metric)"                                                                                         
C3         C2220C663KDGLCAUTO    TopLayer    CAPC5950X155N          -177.165      -767.716      180      "0.066 µF ±10% 1000V (1kV) Ceramic Capacitor C0G, NP0 2220 (5750 Metric)"                                                                          
