
Version : NCV7430 Evaluation 3.5

Released: 1.12.2017

3.5 (1.12.2017)
	- LIN commands tab - Frame creator major re-built
	- Misc tab - User defined baudrate added
	- Example USL updated (Martin Kresta contact info removed)
	- Example USL loaded automatically at startup
	- Help file updated

3.4 (3.6.2016)
	- LIN commands tab - time stamps corrected. Miliseconds are now always displayed with 3 digits.

3.2 (18.9.2014)
	- Default Application data folder location corrected
	- New USL demo added

3.1 (28.7.2014)
	- LIN commands tab - Frame creator - Enhanced checksum support added

3.0 (1.8.2013)
	- new version of USL (support of cycles, highlighlting of very long scripts)
	- updated tab "Network configuration" (more intuitive control)

2.2 (10.5.2013)
	- minor update

2.1 (4.10.2012)
	- User Script Language Tab - bug fixed (An Error appearing when opening a script which is shorter than the previous one)


2.0 (15.5.2012)
	- Supports NCV7430 mask version O1A and higher
	- added support for new OTP bits (BALLAST, TWPROG2)
	- reading of TWPROG2 is not supported in version 2.0
	- OTP bit DIAG_ALL_OFF was removed

1.7 (x86_x64)
	- added support of 64-bit operating system

1.3
	- Changes in calculation of reference XYZ matrix, to avoid "on-chip scalling"
	- The green label "Zapping done succesfully!" is displayed after succesfully zapping of new NAD.
	- Added single Lin frame repetition, when transmission corruption was detected. The warning is displayed after 2 consecutive Lin errors.
	- Corrected spelling errors.
	- Fixed bug - Batch OTP programming, bit DIAG_ALL_OFF.
	- Fixed bug - Set_Intensity frame - calculation on Group ID bits in frame.

1.2
 	- Feature for storing node XYZ values
	- Calculation of reference triangle
	- Arrows keys used for color selection in color dialog istead of num keyboard
	- Color dialog store last setting of Online_set_color CHeckBox
	- Calibration factors for displaying appropriate node gamut in color dialog are readed from shadow registers, instead of OTP

1.1:
	- LED diagnostic acording to datasheet rev. 17	
	- Fixed bug at nework configuration tab (change cancelling)
	- Fixed bug - change cancelling on network configuration tab when only one node is connected

1.0:
	- Corrected calculation of RGB values in color dialog
	- Corrected frame Get_Status on main screen (wrong signalization of LED errors)
	- Automatic detection of USB to LIN Comm board, when some other FTDI devices are connected.