### BB_COEXIFCNTL2

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
11:8 | RW | RX_ANT_DELAY | Time (in us) by which is anticipated bt_rx to be provided before effective radio receipt operation
3:0 | RW | TX_ANT_DELAY | Time (in us) by which is anticipated bt_tx to be provided before effective radio transmit operation

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
11:8 | RX_ANT_DELAY | RX_ANT_DELAY_0 |  | 0x0*
3:0 | TX_ANT_DELAY | TX_ANT_DELAY_0 |  | 0x0*