### LSAD_PRE_SEL_INPUT

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
14:12 | RW | LSAD_PRE_SEL_IN3 | LSAD input pre-selection
10:8 | RW | LSAD_PRE_SEL_IN2 | LSAD input pre-selection
6:4 | RW | LSAD_PRE_SEL_IN1 | LSAD input pre-selection
2:0 | RW | LSAD_PRE_SEL_IN0 | LSAD input pre-selection

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
14:12 | LSAD_PRE_SEL_IN3 | IN3_PRE_SEL_GPIO1 | GPIO1 pre-selected for lsad input 3 | 0x0*
|  | IN3_PRE_SEL_GPIO3 | GPIO3 pre-selected for lsad input 3 | 0x1
|  | IN3_PRE_SEL_GPIO5 | GPIO5 pre-selected for lsad input 3 | 0x2
|  | IN3_PRE_SEL_GPIO7 | GPIO7 pre-selected for lsad input 3 | 0x3
|  | IN3_PRE_SEL_GPIO9 | GPIO9 pre-selected for lsad input 3 | 0x4
|  | IN3_PRE_SEL_GPIO11 | GPIO11 pre-selected for lsad input 3 | 0x5
|  | IN3_PRE_SEL_GPIO13 | GPIO13 pre-selected for lsad input 3 | 0x6
|  | IN3_PRE_SEL_GPIO15 | GPIO15 pre-selected for lsad input 3 | 0x7
10:8 | LSAD_PRE_SEL_IN2 | IN2_PRE_SEL_GPIO0 | GPIO0 pre-selected for lsad input 2 | 0x0*
|  | IN2_PRE_SEL_GPIO2 | GPIO2 pre-selected for lsad input 2 | 0x1
|  | IN2_PRE_SEL_GPIO4 | GPIO4 pre-selected for lsad input 2 | 0x2
|  | IN2_PRE_SEL_GPIO6 | GPIO6 pre-selected for lsad input 2 | 0x3
|  | IN2_PRE_SEL_GPIO8 | GPIO8 pre-selected for lsad input 2 | 0x4
|  | IN2_PRE_SEL_GPIO10 | GPIO10 pre-selected for lsad input 2 | 0x5
|  | IN2_PRE_SEL_GPIO12 | GPIO12 pre-selected for lsad input 2 | 0x6
|  | IN2_PRE_SEL_GPIO14 | GPIO14 pre-selected for lsad input 2 | 0x7
6:4 | LSAD_PRE_SEL_IN1 | IN1_PRE_SEL_GPIO1 | GPIO1 pre-selected for lsad input 1 | 0x0*
|  | IN1_PRE_SEL_GPIO3 | GPIO3 pre-selected for lsad input 1 | 0x1
|  | IN1_PRE_SEL_GPIO5 | GPIO5 pre-selected for lsad input 1 | 0x2
|  | IN1_PRE_SEL_GPIO7 | GPIO7 pre-selected for lsad input 1 | 0x3
|  | IN1_PRE_SEL_GPIO9 | GPIO9 pre-selected for lsad input 1 | 0x4
|  | IN1_PRE_SEL_GPIO11 | GPIO11 pre-selected for lsad input 1 | 0x5
|  | IN1_PRE_SEL_GPIO13 | GPIO13 pre-selected for lsad input 1 | 0x6
|  | IN1_PRE_SEL_GPIO15 | GPIO15 pre-selected for lsad input 1 | 0x7
2:0 | LSAD_PRE_SEL_IN0 | IN0_PRE_SEL_GPIO0 | GPIO0 pre-selected for lsad input 0 | 0x0*
|  | IN0_PRE_SEL_GPIO2 | GPIO2 pre-selected for lsad input 0 | 0x1
|  | IN0_PRE_SEL_GPIO4 | GPIO4 pre-selected for lsad input 0 | 0x2
|  | IN0_PRE_SEL_GPIO6 | GPIO6 pre-selected for lsad input 0 | 0x3
|  | IN0_PRE_SEL_GPIO8 | GPIO8 pre-selected for lsad input 0 | 0x4
|  | IN0_PRE_SEL_GPIO10 | GPIO10 pre-selected for lsad input 0 | 0x5
|  | IN0_PRE_SEL_GPIO12 | GPIO12 pre-selected for lsad input 0 | 0x6
|  | IN0_PRE_SEL_GPIO14 | GPIO14 pre-selected for lsad input 0 | 0x7