### FLASH_COPY_CTRL

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
3 | R | ERROR | Error status
2 | W | STOP | Stop the transfer
1 | W | START | Start the transfer
0 | R | BUSY | Busy status

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
3 | ERROR | COPY_NO_ERROR | No write / comparison error | 0x0*
|  | COPY_ERROR | Write or comparison error | 0x1
2 | STOP | COPY_STOP | Stop the current transfer | 0x1
1 | START | COPY_START | Start the current transfer | 0x1
0 | BUSY | COPY_IDLE | Flash copier is idle | 0x0*
|  | COPY_BUSY | Flash copier is busy | 0x1