### ASCC_CTRL

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
8 | W | PHASE_CNT_START_NO_WAIT | Start the asynchronous clock phase counter mechanism without waiting on a sync pulse
7 | R | PERIOD_CNT_STATUS | Asynchronous clock period counter status
6 | W | PERIOD_CNT_STOP | Stop the asynchronous clock period counter mechanism
5 | W | PERIOD_CNT_START | Start the asynchronous clock period counter mechanism
4 | R | PHASE_CNT_MISSED_STATUS | Asynchronous clock phase counter missed status
3 | R | PHASE_CNT_STATUS | Asynchronous clock phase counter status
2 | W | PHASE_CNT_STOP | Stop the asynchronous clock phase counter mechanism
1 | W | PHASE_CNT_START | Start the asynchronous clock phase counter mechanism and wait for sync pulse
0 | W | CNT_RESET | Reset asynchronous clock counter

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
8 | PHASE_CNT_START_NO_WAIT | PHASE_CNT_START_NO_WAIT | Reset PHASE_CNT and start the asynchronous clock phase counter mechanism without waiting on a sync pulse | 0x1
7 | PERIOD_CNT_STATUS | PERIOD_CNT_IDLE | The asynchronous clock period counter mechanism is idle | 0x0*
|  | PERIOD_CNT_BUSY | The asynchronous clock period counter mechanism is busy | 0x1
6 | PERIOD_CNT_STOP | PERIOD_CNT_STOP | Stop the asynchronous clock period counter mechanism | 0x1
5 | PERIOD_CNT_START | PERIOD_CNT_START | Reset PERIOD_CNT and start the asynchronous clock period counter mechanism | 0x1
4 | PHASE_CNT_MISSED_STATUS | PHASE_CNT_NORMAL | The asynchronous clock phase counter mechanism was not stopped due to a missed synchronization signal | 0x0*
|  | PHASE_CNT_MISSED | The asynchronous clock phase counter mechanism was stopped due to a missed synchronization signal | 0x1
3 | PHASE_CNT_STATUS | PHASE_CNT_IDLE | The asynchronous clock phase counter mechanism is idle | 0x0*
|  | PHASE_CNT_BUSY | The asynchronous clock phase counter mechanism is busy | 0x1
2 | PHASE_CNT_STOP | PHASE_CNT_STOP | Stop the asynchronous clock phase counter mechanism | 0x1
1 | PHASE_CNT_START | PHASE_CNT_START | Reset PHASE_CNT and start the asynchronous clock phase counter mechanism and wait on a sync pulse | 0x1
0 | CNT_RESET | CNT_RESET | Reset asynchronous clock counter | 0x1