# Importing the Sample Code

To import the sample code:

1. In the Pack installer, click on the Examples tab to list all the example projects included in the RSL15 CMSIS-Pack.
2. Choose the example project called blinky, and click the Copy button to import it into your workspace (see the "Pack Manager Perspective: Examples Tab" figure). Choose a destination folder for a copy of the sample code. We recommend leaving the Launch μVision checkbox checked.

Figure: Pack Manager Perspective: Examples Tab

For the blinky sample, the Startup, HAL and GPIO components are preconfigured with the source variant, so the source code of these libraries is included directly (see the "RTE Configuration for the Blinky Example Project in the Keil μVision IDE" figure).

Figure: RTE Configuration for the Blinky Example Project in the Keil μVision IDE