### RF_CODING

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
31 | RW | CODING_EN_DATAWHITE | Data-whitening enabling (banked)
30 | RW | CODING_I_NQ_DELAYED | Channel I delay (banked)
29 | RW | CODING_OFFSET | Offset (delay) introduction (banked)
28 | RW | CODING_BIT_INVERT | Bit value inversion in Tx and Rx modes (banked)
27 | RW | CODING_EVEN_BEFORE_ODD | Determine the bit order in case of a 2 bits per symbol modulation (banked)
26 | RW | CODING_EN_802154_L2F | Linear to frequency encoding needed in order to modulate an OQPSK as an MSK (banked)
25 | RW | CODING_EN_802154_B2C | Bit to chips encoding used in the IEEE 802.15.4 standard (banked)
24 | RW | CODING_EN_MANCHESTER | Manchester encoding (banked)
23 | RW | CHANNELS_2_EN_CHANNEL_SEL | Definition of channels (banked)
22 | RW | CHANNELS_2_EN_CHN_BLE | BLE channels index LUT (banked)
19:16 | RW | CHANNELS_2_CHANNEL_SPACING_HI | Channel spacing MSB (banked)
15:0 | RW | CHANNELS_1_CHANNEL_SPACING_LO | Channel spacing LSB (banked)

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
31 | CODING_EN_DATAWHITE | CODING_EN_DATAWHITE_DISABLE | Disable the data-whitening | 0x0
|  | CODING_EN_DATAWHITE_ENABLE | Enable the data-whitening | 0x1*
30 | CODING_I_NQ_DELAYED | CODING_I_NQ_DELAYED_DISABLE | Channel I is not considered as delayed in case of a 2bit per symbol modulation | 0x0*
|  | CODING_I_NQ_DELAYED_ENABLE | Channel I is considered as delayed in case of a 2bit per symbol modulation | 0x1
29 | CODING_OFFSET | CODING_OFFSET_DISABLE | No offset (delay) is introduced in one of the two channels (2 bits per symbol modulation) | 0x0*
|  | CODING_OFFSET_ENABLE | An offset (delay) is introduced in one of the two channels (2 bits per symbol modulation) | 0x1
28 | CODING_BIT_INVERT | CODING_BIT_INVERT_DISABLE | Original bit value (Tx and Rx) | 0x0*
|  | CODING_BIT_INVERT_ENABLE | Inversed bit value (Tx and Rx) | 0x1
27 | CODING_EVEN_BEFORE_ODD | CODING_EVEN_BEFORE_ODD_DISABLE | Second bit (bit 1, odd) goes to the I path | 0x0*
|  | CODING_EVEN_BEFORE_ODD_ENABLE | First bit (bit 0, even) goes to the I path | 0x1
26 | CODING_EN_802154_L2F | CODING_EN_802154_L2F_DISABLE | Disable the linear to frequency encoding | 0x0*
|  | CODING_EN_802154_L2F_ENABLE | Enable the linear to frequency encoding | 0x1
25 | CODING_EN_802154_B2C | CODING_EN_802154_B2C_DISABLE | Disable the bit to chips encoding used in the IEEE 802.15.4 standard | 0x0*
|  | CODING_EN_802154_B2C_ENABLE | Enable the bit to chips encoding used in the IEEE 802.15.4 standard | 0x1
24 | CODING_EN_MANCHESTER | CODING_EN_MANCHESTER_DISABLE | Disable the Manchester encoding | 0x0*
|  | CODING_EN_MANCHESTER_ENABLE | Enable the Manchester encoding | 0x1
23 | CHANNELS_2_EN_CHANNEL_SEL | CHANNELS_2_EN_CHANNEL_SEL_DISABLE | Disable the definition of channels | 0x0
|  | CHANNELS_2_EN_CHANNEL_SEL_ENABLE | Enable the definition of channels | 0x1*
22 | CHANNELS_2_EN_CHN_BLE | CHANNELS_2_EN_CHN_BLE_DISABLE | Disable the BLE channels index LUT | 0x0
|  | CHANNELS_2_EN_CHN_BLE_ENABLE | Enable the BLE channels index LUT | 0x1*
19:16 | CHANNELS_2_CHANNEL_SPACING_HI | CHANNELS_2_CHANNEL_SPACING_HI_DEFAULT | The formula that determines this value is the same as for the central frequency | 0x7*
15:0 | CHANNELS_1_CHANNEL_SPACING_LO | CHANNELS_1_CHANNEL_SPACING_LO_DEFAULT | The formula that determines this value is the same as for the central frequency | 0x1C72*