### ACS_TEMP_CURR_CFG

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
19:16 | RW | CURRENT_VALUE | Temperature current value
13:8 | RW | CURRENT_TRIM | Temperature current trimming
7:4 | RW | GPIO_IN_USE | GPIO from which the duty cycle is used
1 | RW | DUTY_CURR | Duty cycling current enable
0 | RW | ENABLE | Temperature current enable

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
19:16 | CURRENT_VALUE | TEMP_CURR_1UA | Temperature current set to 1 uA | 0x0
|  | TEMP_CURR_10UA | Temperature current set to 10 uA | 0x9*
|  | TEMP_CURR_16UA | Temperature current set to 16 uA | 0xF
13:8 | CURRENT_TRIM | TEMP_CURR_TRIM_M32 | -10% trimming | 0x0*
|  | TEMP_CURR_TRIM_0 | Default trimming | 0x20
|  | TEMP_CURR_TRIM_P31 | +10% trimming | 0x3F
7:4 | GPIO_IN_USE | TEMP_CURR_GPIO0 | Duty cycle of GPIO0 is used | 0x0*
|  | TEMP_CURR_GPIO1 | Duty cycle of GPIO1 is used | 0x1
|  | TEMP_CURR_GPIO2 | Duty cycle of GPIO2 is used | 0x2
|  | TEMP_CURR_GPIO3 | Duty cycle of GPIO3 is used | 0x3
|  | TEMP_CURR_GPIO4 | Duty cycle of GPIO4 is used | 0x4
|  | TEMP_CURR_GPIO5 | Duty cycle of GPIO5 is used | 0x5
|  | TEMP_CURR_GPIO6 | Duty cycle of GPIO6 is used | 0x6
|  | TEMP_CURR_GPIO7 | Duty cycle of GPIO7 is used | 0x7
|  | TEMP_CURR_GPIO8 | Duty cycle of GPIO8 is used | 0x8
|  | TEMP_CURR_GPIO9 | Duty cycle of GPIO9 is used | 0x9
|  | TEMP_CURR_GPIO10 | Duty cycle of GPIO10 is used | 0xA
|  | TEMP_CURR_GPIO11 | Duty cycle of GPIO11 is used | 0xB
|  | TEMP_CURR_GPIO12 | Duty cycle of GPIO12 is used | 0xC
|  | TEMP_CURR_GPIO13 | Duty cycle of GPIO13 is used | 0xD
|  | TEMP_CURR_GPIO14 | Duty cycle of GPIO14 is used | 0xE
|  | TEMP_CURR_GPIO15 | Duty cycle of GPIO15 is used | 0xF
1 | DUTY_CURR | LSAD_CURR_NORMAL | Normal mode: current enable only controlled by CURR_ENABLE | 0x0*
|  | LSAD_CURR_DUTY | Duty cycling current enable (enabled only during LSAD conversion) | 0x1
0 | ENABLE | TEMP_CURR_DISABLE | Disable the temperature current | 0x0*
|  | TEMP_CURR_ENABLE | Enable the temperature current | 0x1