### NVIC_ICPR0

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
31 | RW | ASCC_PHASE | ASCC_PHASE interrupt clear pending
30 | RW | ASCC_PERIOD | ASCC_PERIOD interrupt clear pending
29 | RW | CC312 | CC312 interrupt clear pending
28 | RW | FPU | FPU interrupt clear pending
27 | RW | LIN0 | LIN0 interrupt clear pending
26 | RW | PCM0_ERROR | PCM0_ERROR interrupt clear pending
25 | RW | PCM0_RX_TX | PCM0_RX_TX interrupt clear pending
24 | RW | UART0_ERROR | UART0_ERROR interrupt clear pending
23 | RW | UART0_TX | UART0_TX interrupt clear pending
22 | RW | UART0_RX | UART0_RX interrupt clear pending
21 | RW | I2C1 | I2C1 interrupt clear pending
20 | RW | I2C0 | I2C0 interrupt clear pending
19 | RW | SPI1_COM | SPI1_COM interrupt clear pending
18 | RW | SPI1_TX | SPI1_TX interrupt clear pending
17 | RW | SPI1_RX | SPI1_RX interrupt clear pending
16 | RW | SPI0_COM | SPI0_COM interrupt clear pending
15 | RW | SPI0_TX | SPI0_TX interrupt clear pending
14 | RW | SPI0_RX | SPI0_RX interrupt clear pending
13 | RW | WATCHDOG | WATCHDOG interrupt clear pending
12 | RW | GPIO3 | GPIO3 interrupt clear pending
11 | RW | GPIO2 | GPIO2 interrupt clear pending
10 | RW | GPIO1 | GPIO1 interrupt clear pending
9 | RW | GPIO0 | GPIO0 interrupt clear pending
8 | RW | FIFO | FIFO interrupt clear pending
7 | RW | TIMER3 | TIMER3 interrupt clear pending
6 | RW | TIMER2 | TIMER2 interrupt clear pending
5 | RW | TIMER1 | TIMER1 interrupt clear pending
4 | RW | TIMER0 | TIMER0 interrupt clear pending
3 | RW | LSAD_MONITOR | LSAD_MONITOR interrupt clear pending
2 | RW | RTC_CLOCK | RTC_CLOCK interrupt clear pending
1 | RW | RTC_ALARM | RTC_ALARM interrupt clear pending
0 | RW | WAKEUP | WAKEUP interrupt clear pending

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
31 | ASCC_PHASE | NVIC_ASCC_PHASE_INT_CLRPEND | Clear the NVIC_ASCC_PHASE_INT_CLRPEND interrupt status bit | 0x1
30 | ASCC_PERIOD | NVIC_ASCC_PERIOD_INT_CLRPEND | Clear the NVIC_ASCC_PERIOD_INT_CLRPEND interrupt status bit | 0x1
29 | CC312 | NVIC_CC312_INT_CLRPEND | Clear the NVIC_CC312_INT_CLRPEND interrupt status bit | 0x1
28 | FPU | NVIC_FPU_INT_CLRPEND | Clear the NVIC_FPU_INT_CLRPEND interrupt status bit | 0x1
27 | LIN0 | NVIC_LIN0_INT_CLRPEND | Clear the NVIC_LIN0_INT_CLRPEND interrupt status bit | 0x1
26 | PCM0_ERROR | NVIC_PCM0_ERROR_INT_CLRPEND | Clear the NVIC_PCM0_ERROR_INT_CLRPEND interrupt status bit | 0x1
25 | PCM0_RX_TX | NVIC_PCM0_RX_TX_INT_CLRPEND | Clear the NVIC_PCM0_RX_TX_INT_CLRPEND interrupt status bit | 0x1
24 | UART0_ERROR | NVIC_UART0_ERROR_INT_CLRPEND | Clear the NVIC_UART0_ERROR_INT_CLRPEND interrupt status bit | 0x1
23 | UART0_TX | NVIC_UART0_TX_INT_CLRPEND | Clear the NVIC_UART0_TX_INT_CLRPEND interrupt status bit | 0x1
22 | UART0_RX | NVIC_UART0_RX_INT_CLRPEND | Clear the NVIC_UART0_RX_INT_CLRPEND interrupt status bit | 0x1
21 | I2C1 | NVIC_I2C1_INT_CLRPEND | Clear the NVIC_I2C1_INT_CLRPEND interrupt status bit | 0x1
20 | I2C0 | NVIC_I2C0_INT_CLRPEND | Clear the NVIC_I2C0_INT_CLRPEND interrupt status bit | 0x1
19 | SPI1_COM | NVIC_SPI1_COM_INT_CLRPEND | Clear the NVIC_SPI1_COM_INT_CLRPEND interrupt status bit | 0x1
18 | SPI1_TX | NVIC_SPI1_TX_INT_CLRPEND | Clear the NVIC_SPI1_TX_INT_CLRPEND interrupt status bit | 0x1
17 | SPI1_RX | NVIC_SPI1_RX_INT_CLRPEND | Clear the NVIC_SPI1_RX_INT_CLRPEND interrupt status bit | 0x1
16 | SPI0_COM | NVIC_SPI0_COM_INT_CLRPEND | Clear the NVIC_SPI0_COM_INT_CLRPEND interrupt status bit | 0x1
15 | SPI0_TX | NVIC_SPI0_TX_INT_CLRPEND | Clear the NVIC_SPI0_TX_INT_CLRPEND interrupt status bit | 0x1
14 | SPI0_RX | NVIC_SPI0_RX_INT_CLRPEND | Clear the NVIC_SPI0_RX_INT_CLRPEND interrupt status bit | 0x1
13 | WATCHDOG | NVIC_WATCHDOG_INT_CLRPEND | Clear the NVIC_WATCHDOG_INT_CLRPEND interrupt status bit | 0x1
12 | GPIO3 | NVIC_GPIO3_INT_CLRPEND | Clear the NVIC_GPIO3_INT_CLRPEND interrupt status bit | 0x1
11 | GPIO2 | NVIC_GPIO2_INT_CLRPEND | Clear the NVIC_GPIO2_INT_CLRPEND interrupt status bit | 0x1
10 | GPIO1 | NVIC_GPIO1_INT_CLRPEND | Clear the NVIC_GPIO1_INT_CLRPEND interrupt status bit | 0x1
9 | GPIO0 | NVIC_GPIO0_INT_CLRPEND | Clear the NVIC_GPIO0_INT_CLRPEND interrupt status bit | 0x1
8 | FIFO | NVIC_FIFO_INT_CLRPEND | Clear the NVIC_FIFO_INT_CLRPEND interrupt status bit | 0x1
7 | TIMER3 | NVIC_TIMER3_INT_CLRPEND | Clear the NVIC_TIMER3_INT_CLRPEND interrupt status bit | 0x1
6 | TIMER2 | NVIC_TIMER2_INT_CLRPEND | Clear the NVIC_TIMER2_INT_CLRPEND interrupt status bit | 0x1
5 | TIMER1 | NVIC_TIMER1_INT_CLRPEND | Clear the NVIC_TIMER1_INT_CLRPEND interrupt status bit | 0x1
4 | TIMER0 | NVIC_TIMER0_INT_CLRPEND | Clear the NVIC_TIMER0_INT_CLRPEND interrupt status bit | 0x1
3 | LSAD_MONITOR | NVIC_LSAD_MONITOR_INT_CLRPEND | Clear the NVIC_LSAD_MONITOR_INT_CLRPEND interrupt status bit | 0x1
2 | RTC_CLOCK | NVIC_RTC_CLOCK_INT_CLRPEND | Clear the NVIC_RTC_CLOCK_INT_CLRPEND interrupt status bit | 0x1
1 | RTC_ALARM | NVIC_RTC_ALARM_INT_CLRPEND | Clear the NVIC_RTC_ALARM_INT_CLRPEND interrupt status bit | 0x1
0 | WAKEUP | NVIC_WAKEUP_INT_CLRPEND | Clear the NVIC_WAKEUP_INT_CLRPEND interrupt status bit | 0x1