### GPIO_SRC_BB_IQ_DATA

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
28:24 | RW | IQ_DATA_3 | Baseband controller IQ_DATA_3 input selection
20:16 | RW | IQ_DATA_2 | Baseband controller IQ_DATA_2 input selection
12:8 | RW | IQ_DATA_1 | Baseband controller IQ_DATA_1 input selection
4:0 | RW | IQ_DATA_0 | Baseband controller IQ_DATA_0 input selection

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
28:24 | IQ_DATA_3 | BB_IQ_DATA_3_SRC_GPIO_0 | Select GPIO[0] as source | 0x0
|  | BB_IQ_DATA_3_SRC_GPIO_1 | Select GPIO[1] as source | 0x1
|  | BB_IQ_DATA_3_SRC_GPIO_2 | Select GPIO[2] as source | 0x2
|  | BB_IQ_DATA_3_SRC_GPIO_3 | Select GPIO[3] as source | 0x3
|  | BB_IQ_DATA_3_SRC_GPIO_4 | Select GPIO[4] as source | 0x4
|  | BB_IQ_DATA_3_SRC_GPIO_5 | Select GPIO[5] as source | 0x5
|  | BB_IQ_DATA_3_SRC_GPIO_6 | Select GPIO[6] as source | 0x6
|  | BB_IQ_DATA_3_SRC_GPIO_7 | Select GPIO[7] as source | 0x7
|  | BB_IQ_DATA_3_SRC_GPIO_8 | Select GPIO[8] as source | 0x8
|  | BB_IQ_DATA_3_SRC_GPIO_9 | Select GPIO[9] as source | 0x9
|  | BB_IQ_DATA_3_SRC_GPIO_10 | Select GPIO[10] as source | 0xA
|  | BB_IQ_DATA_3_SRC_GPIO_11 | Select GPIO[11] as source | 0xB
|  | BB_IQ_DATA_3_SRC_GPIO_12 | Select GPIO[12] as source | 0xC
|  | BB_IQ_DATA_3_SRC_GPIO_13 | Select GPIO[13] as source | 0xD
|  | BB_IQ_DATA_3_SRC_GPIO_14 | Select GPIO[14] as source | 0xE
|  | BB_IQ_DATA_3_SRC_GPIO_15 | Select GPIO[15] as source | 0xF
|  | BB_IQ_DATA_3_SRC_CONST_LOW | Select constant low as source | 0x10
|  | BB_IQ_DATA_3_SRC_CONST_HIGH | Select constant high as source | 0x11
|  | BB_IQ_DATA_3_SRC_RF_IQ_DATA_3 | Select RF front-end IQ_DATA_3 as source | 0x12*
20:16 | IQ_DATA_2 | BB_IQ_DATA_2_SRC_GPIO_0 | Select GPIO[0] as source | 0x0
|  | BB_IQ_DATA_2_SRC_GPIO_1 | Select GPIO[1] as source | 0x1
|  | BB_IQ_DATA_2_SRC_GPIO_2 | Select GPIO[2] as source | 0x2
|  | BB_IQ_DATA_2_SRC_GPIO_3 | Select GPIO[3] as source | 0x3
|  | BB_IQ_DATA_2_SRC_GPIO_4 | Select GPIO[4] as source | 0x4
|  | BB_IQ_DATA_2_SRC_GPIO_5 | Select GPIO[5] as source | 0x5
|  | BB_IQ_DATA_2_SRC_GPIO_6 | Select GPIO[6] as source | 0x6
|  | BB_IQ_DATA_2_SRC_GPIO_7 | Select GPIO[7] as source | 0x7
|  | BB_IQ_DATA_2_SRC_GPIO_8 | Select GPIO[8] as source | 0x8
|  | BB_IQ_DATA_2_SRC_GPIO_9 | Select GPIO[9] as source | 0x9
|  | BB_IQ_DATA_2_SRC_GPIO_10 | Select GPIO[10] as source | 0xA
|  | BB_IQ_DATA_2_SRC_GPIO_11 | Select GPIO[11] as source | 0xB
|  | BB_IQ_DATA_2_SRC_GPIO_12 | Select GPIO[12] as source | 0xC
|  | BB_IQ_DATA_2_SRC_GPIO_13 | Select GPIO[13] as source | 0xD
|  | BB_IQ_DATA_2_SRC_GPIO_14 | Select GPIO[14] as source | 0xE
|  | BB_IQ_DATA_2_SRC_GPIO_15 | Select GPIO[15] as source | 0xF
|  | BB_IQ_DATA_2_SRC_CONST_LOW | Select constant low as source | 0x10
|  | BB_IQ_DATA_2_SRC_CONST_HIGH | Select constant high as source | 0x11
|  | BB_IQ_DATA_2_SRC_RF_IQ_DATA_2 | Select RF front-end IQ_DATA_2 as source | 0x12*
12:8 | IQ_DATA_1 | BB_IQ_DATA_1_SRC_GPIO_0 | Select GPIO[0] as source | 0x0
|  | BB_IQ_DATA_1_SRC_GPIO_1 | Select GPIO[1] as source | 0x1
|  | BB_IQ_DATA_1_SRC_GPIO_2 | Select GPIO[2] as source | 0x2
|  | BB_IQ_DATA_1_SRC_GPIO_3 | Select GPIO[3] as source | 0x3
|  | BB_IQ_DATA_1_SRC_GPIO_4 | Select GPIO[4] as source | 0x4
|  | BB_IQ_DATA_1_SRC_GPIO_5 | Select GPIO[5] as source | 0x5
|  | BB_IQ_DATA_1_SRC_GPIO_6 | Select GPIO[6] as source | 0x6
|  | BB_IQ_DATA_1_SRC_GPIO_7 | Select GPIO[7] as source | 0x7
|  | BB_IQ_DATA_1_SRC_GPIO_8 | Select GPIO[8] as source | 0x8
|  | BB_IQ_DATA_1_SRC_GPIO_9 | Select GPIO[9] as source | 0x9
|  | BB_IQ_DATA_1_SRC_GPIO_10 | Select GPIO[10] as source | 0xA
|  | BB_IQ_DATA_1_SRC_GPIO_11 | Select GPIO[11] as source | 0xB
|  | BB_IQ_DATA_1_SRC_GPIO_12 | Select GPIO[12] as source | 0xC
|  | BB_IQ_DATA_1_SRC_GPIO_13 | Select GPIO[13] as source | 0xD
|  | BB_IQ_DATA_1_SRC_GPIO_14 | Select GPIO[14] as source | 0xE
|  | BB_IQ_DATA_1_SRC_GPIO_15 | Select GPIO[15] as source | 0xF
|  | BB_IQ_DATA_1_SRC_CONST_LOW | Select constant low as source | 0x10
|  | BB_IQ_DATA_1_SRC_CONST_HIGH | Select constant high as source | 0x11
|  | BB_IQ_DATA_1_SRC_RF_IQ_DATA_1 | Select RF front-end IQ_DATA_1 as source | 0x12*
4:0 | IQ_DATA_0 | BB_IQ_DATA_0_SRC_GPIO_0 | Select GPIO[0] as source | 0x0
|  | BB_IQ_DATA_0_SRC_GPIO_1 | Select GPIO[1] as source | 0x1
|  | BB_IQ_DATA_0_SRC_GPIO_2 | Select GPIO[2] as source | 0x2
|  | BB_IQ_DATA_0_SRC_GPIO_3 | Select GPIO[3] as source | 0x3
|  | BB_IQ_DATA_0_SRC_GPIO_4 | Select GPIO[4] as source | 0x4
|  | BB_IQ_DATA_0_SRC_GPIO_5 | Select GPIO[5] as source | 0x5
|  | BB_IQ_DATA_0_SRC_GPIO_6 | Select GPIO[6] as source | 0x6
|  | BB_IQ_DATA_0_SRC_GPIO_7 | Select GPIO[7] as source | 0x7
|  | BB_IQ_DATA_0_SRC_GPIO_8 | Select GPIO[8] as source | 0x8
|  | BB_IQ_DATA_0_SRC_GPIO_9 | Select GPIO[9] as source | 0x9
|  | BB_IQ_DATA_0_SRC_GPIO_10 | Select GPIO[10] as source | 0xA
|  | BB_IQ_DATA_0_SRC_GPIO_11 | Select GPIO[11] as source | 0xB
|  | BB_IQ_DATA_0_SRC_GPIO_12 | Select GPIO[12] as source | 0xC
|  | BB_IQ_DATA_0_SRC_GPIO_13 | Select GPIO[13] as source | 0xD
|  | BB_IQ_DATA_0_SRC_GPIO_14 | Select GPIO[14] as source | 0xE
|  | BB_IQ_DATA_0_SRC_GPIO_15 | Select GPIO[15] as source | 0xF
|  | BB_IQ_DATA_0_SRC_CONST_LOW | Select constant low as source | 0x10
|  | BB_IQ_DATA_0_SRC_CONST_HIGH | Select constant high as source | 0x11
|  | BB_IQ_DATA_0_SRC_RF_IQ_DATA_0 | Select RF front-end IQ_DATA_0 as source | 0x12*