### BB_RADIOPWRUPDN2

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
31:24 | RW | SYNC_POSITION2 | Access address detection pulse/level position for coded PHY at 125kbps
23:16 | RW | RXPWRUP2 | Radio Rx power up (in us) for coded PHY at 125kbps
14:8 | RW | TXPWRDN2 | Radio Tx power down (in us) for coded PHY at 125kbps
7:0 | RW | TXPWRUP2 | Radio Tx power up (in us) for coded PHY at 125kbps

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
31:24 | SYNC_POSITION2 | SYNC_POSITION2_0 |  | 0x0*
23:16 | RXPWRUP2 | RXPWRUP2_0 |  | 0x0*
14:8 | TXPWRDN2 | TXPWRDN2_0 |  | 0x0*
7:0 | TXPWRUP2 | TXPWRUP2_0 |  | 0x0*