### BB_RFTESTCNTL

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
31 | RW | INFINITERX | Applicable in RF test mode only
27 | RW | RXPKTCNTEN | Applicable in RF test mode only
25:24 | RW | PERCOUNT_MODE | Applicable in RF direct Rx test mode only, and when RXPKTCNTEN equals to 1
15 | RW | INFINITETX | Applicable in RF test mode only
14 | RW | TXLENGTHSRC | Applicable only in Tx/Rx RF test mode
13 | RW | PRBSTYPE | Applicable only in Tx/Rx RF test mode
12 | RW | TXPLDSRC | Applicable only in Tx/Rx RF test mode
11 | RW | TXPKTCNTEN | Applicable in RF test mode only
7:0 | RW | TXLENGTH | Tx packet length in number of byte

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
31 | INFINITERX | INFINITERX_0 | Normal mode of operation | 0x0*
|  | INFINITERX_1 | Infinite Rx window | 0x1
27 | RXPKTCNTEN | RXPKTCNTEN_0 | Rx packet count disabled | 0x0*
25:24 | PERCOUNT_MODE | PERCOUNT_MODE_0 | Counts number of correctly received packets (no error) | 0x0*
|  | PERCOUNT_MODE_1 | Counts number of Access Address error detection only | 0x1
|  | PERCOUNT_MODE_2 | Counts number of CRC Error detection only (or any error leading to CRC error, such as length error or Rx time error) | 0x2
|  | PERCOUNT_MODE_3 | Counts Reception Error detected | 0x3
15 | INFINITETX | INFINITETX_0 | Normal mode of operation | 0x0*
|  | INFINITETX_1 | Infinite Tx packet / Normal start of a packet but endless payload | 0x1
14 | TXLENGTHSRC | TXLENGTHSRC_0 | Normal mode of operation: TxDESC-TXADVLEN controls the Tx packet payload size | 0x0*
|  | TXLENGTHSRC_1 | Uses RFTESTCTRL-TXLENGTH packet length (can support up to 512 bytes transmit) | 0x1
13 | PRBSTYPE | PRBSTYPE_0 | Tx packet payload are PRBS9 type | 0x0*
|  | PRBSTYPE_1 | Tx packet payload are PRBS15 type | 0x1
12 | TXPLDSRC | TXPLDSRC_0 | Tx packet payload source is the control structure | 0x0*
|  | TXPLDSRC_1 | Tx packet payload are PRBS generator | 0x1
11 | TXPKTCNTEN | TXPKTCNTEN_0 | Tx packet count disabled | 0x0*
|  | TXPKTCNTEN_1 | Tx packet count enabled, and reported in CS-TXCCMPKTCNT and RFTESTTXSTAT-TXPKTCNT on RF abort command | 0x1
7:0 | TXLENGTH | TXLENGTH_0 |  | 0x0*