### SYSCTRL_NS_ACCESS_PERIPH_CFG0

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
28 | RW | PWM_ACCESS | Allow Non-Secure code to access the PWM
27 | RW | LIN_ACCESS | Allow Non-Secure code to access the LIN[0:0]
26 | RW | TOF_ACCESS | Allow Non-Secure code to access the TOF
25 | RW | PCM_ACCESS | Allow Non-Secure code to access the PCM[0:0]
24 | RW | UART_ACCESS | Allow Non-Secure code to access the UART[0:0]
23:22 | RW | I2C_ACCESS | Allow Non-Secure code to access the I2C[1:0]
21:20 | RW | SPI_ACCESS | Allow Non-Secure code to access the SPI[1:0]
19 | RW | GPIO_SRC_ACCESS | Allow Non-Secure code to access the GPIO_SRC
18 | RW | GPIO_ACCESS | Allow Non-Secure code to access the GPIO
17 | RW | CC312_ACCESS | Allow Non-Secure code to access the CC312
16 | RW | ASCC_ACCESS | Allow Non-Secure code to access the ASCC
15:12 | RW | TIMER_ACCESS | Allow Non-Secure code to access the Timer[3:0]
10 | RW | CRC_ACCESS | Allow Non-Secure code to access the CRC
8 | RW | NMI_ACCESS | Allow Non-Secure code to access the NMI
7 | RW | WATCHDOG_ACCESS | Allow Non-Secure code to access the Watchdog
6 | RW | SYSCTRL_ACCESS | Allow Non-Secure code to access the SYSCTRL
5 | RW | SENSOR_ACCESS | Allow Non-Secure code to access the Sensor
4 | RW | ACS_ACCESS | Allow Non-Secure code to access the ACS
3 | RW | LSAD_ACCESS | Allow Non-Secure code to access the LSAD config
2 | RW | TEST_CTRL_ACCESS | Allow Non-Secure code to access the TEST_CTRL config
1 | RW | CLK_ACCESS | Allow Non-Secure code to access the CLK config
0 | RW | RESET_ACCESS | Allow Non-Secure code to access the Reset

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
28 | PWM_ACCESS | NS_CANNOT_ACCESS_PWM | Non-Secure code cannot access the PWM | 0x0*
|  | NS_CAN_ACCESS_PWM | Non-Secure code can access the PWM | 0x1
27 | LIN_ACCESS | NS_CANNOT_ACCESS_LIN | Non-Secure code cannot access the LIN | 0x0*
|  | NS_CAN_ACCESS_LIN | Non-Secure code can access the LIN | 0x1
26 | TOF_ACCESS | NS_CANNOT_ACCESS_TOF | Non-Secure code cannot access the TOF | 0x0*
|  | NS_CAN_ACCESS_TOF | Non-Secure code can access the TOF | 0x1
25 | PCM_ACCESS | NS_CANNOT_ACCESS_PCM0 | Non-Secure code cannot access the PCM0 | 0x0*
|  | NS_CAN_ACCESS_PCM0 | Non-Secure code can access the PCM0 | 0x1
24 | UART_ACCESS | NS_CANNOT_ACCESS_UART0 | Non-Secure code cannot access the UART0 | 0x0*
|  | NS_CAN_ACCESS_UART0 | Non-Secure code can access the UART0 | 0x1
23:22 | I2C_ACCESS | NS_CANNOT_ACCESS_I2C0 | Non-Secure code cannot access the I2C0 | 0x0*
|  | NS_CANNOT_ACCESS_I2C1 | Non-Secure code cannot access the I2C1 | 0x0*
|  | NS_CAN_ACCESS_I2C0 | Non-Secure code can access the I2C0 | 0x1
|  | NS_CAN_ACCESS_I2C1 | Non-Secure code can access the I2C1 | 0x2
21:20 | SPI_ACCESS | NS_CANNOT_ACCESS_SPI0 | Non-Secure code cannot access the SPI0 | 0x0*
|  | NS_CANNOT_ACCESS_SPI1 | Non-Secure code cannot access the SPI1 | 0x0*
|  | NS_CAN_ACCESS_SPI0 | Non-Secure code can access the SPI0 | 0x1
|  | NS_CAN_ACCESS_SPI1 | Non-Secure code can access the SPI1 | 0x2
19 | GPIO_SRC_ACCESS | NS_CANNOT_ACCESS_GPIO_SRC | Non-Secure code cannot access the GPIO_SRC | 0x0*
|  | NS_CAN_ACCESS_GPIO_SRC | Non-Secure code can access the GPIO_SRC | 0x1
18 | GPIO_ACCESS | NS_CANNOT_ACCESS_GPIO | Non-Secure code cannot access the GPIO | 0x0*
|  | NS_CAN_ACCESS_GPIO | Non-Secure code can access the GPIO | 0x1
17 | CC312_ACCESS | NS_CANNOT_ACCESS_CC312 | Non-Secure code cannot access the CC312 | 0x0*
|  | NS_CAN_ACCESS_CC312 | Non-Secure code can access the CC312 | 0x1
16 | ASCC_ACCESS | NS_CANNOT_ACCESS_ASCC | Non-Secure code cannot access the ASCC | 0x0*
|  | NS_CAN_ACCESS_ASCC | Non-Secure code can access the ASCC | 0x1
15:12 | TIMER_ACCESS | NS_CANNOT_ACCESS_TIMER0 | Non-Secure code cannot access the Timer0 | 0x0*
|  | NS_CANNOT_ACCESS_TIMER1 | Non-Secure code cannot access the Timer1 | 0x0*
|  | NS_CANNOT_ACCESS_TIMER2 | Non-Secure code cannot access the Timer2 | 0x0*
|  | NS_CANNOT_ACCESS_TIMER3 | Non-Secure code cannot access the Timer3 | 0x0*
|  | NS_CAN_ACCESS_TIMER0 | Non-Secure code can access the Timer0 | 0x1
|  | NS_CAN_ACCESS_TIMER1 | Non-Secure code can access the Timer1 | 0x2
|  | NS_CAN_ACCESS_TIMER2 | Non-Secure code can access the Timer2 | 0x4
|  | NS_CAN_ACCESS_TIMER3 | Non-Secure code can access the Timer3 | 0x8
10 | CRC_ACCESS | NS_CANNOT_ACCESS_CRC | Non-Secure code cannot access the CRC | 0x0*
|  | NS_CAN_ACCESS_CRC | Non-Secure code can access the CRC | 0x1
8 | NMI_ACCESS | NS_CANNOT_ACCESS_NMI | Non-Secure code cannot access the NMI | 0x0*
|  | NS_CAN_ACCESS_NMI | Non-Secure code can access the NMI | 0x1
7 | WATCHDOG_ACCESS | NS_CANNOT_ACCESS_WATCHDOG | Non-Secure code cannot access the Watchdog | 0x0*
|  | NS_CAN_ACCESS_WATCHDOG | Non-Secure code can access the Watchdog | 0x1
6 | SYSCTRL_ACCESS | NS_CANNOT_ACCESS_SYSCTRL | Non-Secure code cannot access the SYSCTRL | 0x0*
|  | NS_CAN_ACCESS_SYSCTRL | Non-Secure code can access the SYSCTRL | 0x1
5 | SENSOR_ACCESS | NS_CANNOT_ACCESS_SENSOR | Non-Secure code cannot access the Sensor | 0x0*
|  | NS_CAN_ACCESS_SENSOR | Non-Secure code can access the Sensor | 0x1
4 | ACS_ACCESS | NS_CANNOT_ACCESS_ACS | Non-Secure code cannot access the ACS | 0x0*
|  | NS_CAN_ACCESS_ACS | Non-Secure code can access the ACS | 0x1
3 | LSAD_ACCESS | NS_CANNOT_ACCESS_LSAD | Non-Secure code cannot access the LSAD | 0x0*
|  | NS_CAN_ACCESS_LSAD | Non-Secure code can access the LSAD | 0x1
2 | TEST_CTRL_ACCESS | NS_CANNOT_ACCESS_TEST_CTRL | Non-Secure code cannot access the TEST_CTRL | 0x0*
|  | NS_CAN_ACCESS_TEST_CTRL | Non-Secure code can access the TEST_CTRL | 0x1
1 | CLK_ACCESS | NS_CANNOT_ACCESS_CLK | Non-Secure code cannot access the CLK config | 0x0*
|  | NS_CAN_ACCESS_CLK | Non-Secure code can access the CLK config | 0x1
0 | RESET_ACCESS | NS_CANNOT_ACCESS_RESET | Non-Secure code cannot access the Reset | 0x0*
|  | NS_CAN_ACCESS_RESET | Non-Secure code can access the Reset | 0x1