### RF_REG53

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
23:16 | R | RSSI_MAX_RM | Remapped register of RSSI_MAX
15:8 | R | RSSI_MIN_RM | Remapped register of RSSI_MIN
7:0 | R | RSSI_AVG_RM | Remapped register of RSSI_AVG

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
23:16 | RSSI_MAX_RM | RSSI_MAX_RM_DEFAULT | The remapped registers are accessible over SPI only | 0x0*
15:8 | RSSI_MIN_RM | RSSI_MIN_RM_DEFAULT | The remapped registers are accessible over SPI only | 0x0*
7:0 | RSSI_AVG_RM | RSSI_AVG_RM_DEFAULT | The remapped registers are accessible over SPI only | 0x0*