### RF_CTE_OPTS

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
29 | RW | CTE_OPTS_RECT_PS_CTE | Use rectangular pulse shape during the CTE
28 | RW | CTE_OPTS_USE_CTE_WO_CP | Enable the CTE without reading or inserting the CP
27 | RW | CTE_OPTS_CTE_AMPL | Enable the usage of the RSSI values to adapt the amplitude of the IQ signal based to the RSSI value
26 | RW | CTE_OPTS_DF_AOA_SLOT_TIME | Indicate the switching/sampling slot period for AoA
25 | RW | CTE_OPTS_CP_INSERT | Force the CP bit in the packet header to 1
24 | RW | CTE_OPTS_EN_READ_CP | CP bit is read in the packet header (BLE standard)
23:16 | RW | CTE_OPTS_CTE_INFO | Set the CTEInfo field in the packet header while cp_insert is set to 1
14:10 | RW | ASK_MOD_ASK_MAX | Set the maximum value for the ASK modulation
9:5 | RW | ASK_MOD_ASK_MIN | Set the minimum value for the ASK modulation
4:1 | RW | ASK_MOD_ASK_CNT | Set the how long to count for the ASK modulation
0 | RW | ASK_MOD_EN_RSSI_ASK | PA will perform an ASK modulation

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
29 | CTE_OPTS_RECT_PS_CTE | CTE_OPTS_RECT_PS_CTE_DISABLE | Disable CTE with rectangular pulse shaping | 0x0*
|  | CTE_OPTS_RECT_PS_CTE_ENABLE | Enable CTE with rectangular pulse shaping | 0x1
28 | CTE_OPTS_USE_CTE_WO_CP | CTE_OPTS_USE_CTE_WO_CP_DISABLE | Disable CTE without reading CP | 0x0*
|  | CTE_OPTS_USE_CTE_WO_CP_ENABLE | Enable CTE without reading CP | 0x1
27 | CTE_OPTS_CTE_AMPL | CTE_OPTS_CTE_AMPL_DISABLE | Disable RSSI for IQ signal validation | 0x0*
|  | CTE_OPTS_CTE_AMPL_ENABLE | Enable RSSI for IQ signal validation | 0x1
26 | CTE_OPTS_DF_AOA_SLOT_TIME | CTE_OPTS_DF_AOA_SLOT_TIME_1 | 1us switching period | 0x0*
|  | CTE_OPTS_DF_AOA_SLOT_TIME_2 | 2us switching period | 0x1
25 | CTE_OPTS_CP_INSERT | CTE_OPTS_CP_INSERT_DISABLE | Disable forcing CP bit to 1 | 0x0*
|  | CTE_OPTS_CP_INSERT_ENABLE | Enable forcing CP bit to 1 | 0x1
24 | CTE_OPTS_EN_READ_CP | CTE_OPTS_EN_READ_CP_DISABLE | Disable reading CP bit | 0x0*
|  | CTE_OPTS_EN_READ_CP_ENABLE | Enable reading CP bit | 0x1
23:16 | CTE_OPTS_CTE_INFO | CTE_OPTS_CTE_INFO_DEFAULT |  | 0x0*
14:10 | ASK_MOD_ASK_MAX | ASK_MOD_ASK_MAX_DEFAULT |  | 0xC*
9:5 | ASK_MOD_ASK_MIN | ASK_MOD_ASK_MIN_DEFAULT |  | 0x0*
4:1 | ASK_MOD_ASK_CNT | ASK_MOD_ASK_CNT_DEFAULT |  | 0x7*
0 | ASK_MOD_EN_RSSI_ASK | ASK_MOD_EN_RSSI_ASK_DISABLE | Disable PA ASK modulation | 0x0*
|  | ASK_MOD_EN_RSSI_ASK_ENABLE | Enable PA ASK modulation | 0x1