### ACS_VDDM_CTRL

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
24 | R | READY | Supply ready
21:16 | RW | STANDBY_VTRIM | VDDM standby voltage trimming (10 mV steps)
12 | RW | ENABLE_LOW_BIAS | Low power mode control
8 | RW | SLEEP_CLAMP | Sleep mode clamp control
5:0 | RW | VTRIM | Output voltage trimming configuration in 10 mV steps

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
24 | READY | VDDM_NOT_READY | Supply voltage not ready | 0x0*
|  | VDDM_READY | Supply voltage ready | 0x1
21:16 | STANDBY_VTRIM | VDDM_STANDBY_TRIM_0P75V | 0.75 V | 0x0
|  | VDDM_STANDBY_TRIM_0P76V | 0.76 V | 0x1
|  | VDDM_STANDBY_TRIM_1P20V | 1.2 V | 0x2D*
|  | VDDM_STANDBY_TRIM_1P32V | 1.32 V | 0x39
|  | VDDM_STANDBY_TRIM_1P38V | 1.38 V | 0x3F
12 | ENABLE_LOW_BIAS | VDDM_NOMINAL_BIAS | Nominal regulator biasing | 0x0*
|  | VDDM_LOW_BIAS | Low regulator biasing | 0x1
8 | SLEEP_CLAMP | VDDM_SLEEP_HIZ | Set the output HIZ (floating) in sleep mode | 0x0*
|  | VDDM_SLEEP_GND | Clamp output to ground in sleep mode | 0x1
5:0 | VTRIM | VDDM_TRIM_0P75V | 0.75 V | 0x0
|  | VDDM_TRIM_0P76V | 0.76 V | 0x1
|  | VDDM_TRIM_1P00V | 1.0 V | 0x19
|  | VDDM_TRIM_1P08V | 1.08 V | 0x21
|  | VDDM_TRIM_1P10V | 1.1 V | 0x23
|  | VDDM_TRIM_1P15V | 1.15 V | 0x28*
|  | VDDM_TRIM_1P20V | 1.2 V | 0x2D
|  | VDDM_TRIM_1P25V | 1.25 V | 0x32
|  | VDDM_TRIM_1P32V | 1.32 V | 0x39
|  | VDDM_TRIM_1P38V | 1.38 V | 0x3F