### GPIO_INT_STATUS

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
4 | R | GPIO_INT_STATUS | GPIO interrupt status
0 | W | GPIO_INT_CLEAR | GPIO interrupt clear

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
4 | GPIO_INT_STATUS | GPIO_INT_FALSE | Interrupt not triggered | 0x0*
|  | GPIO_INT_TRUE | Interrupt triggered | 0x1
0 | GPIO_INT_CLEAR | GPIO_INT_CLEAR | Interrupt clear | 0x1