### FLASH_ECC_STATUS

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
6 | W | ECC_COR_ERROR_CNT_CLEAR | Reset the Flash corrected errors counter
5 | W | ECC_UNCOR_ERROR_CNT_CLEAR | Reset the Flash uncorrected errors counter
4 | W | ECC_ERROR_ADDR_CLEAR | Reset the Flash address of the last detected error
1 | R | ECC_COR_ERROR_CNT_STATUS | FLASH_ECC_ERROR_COR_CNT status
0 | R | ECC_UNCOR_ERROR_CNT_STATUS | FLASH_ECC_ERROR_UNCOR_CNT status

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
6 | ECC_COR_ERROR_CNT_CLEAR | FLASH_ECC_COR_ERROR_CNT_CLEAR | Reset the Flash corrected errors counter | 0x1
5 | ECC_UNCOR_ERROR_CNT_CLEAR | FLASH_ECC_UNCOR_ERROR_CNT_CLEAR | Reset the Flash uncorrected errors counter | 0x1
4 | ECC_ERROR_ADDR_CLEAR | FLASH_ECC_ERROR_ADDR_CLEAR | Reset the Flash address of the latest detected error | 0x1
1 | ECC_COR_ERROR_CNT_STATUS | FLASH_ECC_NO_CORRECTED_ERROR | Indicates FLASH_ECC_COR_ERROR_CNT is zero | 0x0*
|  | FLASH_ECC_CORRECTED_ERROR | Indicates FLASH_ECC_COR_ERROR_CNT is not zero | 0x1
0 | ECC_UNCOR_ERROR_CNT_STATUS | FLASH_ECC_NO_UNCORRECTED_ERROR | Indicates FLASH_ECC_UNCOR_ERROR_CNT is zero | 0x0*
|  | FLASH_ECC_UNCORRECTED_ERROR | Indicates FLASH_ECC_UNCOR_ERROR_CNT is not zero | 0x1