### ACS_CLK_DET_CTRL

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
8 | R | CLOCK_PRESENT | Clock present flag
1 | RW | RESET_IGNORE | Clock detector reset condition ignore
0 | RW | ENABLE | Clock detector enable

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
8 | CLOCK_PRESENT | ACS_CLK_DET_NO_CLOCK | No clock detected | 0x0
|  | ACS_CLK_DET_CLOCK_PRESENT | Clock detected | 0x1*
1 | RESET_IGNORE | ACS_CLK_DET_RESET_DISABLE | Clock detector reset condition ignore | 0x1
|  | ACS_CLK_DET_RESET_ENABLE | Clock detector reset condition accept | 0x0*
0 | ENABLE | ACS_CLK_DET_ENABLE | Clock detector enable | 0x1*
|  | ACS_CLK_DET_DISABLE | Clock detector disable | 0x0