### RF_IRQ_STATUS

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
5 | R | IRQ_STATUS_FLAG_RXFIFO | IRQ RXFIFO status
4 | R | IRQ_STATUS_FLAG_TXFIFO | IRQ TXFIFO status
3 | R | IRQ_STATUS_FLAG_SYNC | IRQ SYNC status
2 | R | IRQ_STATUS_FLAG_RECEIVED | IRQ RECEIVED status
1 | R | IRQ_STATUS_FLAG_RXSTOP | IRQ RXSTOP status
0 | R | IRQ_STATUS_FLAG_TX | IRQ Tx status

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
5 | IRQ_STATUS_FLAG_RXFIFO | IRQ_STATUS_FLAG_RXFIFO_IDLE | IRQ RXFIFO is not active | 0x0*
|  | IRQ_STATUS_FLAG_RXFIFO_ACTIVE | IRQ RXFIFO is active | 0x1
4 | IRQ_STATUS_FLAG_TXFIFO | IRQ_STATUS_FLAG_TXFIFO_IDLE | IRQ TXFIFO is not active | 0x0*
|  | IRQ_STATUS_FLAG_TXFIFO_ACTIVE | IRQ TXFIFO is active | 0x1
3 | IRQ_STATUS_FLAG_SYNC | IRQ_STATUS_FLAG_SYNC_IDLE | IRQ SYNC is not active | 0x0*
|  | IRQ_STATUS_FLAG_SYNC_ACTIVE | IRQ SYNC is active | 0x1
2 | IRQ_STATUS_FLAG_RECEIVED | IRQ_STATUS_FLAG_RECEIVED_IDLE | IRQ RECEIVED is not active | 0x0*
|  | IRQ_STATUS_FLAG_RECEIVED_ACTIVE | IRQ RECEIVED is active | 0x1
1 | IRQ_STATUS_FLAG_RXSTOP | IRQ_STATUS_FLAG_RXSTOP_IDLE | IRQ RXSTOP is not active | 0x0*
|  | IRQ_STATUS_FLAG_RXSTOP_ACTIVE | IRQ RXSTOP is active | 0x1
0 | IRQ_STATUS_FLAG_TX | IRQ_STATUS_FLAG_TX_IDLE | IRQ TX is not active | 0x0*
|  | IRQ_STATUS_FLAG_TX_ACTIVE | IRQ TX is active | 0x1