### ACS_RESET_STATUS

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
25 | R | CCAO_REBOOT_RESET_FLAG | Sticky flag that detects that a CryptoCell Alway ON reboot reset occurred
24 | R | WRONG_STATE_RESET_FLAG | Sticky flag that detects that a wrong state reset occurred
23 | R | TIMEOUT_RESET_FLAG | Sticky flag that detects that a timeout in the power up sequence occurred
22 | R | CLK_DET_RESET_FLAG | Sticky flag that detects that a clock detector reset occurred
21 | R | VDDFLASH_RESET_FLAG | Sticky flag that detects that a VDDFLASH reset occurred (triggered by VDDFLASH_ready = 0)
20 | R | VDDM_RESET_FLAG | Sticky flag that detects that a VDDM reset occurred (triggered by VDDM_ready = 0)
19 | R | VDDC_RESET_FLAG | Sticky flag that detects that a VDDC reset occurred (triggered by VDDC_ready = 0)
18 | R | BG_VREF_RESET_FLAG | Sticky flag that detects that a Bandagap reference voltage reset occurred
17 | R | PAD_RESET_FLAG | Sticky flag that detects that a reset occurred due to pad NRESET
16 | R | POR_RESET_FLAG | Sticky flag that detects that a POR reset occurred
9 | W | CCAO_REBOOT_RESET_FLAG_CLEAR | Reset the sticky CCAO_REBOOT_RESET flag.
8 | W | WRONG_STATE_RESET_FLAG_CLEAR | Reset the sticky WRONG_STATE_RESET flag.
7 | W | TIMEOUT_RESET_FLAG_CLEAR | Reset the sticky TIMEOUT_RESET flag.
6 | W | CLK_DET_RESET_FLAG_CLEAR | Reset the sticky CLK_DET_RESET flag.
5 | W | VDDFLASH_RESET_FLAG_CLEAR | Reset the sticky VDDFLASH_RESET flag.
4 | W | VDDM_RESET_FLAG_CLEAR | Reset the sticky VDDM_RESET flag.
3 | W | VDDC_RESET_FLAG_CLEAR | Reset the sticky VDDC_RESET flag.
2 | W | BG_VREF_RESET_FLAG_CLEAR | Reset the sticky BG_VREF_RESET flag.
1 | W | PAD_RESET_FLAG_CLEAR | Reset the sticky PAD_RESET flag.
0 | W | POR_RESET_FLAG_CLEAR | Reset the sticky POR_RESET flag.

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
25 | CCAO_REBOOT_RESET_FLAG | CCAO_REBOOT_RESET_FLAG_NOT_SET | The CryptoCell Always ON reboot reset has not triggered at least once | 0x0
|  | CCAO_REBOOT_RESET_FLAG_SET | The CryptoCell Always ON reboot reset was triggered at least once since this status bit was last cleared | 0x1*
24 | WRONG_STATE_RESET_FLAG | WRONG_STATE_RESET_FLAG_NOT_SET | The wrong state reset has not triggered at least once | 0x0
|  | WRONG_STATE_RESET_FLAG_SET | The wrong state reset was triggered at least once since this status bit was last cleared | 0x1*
23 | TIMEOUT_RESET_FLAG | TIMEOUT_RESET_FLAG_NOT_SET | The timeout reset has not triggered at least once | 0x0
|  | TIMEOUT_RESET_FLAG_SET | The timeout reset was triggered at least once since this status bit was last cleared | 0x1*
22 | CLK_DET_RESET_FLAG | CLK_DET_RESET_FLAG_NOT_SET | The clock detector reset has not triggered at least once | 0x0
|  | CLK_DET_RESET_FLAG_SET | The clock detector reset was triggered at least once since this status bit was last cleared | 0x1*
21 | VDDFLASH_RESET_FLAG | VDDFLASH_RESET_FLAG_NOT_SET | The VDDFLASH reset has not triggered at least once | 0x0
|  | VDDFLASH_RESET_FLAG_SET | The VDDFLASH reset was triggered at least once since this status bit was last cleared | 0x1*
20 | VDDM_RESET_FLAG | VDDM_RESET_FLAG_NOT_SET | The VDDM reset has not triggered at least once | 0x0
|  | VDDM_RESET_FLAG_SET | The VDDM reset was triggered at least once since this status bit was last cleared | 0x1*
19 | VDDC_RESET_FLAG | VDDC_RESET_FLAG_NOT_SET | The VDDC reset has not triggered at least once | 0x0
|  | VDDC_RESET_FLAG_SET | The VDDC reset was triggered at least once since this status bit was last cleared | 0x1*
18 | BG_VREF_RESET_FLAG | BG_VREF_RESET_FLAG_NOT_SET | The band-gap reference voltage reset has not triggered at least once | 0x0
|  | BG_VREF_RESET_FLAG_SET | The band-gap reference voltage was triggered at least once since this status bit was last cleared | 0x1*
17 | PAD_RESET_FLAG | PAD_RESET_FLAG_NOT_SET | The NRESET pad reset has not triggered at least once | 0x0
|  | PAD_RESET_FLAG_SET | The NRESET pad reset was triggered at least once since this status bit was last cleared | 0x1*
16 | POR_RESET_FLAG | POR_RESET_FLAG_NOT_SET | The POR reset has not triggered at least once | 0x0
|  | POR_RESET_FLAG_SET | The POR reset was triggered at least once since this status bit was last cleared | 0x1*
9 | CCAO_REBOOT_RESET_FLAG_CLEAR | CCAO_REBOOT_RESET_FLAG_CLEAR | Reset the sticky CCAO_REBOOT_RESET flag. | 0x1
8 | WRONG_STATE_RESET_FLAG_CLEAR | WRONG_STATE_RESET_FLAG_CLEAR | Reset the sticky WRONG_STATE_RESET flag. | 0x1
7 | TIMEOUT_RESET_FLAG_CLEAR | TIMEOUT_RESET_FLAG_CLEAR | Reset the sticky TIMEOUT_RESET flag. | 0x1
6 | CLK_DET_RESET_FLAG_CLEAR | CLK_DET_RESET_FLAG_CLEAR | Reset the sticky CLK_DET_RESET flag. | 0x1
5 | VDDFLASH_RESET_FLAG_CLEAR | VDDFLASH_RESET_FLAG_CLEAR | Reset the sticky VDDFLASH_RESET flag. | 0x1
4 | VDDM_RESET_FLAG_CLEAR | VDDM_RESET_FLAG_CLEAR | Reset the sticky VDDM_RESET flag. | 0x1
3 | VDDC_RESET_FLAG_CLEAR | VDDC_RESET_FLAG_CLEAR | Reset the sticky VDDC_RESET flag. | 0x1
2 | BG_VREF_RESET_FLAG_CLEAR | BG_VREF_RESET_FLAG_CLEAR | Reset the sticky BG_VREF_RESET flag. | 0x1
1 | PAD_RESET_FLAG_CLEAR | PAD_RESET_FLAG_CLEAR | Reset the sticky PAD_RESET flag. | 0x1
0 | POR_RESET_FLAG_CLEAR | POR_RESET_FLAG_CLEAR | Reset the sticky POR_RESET flag. | 0x1