### SYSCTRL_CC_DCU_LOCK1

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
31:16 | R | CC_DCU_LOCK_OEM_GP | Always On OEM governed dcu_en1 general purpose bits lock
15:13 | R | CC_DCU_LOCK_OEM_SEC_RST | Always On OEM governed secure reset lock. All bits must be locked to assure that the state is locked
12:10 | R | CC_DCU_LOCK_OEM_SPINDEN | Always On OEM governed CM33 secure non-intrusive debug enable control lock. All bits must be locked to assure that the state is locked
9:7 | R | CC_DCU_LOCK_OEM_SPIDEN | Always On OEM governed CM33 secure intrusive debug enable control lock. All bits must be locked to assure that the state is locked
6:4 | R | CC_DCU_LOCK_OEM_NIDEN | Always On OEM governed CM33 non-intrusive debug enable control lock. All bits must be locked to assure that the state is locked
3:1 | R | CC_DCU_LOCK_OEM_DBGEN | Always On OEM governed CM33 debug enable control lock. All bits must be locked to assure that the state is locked
0 | R | CC_DCU_LOCK_OEM_RESERVED | Always On OEM allocated reserved bit (unused)