### RF_CTE_IF

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
25:16 | RW | CTE_CTRL_DELAY_TX_DF_DELAY_TX | Delay (in 62.5ns) form the serializer up to the antenna in direction finding (banked)
15 | RW | ANTENNA_CONF_DF_IND_PATTERN | Separate the antenna switching pattern from the reference one
14 | RW | ANTENNA_CONF_DF_IND_ANTENNA | Make the antenna for DF independent from the rest of the packet
13:8 | RW | ANTENNA_CONF_ANT_LUT_M | Number of states used (-1) in the antenna LUT
5 | RW | CTE_AUTO_PULL_EXT_IQ_SMP_TYPE | Select the external IQ sample signal qualifier type
4 | RW | CTE_AUTO_PULL_IQ_MSB | Select which signal is sent over the MSB in case of a 16bits buffers
3:2 | RW | CTE_AUTO_PULL_IQ_DATA_BUS_SIZE | Select the bus data size of IQ signals
1 | RW | CTE_AUTO_PULL_CTE_QUAL | Select the CTE data qualifier
0 | RW | CTE_AUTO_PULL_EN_CTE_AUTO_PULL | Enable the automatic push of CTE data to an external IP

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
25:16 | CTE_CTRL_DELAY_TX_DF_DELAY_TX | CTE_CTRL_DELAY_TX_DF_DELAY_TX_DEFAULT |  | 0x0*
15 | ANTENNA_CONF_DF_IND_PATTERN | ANTENNA_CONF_DF_IND_PATTERN_DISABLE | Disable the seperation of the antenna switching pattern | 0x0*
|  | ANTENNA_CONF_DF_IND_PATTERN_ENABLE | Enable the seperation of the antenna switching pattern | 0x1
14 | ANTENNA_CONF_DF_IND_ANTENNA | ANTENNA_CONF_DF_IND_ANTENNA_DISABLE | Disable the independancy of the antenna | 0x0*
|  | ANTENNA_CONF_DF_IND_ANTENNA_ENABLE | Enable the independancy of the antenna | 0x1
13:8 | ANTENNA_CONF_ANT_LUT_M | ANTENNA_CONF_ANT_LUT_M_DEFAULT |  | 0x0*
5 | CTE_AUTO_PULL_EXT_IQ_SMP_TYPE | CTE_AUTO_PULL_EXT_IQ_SMP_TYPE_PULSE | Pulse | 0x0*
|  | CTE_AUTO_PULL_EXT_IQ_SMP_TYPE_TOGGLE | Toggle | 0x1
4 | CTE_AUTO_PULL_IQ_MSB | CTE_AUTO_PULL_IQ_MSB_Q | I LSB, Q MSB | 0x0*
|  | CTE_AUTO_PULL_IQ_MSB_I | Q LSB, I MSB | 0x1
3:2 | CTE_AUTO_PULL_IQ_DATA_BUS_SIZE | CTE_AUTO_PULL_IQ_DATA_BUS_SIZE_4 | 4 bits | 0x0*
|  | CTE_AUTO_PULL_IQ_DATA_BUS_SIZE_8 | 8 bits | 0x1
|  | CTE_AUTO_PULL_IQ_DATA_BUS_SIZE_16 | 16 bits | 0x2
1 | CTE_AUTO_PULL_CTE_QUAL | CTE_AUTO_PULL_CTE_QUAL_TOGGLE | Toggling signal | 0x0*
|  | CTE_AUTO_PULL_CTE_QUAL_CLOCK | Clock signal | 0x1
0 | CTE_AUTO_PULL_EN_CTE_AUTO_PULL | CTE_AUTO_PULL_EN_CTE_AUTO_PULL_DISABLE | Disable automatic push of CTE data | 0x0*
|  | CTE_AUTO_PULL_EN_CTE_AUTO_PULL_ENABLE | Enable automatic push of CTE data | 0x1