### BB_AESCNTL

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
1 | RW | AES_MODE | Cipher mode control
0 | RW | AES_START | Start AES-128 ciphering/deciphering process

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
1 | AES_MODE | AES_MODE_0 | Cipher mode | 0x0*
|  | AES_MODE_1 | Decipher mode | 0x1
0 | AES_START | AES_START_0 |  | 0x0*
|  | AES_START_1 | Starts AES-128 ciphering/deciphering process (the bit is reset once the process is finished) | 0x1