### FLASH_NVM_STATUS

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
16 | W | CLEAR_NVM_STATUS | Clear all the NVM status bits
8 | R | NVM_BIT_FAILURE | Indicates if a bit has failed in an address from the CC-NVM layout used by the CryptoCell
5:0 | R | FAILED_NVM_ADDRESS | Last failing word address in CC-NVM layout (0x00 to 0x3F)

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
16 | CLEAR_NVM_STATUS | CLEAR_NVM_STATUS | Clear all the NVM status bits | 0x1
8 | NVM_BIT_FAILURE | NVM_OK | No bit failure detection in the CC-NVM layout | 0x0*
|  | NVM_BIT_FAILED | At least a bit has failed in the CC-NVM layout | 0x1