### FLASH_MAIN_CTRL

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
11 | RW | DATA_A_35K_TO_40K_W_EN | Authorize the write access to the Flash MAIN Data array from 35K to 40K word block through the FLASH_IF registers.
10 | RW | DATA_A_30K_TO_35K_W_EN | Authorize the write access to the Flash MAIN Data array from 30K to 35K word block through the FLASH_IF registers.
9 | RW | DATA_A_25K_TO_30K_W_EN | Authorize the write access to the Flash MAIN Data array from 25K to 30K word block through the FLASH_IF registers.
8 | RW | DATA_A_20K_TO_25K_W_EN | Authorize the write access to the Flash MAIN Data array from 20K to 25K word block through the FLASH_IF registers.
7 | RW | DATA_A_15K_TO_20K_W_EN | Authorize the write access to the Flash MAIN Data array from 15K to 20K word block through the FLASH_IF registers.
6 | RW | DATA_A_10K_TO_15K_W_EN | Authorize the write access to the Flash MAIN Data array from 10K to 15K word block through the FLASH_IF registers.
5 | RW | DATA_A_5K_TO_10K_W_EN | Authorize the write access to the Flash MAIN Data array from 5K to 10K word block through the FLASH_IF registers.
4 | RW | DATA_A_0K_TO_5K_W_EN | Authorize the write access to the Flash MAIN Data array from 0 to 5K word block through the FLASH_IF registers.
3 | RW | CODE_A_66K_TO_88K_W_EN | Authorize the write access to the Flash MAIN Code array from 66K to 88K word block through the FLASH_IF registers.
2 | RW | CODE_A_44K_TO_66K_W_EN | Authorize the write access to the Flash MAIN Code array from 44K to 66K word block through the FLASH_IF registers.
1 | RW | CODE_A_22K_TO_44K_W_EN | Authorize the write access to the Flash MAIN Code array from 22K to 44K word block through the FLASH_IF registers.
0 | RW | CODE_A_0K_TO_22K_W_EN | Authorize the write access to the Flash MAIN Code array from 0 to 22K word block through the FLASH_IF registers.

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
11 | DATA_A_35K_TO_40K_W_EN | DATA_A_35K_TO_40K_W_DISABLE | The part K to K of the Flash MAIN Data array is protected against write access | 0x0*
|  | DATA_A_35K_TO_40K_W_ENABLE | The part K to K of the Flash MAIN Data array can be written | 0x1
10 | DATA_A_30K_TO_35K_W_EN | DATA_A_30K_TO_35K_W_DISABLE | The part K to K of the Flash MAIN Data array is protected against write access | 0x0*
|  | DATA_A_30K_TO_35K_W_ENABLE | The part K to K of the Flash MAIN Data array can be written | 0x1
9 | DATA_A_25K_TO_30K_W_EN | DATA_A_25K_TO_30K_W_DISABLE | The part K to K of the Flash MAIN Data array is protected against write access | 0x0*
|  | DATA_A_25K_TO_30K_W_ENABLE | The part K to K of the Flash MAIN Data array can be written | 0x1
8 | DATA_A_20K_TO_25K_W_EN | DATA_A_20K_TO_25K_W_DISABLE | The part K to K of the Flash MAIN Data array is protected against write access | 0x0*
|  | DATA_A_20K_TO_25K_W_ENABLE | The part K to K of the Flash MAIN Data array can be written | 0x1
7 | DATA_A_15K_TO_20K_W_EN | DATA_A_15K_TO_20K_W_DISABLE | The part K to K of the Flash MAIN Data array is protected against write access | 0x0*
|  | DATA_A_15K_TO_20K_W_ENABLE | The part K to K of the Flash MAIN Data array can be written | 0x1
6 | DATA_A_10K_TO_15K_W_EN | DATA_A_10K_TO_15K_W_DISABLE | The part K to K of the Flash MAIN Data array is protected against write access | 0x0*
|  | DATA_A_10K_TO_15K_W_ENABLE | The part K to K of the Flash MAIN Data array can be written | 0x1
5 | DATA_A_5K_TO_10K_W_EN | DATA_A_5K_TO_10K_W_DISABLE | The part K to K of the Flash MAIN Data array is protected against write access | 0x0*
|  | DATA_A_5K_TO_10K_W_ENABLE | The part K to K of the Flash MAIN Data array can be written | 0x1
4 | DATA_A_0K_TO_5K_W_EN | DATA_A_0K_TO_5K_W_DISABLE | The part K to K of the Flash MAIN Data array is protected against write access | 0x0*
|  | DATA_A_0K_TO_5K_W_ENABLE | The part K to K of the Flash MAIN Data array can be written | 0x1
3 | CODE_A_66K_TO_88K_W_EN | CODE_A_66K_TO_88K_W_DISABLE | The part K to K of the Flash MAIN Code array is protected against write access | 0x0*
|  | CODE_A_66K_TO_88K_W_ENABLE | The part K to K of the Flash MAIN Code array can be written | 0x1
2 | CODE_A_44K_TO_66K_W_EN | CODE_A_44K_TO_66K_W_DISABLE | The part K to K of the Flash MAIN Code array is protected against write access | 0x0*
|  | CODE_A_44K_TO_66K_W_ENABLE | The part K to K of the Flash MAIN Code array can be written | 0x1
1 | CODE_A_22K_TO_44K_W_EN | CODE_A_22K_TO_44K_W_DISABLE | The part K to K of the Flash MAIN Code array is protected against write access | 0x0*
|  | CODE_A_22K_TO_44K_W_ENABLE | The part K to K of the Flash MAIN Code array can be written | 0x1
0 | CODE_A_0K_TO_22K_W_EN | CODE_A_0K_TO_22K_W_DISABLE | The part K to K of the Flash MAIN Code array is protected against write access | 0x0*
|  | CODE_A_0K_TO_22K_W_ENABLE | The part K to K of the Flash MAIN Code array can be written | 0x1