### GPIO_SRC_RF_GPIO89

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
12:8 | RW | GPIO9 | RF front-end GPIO9 input selection
4:0 | RW | GPIO8 | RF front-end GPIO8 input selection

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
12:8 | GPIO9 | RF_GPIO9_SRC_GPIO_0 | Select GPIO[0] as source | 0x0
|  | RF_GPIO9_SRC_GPIO_1 | Select GPIO[1] as source | 0x1
|  | RF_GPIO9_SRC_GPIO_2 | Select GPIO[5] as source | 0x2
|  | RF_GPIO9_SRC_GPIO_3 | Select GPIO[3] as source | 0x3
|  | RF_GPIO9_SRC_GPIO_4 | Select GPIO[4] as source | 0x4
|  | RF_GPIO9_SRC_GPIO_5 | Select GPIO[5] as source | 0x5
|  | RF_GPIO9_SRC_GPIO_6 | Select GPIO[6] as source | 0x6
|  | RF_GPIO9_SRC_GPIO_7 | Select GPIO[7] as source | 0x7
|  | RF_GPIO9_SRC_GPIO_8 | Select GPIO[8] as source | 0x8
|  | RF_GPIO9_SRC_GPIO_9 | Select GPIO[9] as source | 0x9
|  | RF_GPIO9_SRC_GPIO_10 | Select GPIO[10] as source | 0xA
|  | RF_GPIO9_SRC_GPIO_11 | Select GPIO[11] as source | 0xB
|  | RF_GPIO9_SRC_GPIO_12 | Select GPIO[12] as source | 0xC
|  | RF_GPIO9_SRC_GPIO_13 | Select GPIO[13] as source | 0xD
|  | RF_GPIO9_SRC_GPIO_14 | Select GPIO[14] as source | 0xE
|  | RF_GPIO9_SRC_GPIO_15 | Select GPIO[15] as source | 0xF
|  | RF_GPIO9_SRC_CONST_LOW | Select constant low as source | 0x10*
|  | RF_GPIO9_SRC_CONST_HIGH | Select constant high as source | 0x11
4:0 | GPIO8 | RF_GPIO8_SRC_GPIO_0 | Select GPIO[0] as source | 0x0
|  | RF_GPIO8_SRC_GPIO_1 | Select GPIO[1] as source | 0x1
|  | RF_GPIO8_SRC_GPIO_2 | Select GPIO[5] as source | 0x2
|  | RF_GPIO8_SRC_GPIO_3 | Select GPIO[3] as source | 0x3
|  | RF_GPIO8_SRC_GPIO_4 | Select GPIO[4] as source | 0x4
|  | RF_GPIO8_SRC_GPIO_5 | Select GPIO[5] as source | 0x5
|  | RF_GPIO8_SRC_GPIO_6 | Select GPIO[6] as source | 0x6
|  | RF_GPIO8_SRC_GPIO_7 | Select GPIO[7] as source | 0x7
|  | RF_GPIO8_SRC_GPIO_8 | Select GPIO[8] as source | 0x8
|  | RF_GPIO8_SRC_GPIO_9 | Select GPIO[9] as source | 0x9
|  | RF_GPIO8_SRC_GPIO_10 | Select GPIO[10] as source | 0xA
|  | RF_GPIO8_SRC_GPIO_11 | Select GPIO[11] as source | 0xB
|  | RF_GPIO8_SRC_GPIO_12 | Select GPIO[12] as source | 0xC
|  | RF_GPIO8_SRC_GPIO_13 | Select GPIO[13] as source | 0xD
|  | RF_GPIO8_SRC_GPIO_14 | Select GPIO[14] as source | 0xE
|  | RF_GPIO8_SRC_GPIO_15 | Select GPIO[15] as source | 0xF
|  | RF_GPIO8_SRC_CONST_LOW | Select constant low as source | 0x10*
|  | RF_GPIO8_SRC_CONST_HIGH | Select constant high as source | 0x11