### BB_RADIOPWRUPDN1

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
31:24 | RW | SYNC_POSITION1 | Access address detection pulse/level position for uncoded PHY at 2Mbps
23:16 | RW | RXPWRUP1 | Radio Rx power up (in us) for uncoded PHY at 2Mbps
14:8 | RW | TXPWRDN1 | Radio Tx power down (in us) for uncoded PHY at 2Mbps
7:0 | RW | TXPWRUP1 | Radio Tx power up (in us) for uncoded PHY at 2Mbps

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
31:24 | SYNC_POSITION1 | SYNC_POSITION1_0 |  | 0x0*
23:16 | RXPWRUP1 | RXPWRUP1_0 |  | 0x0*
14:8 | TXPWRDN1 | TXPWRDN1_0 |  | 0x0*
7:0 | TXPWRUP1 | TXPWRUP1_0 |  | 0x0*