### SYSCTRL_CC_STATUS

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
25 | R | CC_SEC_DEBUG_RESET | Always On block secure debug reset status
24 | R | CC_HOST_DFA_ENABLE_LOCK | Always On block host AES DFA lock status
23 | R | CC_HOST_FORCE_DFA_ENABLE | Always On block host AES DFA status
22 | R | CC_RESET_UPON_DEBUG_DISABLE | Always On block HUK reset mechanism configuration status
21 | R | CC_HOST_ICV_RMA_LOCK | Always On block host icv rma bit in NVM lock status
20 | R | CC_HOST_KCE_LOCK | Always On block host OEM code encryption key lock status
19 | R | CC_HOST_KCP_LOCK | Always On block host OEM provisioning key lock status
18 | R | CC_HOST_KCEICV_LOCK | Always On block host ICV code encryption key lock status
17 | R | CC_HOST_KPICV_LOCK | Always On block host ICV provisioning key lock status
16 | R | CC_HOST_FATAL_ERR | Always On block host fatal error flag
15 | R | CC_APB_ONLY_PRIV_ACCESS_LOCK | Always On block APB filtering privileged access configuration lock
14 | R | CC_APB_ONLY_PRIV_ACCESS | Always On block APB filtering privileged access configuration
13 | R | CC_APB_ONLY_SEC_ACCESS_LOCK | Always On block APB filtering secure access configuration lock
12 | R | CC_APB_ONLY_SEC_ACCESS | Always On block APB filtering secure access configuration
11:4 | R | CC_GPPC | Always On block GPPC register
3 | R | CC_LCS_VALID | Always On block life cycle state valid
2:0 | R | CC_LCS | Always On block life cycle state

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
25 | CC_SEC_DEBUG_RESET | CC_SEC_DBG_RST_IDLE | The CC312 does not have the secure debug reset activated | 0x0*
|  | CC_SEV_DBG_RST_ACTIVATED | The CC312 has secure debug reset fired, can't fire again | 0x1
24 | CC_HOST_DFA_ENABLE_LOCK | CC_DFA_CFG_UNLOCKED | The CC312 AES DFA configuration register is unlocked | 0x0*
|  | CC_DFA_CFG_LOCKED | The CC312 AES DFA configuration register is locked | 0x1
23 | CC_HOST_FORCE_DFA_ENABLE | CC_DFA_DIS | The CC312 AES DFA counter measures are not enabled | 0x0*
|  | CC_DFA_EN | The CC312 AES DFA counter measures are enabled | 0x1
22 | CC_RESET_UPON_DEBUG_DISABLE | CC_RESET_UPON_DEBUG_EN | The CC312 HUK reset mechanism is enabled | 0x0*
|  | CC_RESET_UPON_DEBUG_DIS | The CC312 HUK reset mechanism is disabled | 0x1
21 | CC_HOST_ICV_RMA_LOCK | CC_ICV_RMA_UNLOCKED | The CC312 icv_rma flag in NVM can be written | 0x0*
|  | CC_ICV_RMA_LOCKED | The CC312 icv_rma flag in NVM is locked, can't be written | 0x1
20 | CC_HOST_KCE_LOCK | CC_KCE_UNLOCKED | The CC312 KCE is unlocked | 0x0*
|  | CC_KCE_LOCKED | The CC312 KCE is masked, locked by the SW | 0x1
19 | CC_HOST_KCP_LOCK | CC_KCP_UNLOCKED | The CC312 KCP is unlocked | 0x0*
|  | CC_KCP_LOCKED | The CC312 KCP is masked, locked by the SW | 0x1
18 | CC_HOST_KCEICV_LOCK | CC_KCEICV_UNLOCKED | The CC312 KCEICV is unlocked | 0x0*
|  | CC_KCEICV_LOCKED | The CC312 KCEICV is masked, locked by the SW | 0x1
17 | CC_HOST_KPICV_LOCK | CC_KPICV_UNLOCKED | The CC312 KPICV is unlocked | 0x0*
|  | CC_KPICV_LOCKED | The CC312 KPICV is masked, locked by the SW | 0x1
16 | CC_HOST_FATAL_ERR | CC_HOST_NO_FATAL_ERROR | The CC312 does not have any fatal error | 0x0*
|  | CC_HOST_FATAL_ERROR | The CC312 reports a fatal error | 0x1
15 | CC_APB_ONLY_PRIV_ACCESS_LOCK | CC_APB_PRIV_CFG_UNLOCK | The CC312 privileged access configuration field unlocked | 0x0*
|  | CC_APB_PRIV_CFG_LOCK | The CC312 privileged access configuration field locked | 0x1
14 | CC_APB_ONLY_PRIV_ACCESS | CC_APB_NORMAL_ACCESS | The CC312 serve both privileged and normal access | 0x0*
|  | CC_APB_PRIV_ACCESS | The CC312 serve only privileged access | 0x1
13 | CC_APB_ONLY_SEC_ACCESS_LOCK | CC_APB_SEC_CFG_UNLOCK | The CC312 secure access configuration field is unlocked | 0x0*
|  | CC_APB_SEC_CFG_LOCKED | The CC312 secure access configuration field is locked | 0x1
12 | CC_APB_ONLY_SEC_ACCESS | CC_APB_NON_SEC_ACCESS | The CC312 allow both secure and non-secure access | 0x0*
|  | CC_APB_ONLY_SEC_ACCESS | The CC312 allow only secure access | 0x1
3 | CC_LCS_VALID | CC_LCS_IS_INVALID | The CC312 does not have LCS defined after reset | 0x0*
|  | CC_LCS_IS_VALID | The CC312 has LCS defined after reset | 0x1
2:0 | CC_LCS | CC_LCS_CM | The CC312 is in CM lifecycle state | 0x0*
|  | CC_LCS_DM | The CC312 is in DM lifecycle state | 0x1
|  | CC_LCS_SECURE | The CC312 is in Secure lifecycle state | 0x5
|  | CC_LCS_RMA | The CC312 is in RMA lifecycle state | 0x7