### GPIO_JTAG_SW_PAD_CFG

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
9 | RW | SWCLK_LPF | SWCLK Low-Pass-Filter enable / disable
8 | RW | SWDIO_LPF | SWDIO Low-Pass-Filter enable / disable
7 | RW | CM33_JTAG_DATA_EN | CM33 JTAG data (TDI and TDO) on GPIO[3:2]
6 | RW | CM33_JTAG_TRST_EN | CM33 JTAG TRST on GPIO4
5:4 | RW | SWCLK_PULL | SWCLK pull-up enable / disable
3:2 | RW | SWDIO_DRIVE | SWDIO drive strength
1:0 | RW | SWDIO_PULL | SWDIO pull-up enable / disable

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
9 | SWCLK_LPF | SWCLK_LPF_DISABLED | Disable low pass filter | 0x0*
|  | SWCLK_LPF_ENABLED | Enable low pass filter | 0x1
8 | SWDIO_LPF | SWDIO_LPF_DISABLED | Disable low pass filter | 0x0*
|  | SWDIO_LPF_ENABLED | Enable low pass filter | 0x1
7 | CM33_JTAG_DATA_EN | CM33_JTAG_DATA_DISABLED | CM33 JTAG data (TDI and TDO) not available on GPIO[3:2] | 0x0
|  | CM33_JTAG_DATA_ENABLED | CM33 JTAG data (TDI and TDO) connected through GPIO[3:2] | 0x1*
6 | CM33_JTAG_TRST_EN | CM33_JTAG_TRST_DISABLED | CM33 JTAG TRST not available on GPIO4 | 0x0
|  | CM33_JTAG_TRST_ENABLED | CM33 JTAG TRST connected through GPIO4 | 0x1*
5:4 | SWCLK_PULL | SWCLK_NO_PULL | No pull selected | 0x0
|  | SWCLK_WEAK_PULL_UP | Weak pull-up selected | 0x1*
|  | SWCLK_WEAK_PULL_DOWN | Weak pull-down selected | 0x2
|  | SWCLK_STRONG_PULL_UP | Strong pull-up selected | 0x3
3:2 | SWDIO_DRIVE | SWDIO_2X_DRIVE | 2x drive strength | 0x0
|  | SWDIO_3X_DRIVE | 3x drive strength | 0x1
|  | SWDIO_5X_DRIVE | 5x drive strength | 0x2
|  | SWDIO_6X_DRIVE | 6x drive strength | 0x3*
1:0 | SWDIO_PULL | SWDIO_NO_PULL | No pull selected | 0x0
|  | SWDIO_WEAK_PULL_UP | Weak pull-up selected | 0x1*
|  | SWDIO_WEAK_PULL_DOWN | Weak pull-down selected | 0x2
|  | SWDIO_STRONG_PULL_UP | Strong pull-up selected | 0x3