### RF_PADS_89

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
31:24 | RW | TX_MAC_TIMER_TX_MAC_TIMER | Time to wait after the Tx mode
23:16 | RW | RX_MAC_TIMER_RX_MAC_TIMER | Time to wait after the Rx mode
12:8 | RW | PAD_CONF_3_PAD_9_CONF | Configuration of GPIO pad 9
4:0 | RW | PAD_CONF_3_PAD_8_CONF | Configuration of GPIO pad 8

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
31:24 | TX_MAC_TIMER_TX_MAC_TIMER | TX_MAC_TIMER_TX_MAC_TIMER_DEFAULT |  | 0x82*
23:16 | RX_MAC_TIMER_RX_MAC_TIMER | RX_MAC_TIMER_RX_MAC_TIMER_DEFAULT |  | 0x23*
12:8 | PAD_CONF_3_PAD_9_CONF | PAD_CONF_3_PAD_9_OFF |  | 0x0*
|  | PAD_CONF_3_PAD_9_TEST_MODE |  | 0xF
4:0 | PAD_CONF_3_PAD_8_CONF | PAD_CONF_3_PAD_8_OFF |  | 0x0*
|  | PAD_CONF_3_PAD_8_TEST_MODE |  | 0xF