### FLASH_PATCH_ADDR

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
31 | RW | PATCH_NOT_VALID | Indicates if the patch address is valid
20:8 | RW | PATCH_ADDR |

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
31 | PATCH_NOT_VALID | PATCH_VALID | This bit must be cleared in order for the patching to be taken into consideration. | 0x0
|  | PATCH_NOT_VALID |  | 0x1*