### RF_CTE_CTRL

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
25:16 | RW | CTE_CTRL_DELAY_RX_DF_DELAY_SWITCH_RX | Delay (in 62.5ns) from the antenna up to the deserializer in direction finding (banked)
9:0 | RW | CTE_CTRL_DELAY_RX_DF_DELAY_SAMPLE_RX | Delay (in 62.5ns) from the matched filter up to the deserializer in direction finding (banked)

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
25:16 | CTE_CTRL_DELAY_RX_DF_DELAY_SWITCH_RX | CTE_CTRL_DELAY_RX_DF_DELAY_SWITCH_RX_DEFAULT |  | 0x0*
9:0 | CTE_CTRL_DELAY_RX_DF_DELAY_SAMPLE_RX | CTE_CTRL_DELAY_RX_DF_DELAY_SAMPLE_RX_DEFAULT |  | 0x0*