### ACS_PWM_AO_CTRL

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
8 | R | ENABLE_STATUS | Status of the PWM enable
2 | W | RESET | Reset the PWM
1 | W | DISABLE | Disable the PWM
0 | W | ENABLE | Enable the PWM

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
8 | ENABLE_STATUS | PWM_IS_DISABLED | PWM is disabled | 0x0*
|  | PWM_IS_ENABLED | PWM is enabled | 0x1
2 | RESET | PWM_RESET | Reset PWM | 0x1
1 | DISABLE | PWM_DISABLE | Disable PWM | 0x1
0 | ENABLE | PWM_ENABLE | Enable PWM | 0x1