### RF_RSSI_CTRL

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
31:30 | RW | RSSI_CTRL_AGC_DECAY_TAU | Time constant of the decay speed
29 | RW | RSSI_CTRL_AGC_USE_LNA | AGC algorithm uses LNA bias
28 | RW | RSSI_CTRL_AGC_MODE | AGC algorithm selection
27:26 | RW | RSSI_CTRL_AGC_WAIT | Set the wait time of the AGC after switching between state
25 | RW | RSSI_CTRL_PAYLOAD_BLOCKS_AGC | AGC payload blocking
24 | RW | RSSI_CTRL_BYPASS_AGC | AGC algorithm bypass
20:16 | RW | PA_PWR_OFFSET_PA_PWR_OFFSET | Signed value that sets the PA power (banked)
12:8 | RW | FILTER_BIAS_IQ_FI_BW | Bias for the bandwidth of the channel filter (banked)
4:0 | RW | FILTER_BIAS_IQ_FI_FC | Bias for the central frequency of the channel filter (banked)

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
31:30 | RSSI_CTRL_AGC_DECAY_TAU | RSSI_CTRL_AGC_DECAY_TAU_DEFAULT | High values corresponds to a slow decay | 0x3*
29 | RSSI_CTRL_AGC_USE_LNA | RSSI_CTRL_AGC_USE_LNA_DISABLE | AGC algorithm doesn't use the LNA bias | 0x0
|  | RSSI_CTRL_AGC_USE_LNA_ENABLE | AGC algorithm uses the LNA bias | 0x1*
28 | RSSI_CTRL_AGC_MODE | RSSI_CTRL_AGC_MODE_DISABLE | Old AGC algorithm | 0x0
|  | RSSI_CTRL_AGC_MODE_ENABLE | New AGC algorithm | 0x1*
27:26 | RSSI_CTRL_AGC_WAIT | RSSI_CTRL_AGC_WAIT_0 | Don't wait | 0x0
|  | RSSI_CTRL_AGC_WAIT_1 | Wait 1x RSSI filtering period | 0x1
|  | RSSI_CTRL_AGC_WAIT_2 | Wait 2x RSSI filtering period | 0x2
|  | RSSI_CTRL_AGC_WAIT_3 | Wait 3x RSSI filtering period | 0x3*
25 | RSSI_CTRL_PAYLOAD_BLOCKS_AGC | RSSI_CTRL_PAYLOAD_BLOCKS_AGC_DISABLE | AGC is not blocked during the payload | 0x0
|  | RSSI_CTRL_PAYLOAD_BLOCKS_AGC_ENABLE | AGC is blocked during the payload | 0x1*
24 | RSSI_CTRL_BYPASS_AGC | RSSI_CTRL_BYPASS_AGC_DISABLE | AGC algorithm is not bypassed | 0x0*
|  | RSSI_CTRL_BYPASS_AGC_ENABLE | AGC algorithm is bypassed | 0x1
20:16 | PA_PWR_OFFSET_PA_PWR_OFFSET | PA_PWR_OFFSET_PA_PWR_OFFSET_DEFAULT |  | 0x0*
12:8 | FILTER_BIAS_IQ_FI_BW | FILTER_BIAS_IQ_FI_BW_DEFAULT |  | 0x14*
4:0 | FILTER_BIAS_IQ_FI_FC | FILTER_BIAS_IQ_FI_FC_DEFAULT |  | 0xB*