### BBIF_STATUS

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
16:12 | R | LINK_FORMAT | BLE link format
8:4 | R | LINK_LABEL | BLE link label
2 | R | CLK_STATUS | Clock status defining the current active clock in use
1 | R | OSC_EN | Oscillator front-end enabling
0 | R | RADIO_EN | RF front-end enabling

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
2 | CLK_STATUS | MASTER_CLK | Baseband controller running on master1/2_clk | 0x0*
|  | LOW_POWER_CLK | Baseband controller running on low_power_clk | 0x1
1 | OSC_EN | OSC_DISABLED | Oscillator can be safely disabled | 0x0
|  | OSC_ENABLED | Oscillator must be enabled | 0x1*
0 | RADIO_EN | RF_DISABLED | RF front-end can be safely disabled | 0x0
|  | RF_ENABLED | RF front-end must be enabled | 0x1*