### RF_REG10

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
25:21 | RW | CONV_CODES_PUNCT_CC_PUNCT_1 | Puncture of the second convolutional code (banked)
20:16 | RW | CONV_CODES_PUNCT_CC_PUNCT_0 | Puncture of the first convolutional code (banked)
11 | RW | FRAC_CONF_TX_FRAC_GAIN | Additional gain for fractional data-rates in Tx mode (banked)
10 | RW | FRAC_CONF_RX_FRAC_GAIN | Additional gain for fractional data-rates in Rx mode (banked)
9 | RW | FRAC_CONF_TX_EN_FRAC | Fractional data-rates in Tx mode (banked)
8 | RW | FRAC_CONF_RX_EN_FRAC | Fractional data-rates in Rx mode (banked)
7:4 | RW | CONV_CODES_POLY_CC_POLY_1 | Second convolutional code (banked)
3:0 | RW | CONV_CODES_POLY_CC_POLY_0 | First convolutional code (banked)

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
25:21 | CONV_CODES_PUNCT_CC_PUNCT_1 | CONV_CODES_PUNCT_CC_PUNCT_1_DEFAULT |  | 0x1*
20:16 | CONV_CODES_PUNCT_CC_PUNCT_0 | CONV_CODES_PUNCT_CC_PUNCT_0_DEFAULT |  | 0x1*
11 | FRAC_CONF_TX_FRAC_GAIN | FRAC_CONF_TX_FRAC_GAIN_DISABLE | Disable the additional gain for fractional data-rates in Tx mode | 0x0*
|  | FRAC_CONF_TX_FRAC_GAIN_ENABLE | Enable the additional gain for fractional data-rates in Tx mode | 0x1
10 | FRAC_CONF_RX_FRAC_GAIN | FRAC_CONF_RX_FRAC_GAIN_DISABLE | Disable the additional gain for fractional data-rates in Rx mode | 0x0*
|  | FRAC_CONF_RX_FRAC_GAIN_ENABLE | Enable the additional gain for fractional data-rates in Rx mode | 0x1
9 | FRAC_CONF_TX_EN_FRAC | FRAC_CONF_TX_EN_FRAC_DISABLE | Disable the fractional data-rates in Tx mode | 0x0*
|  | FRAC_CONF_TX_EN_FRAC_ENABLE | Enable the fractional data-rates in Tx mode | 0x1
8 | FRAC_CONF_RX_EN_FRAC | FRAC_CONF_RX_EN_FRAC_DISABLE | Disable the fractional data-rates in Rx mode | 0x0*
|  | FRAC_CONF_RX_EN_FRAC_ENABLE | Enable the fractional data-rates in Rx mode | 0x1
7:4 | CONV_CODES_POLY_CC_POLY_1 | CONV_CODES_POLY_CC_POLY_1_DEFAULT |  | 0xD*
3:0 | CONV_CODES_POLY_CC_POLY_0 | CONV_CODES_POLY_CC_POLY_0_DEFAULT |  | 0xF*