### I2C_CTRL

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
9 | R | LAST_DATA_STATUS | I2C last data status
8 | R | ENABLE_STATUS | I2C enable status
6 | W | LAST_DATA | Indicate that the current data is the last byte of a data transfer
5 | W | STOP | Issue a stop condition on the I2C interface bus
4 | W | NACK | Issue a not acknowledge on the I2C interface bus
3 | W | ACK | Issue an acknowledge on the I2C interface bus
2 | W | RESET | Reset the I2C interface
1 | W | DISABLE | Disable the I2C interface
0 | W | ENABLE | Enable the I2C interface

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
9 | LAST_DATA_STATUS | I2C_LAST_DATA_DISABLED | I2C last data is disabled | 0x0*
|  | I2C_LAST_DATA_ENABLED | I2C last data is enabled | 0x1
8 | ENABLE_STATUS | I2C_STATUS_DISABLED | I2C interface is disabled | 0x0*
|  | I2C_STATUS_ENABLED | I2C interface is enabled | 0x1
6 | LAST_DATA | I2C_LAST_DATA | Indicate that the current data is the last byte of a data transfer | 0x1
5 | STOP | I2C_STOP | Issue a stop condition on the I2C interface bus | 0x1
4 | NACK | I2C_NACK | Issue a not acknowledge on the I2C interface bus | 0x1
3 | ACK | I2C_ACK | Issue an acknowledge on the I2C interface bus | 0x1
|  | I2C_RESUME | Resume I2C interface after receiving address ACK/NACK in master read auto ack disable mode | 0x1
2 | RESET | I2C_RESET | Reset the I2C interface | 0x1
1 | DISABLE | I2C_DISABLE | Disable the I2C interface | 0x1
0 | ENABLE | I2C_ENABLE | Enable the I2C interface | 0x1