### RF_AGC_ADVANCED

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
26:16 | RW | AGC_SWITCHES_AGC_SHORTS_LUT | Array of values that indicates if the highpass shorts must be set for the AGC state passage from n -> n+1
8 | RW | DEBUG_FAKE_IQ_SAMPLES | Generate fake IQ samples
7:4 | RW | AGC_ADVANCED_AGC_TAU_SHORTS | Time constant that indicates the time that shorts must be on
3 | RW | AGC_ADVANCED_AGC_EN_SHORT_PHADC | Enable the short on the phase ADC highpass filter
2 | RW | AGC_ADVANCED_AGC_EN_SHORT_IFA | Enable the short on the IFA highpass filter
1 | RW | AGC_ADVANCED_AGC_USE_SHORTS | Enable the usage of the shorts located in the BB path
0 | RW | AGC_ADVANCED_AGC_FULL_SPEED | Enable the maximum speed in AGC

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
26:16 | AGC_SWITCHES_AGC_SHORTS_LUT | AGC_SWITCHES_AGC_SHORTS_LUT_DEFAULT |  | 0x0*
8 | DEBUG_FAKE_IQ_SAMPLES | DEBUG_FAKE_IQ_SAMPLES_DISABLE | Disable fake IQ samples | 0x0*
|  | DEBUG_FAKE_IQ_SAMPLES_ENABLE | Enable fake IQ samples | 0x1
7:4 | AGC_ADVANCED_AGC_TAU_SHORTS | AGC_ADVANCED_AGC_TAU_SHORTS_DEFAULT |  | 0x0*
3 | AGC_ADVANCED_AGC_EN_SHORT_PHADC | AGC_ADVANCED_AGC_EN_SHORT_PHADC_DISABLE | Disable the short on the phase ADC highpass filter | 0x0*
|  | AGC_ADVANCED_AGC_EN_SHORT_PHADC_ENABLE | Enable the short on the phase ADC highpass filter | 0x1
2 | AGC_ADVANCED_AGC_EN_SHORT_IFA | AGC_ADVANCED_AGC_EN_SHORT_IFA_DISABLE | Disable the short on the IFA highpass filter | 0x0*
|  | AGC_ADVANCED_AGC_EN_SHORT_IFA_ENABLE | Enable the short on the IFA highpass filter | 0x1
1 | AGC_ADVANCED_AGC_USE_SHORTS | AGC_ADVANCED_AGC_USE_SHORTS_DISABLE | Disable using shorts located in BB path | 0x0*
|  | AGC_ADVANCED_AGC_USE_SHORTS_ENABLE | Enable using shorts located in BB path | 0x1
0 | AGC_ADVANCED_AGC_FULL_SPEED | AGC_ADVANCED_AGC_FULL_SPEED_DISABLE | Disable maximum AGC speed | 0x0*
|  | AGC_ADVANCED_AGC_FULL_SPEED_ENABLE | Enable maximum speed AGC | 0x1