### TOF_CTRL

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
8 | R | ENABLE_STATUS | Status of the time of flight timer
4 | W | STOP | Stop the time of flight timer
3 | W | START | Start the time of flight timer
2 | W | RESET | Synchronously reset the time of flight timer
1 | W | DISABLE | Disable the time of flight timer
0 | W | ENABLE | Enable the time of flight timer

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
8 | ENABLE_STATUS | TOF_STATUS_DISABLED | Time of flight timer is disabled | 0x0*
|  | TOF_STATUS_ENABLED | Time of flight timer is enabled | 0x1
4 | STOP | TOF_STOP | Stop the time of flight timer | 0x1
3 | START | TOF_START | Start the time of flight timer | 0x1
2 | RESET | TOF_RESET | Synchronously reset the time of flight timer | 0x1
1 | DISABLE | TOF_DISABLE | Disable the time of flight timer | 0x1
0 | ENABLE | TOF_ENABLE | Enable the time of flight timer | 0x1