### RF_DATA_STREAMING

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
9 | RW | DATA_STREAMING_DMA_PHASE_TYPE | Use the phase after the rescaler instead of the raw phase from phase ADC (banked)
8 | RW | DATA_STREAMING_DMA_EN_BUS | Enable the DMA bus on the IP interface (banked)
6 | RW | DATA_STREAMING_PERIODIC_SAMPLE_AFTER_CTE | Restart sampling after the CTE period (banked)
5 | RW | DATA_STREAMING_PERIODIC_SAMPLE_AT_SYNC | Start sampling at the sync detection signal from the delay line (banked)
4 | RW | DATA_STREAMING_PERIODIC_SAMPLE_OSR_CLK | Oversample (8x) the reference clock of the periodic sample (banked)
3:1 | RW | DATA_STREAMING_PERIODIC_SAMPLE_OSR | Division factor (-1) of for the sampling period of the periodic IQ sampling (banked)
0 | RW | DATA_STREAMING_PERIODIC_SAMPLE_EN_IQ | Sample periodically I and Q channels after the matched filter and put into the IQ FIFO (banked)

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
9 | DATA_STREAMING_DMA_PHASE_TYPE | DATA_STREAMING_DMA_PHASE_TYPE_PHADC | Use the raw phase from the phase ADC | 0x0*
|  | DATA_STREAMING_DMA_PHASE_TYPE_RESCALER | Use the phase after the rescaler | 0x1
8 | DATA_STREAMING_DMA_EN_BUS | DATA_STREAMING_DMA_BUS_DISABLE | Enable the DMA bus on the IP interface | 0x0*
|  | DATA_STREAMING_DMA_BUS_ENABLE | Disable the DMA bus on the IP interface | 0x1
6 | DATA_STREAMING_PERIODIC_SAMPLE_AFTER_CTE | DATA_STREAMING_PERIODIC_SAMPLE_AFTER_CTE_DISABLE | Stop sampling after the CTE event | 0x0
|  | DATA_STREAMING_PERIODIC_SAMPLE_AFTER_CTE_ENABLE | Restart sampling after the CTE event | 0x1*
5 | DATA_STREAMING_PERIODIC_SAMPLE_AT_SYNC | DATA_STREAMING_PERIODIC_SAMPLE_AT_SYNC_DISABLE | Sample at the Rx activation | 0x0*
|  | DATA_STREAMING_PERIODIC_SAMPLE_AT_SYNC_ENABLE | Sample at the sync detection signal from the delay line | 0x1
4 | DATA_STREAMING_PERIODIC_SAMPLE_OSR_CLK | DATA_STREAMING_PERIODIC_SAMPLE_OSR_CLK_DISABLE | Use the system clock | 0x0*
|  | DATA_STREAMING_PERIODIC_SAMPLE_OSR_CLK_ENABLE | Oversample the reference clock of the periodic sample | 0x1
3:1 | DATA_STREAMING_PERIODIC_SAMPLE_OSR | DATA_STREAMING_PERIODIC_SAMPLE_OSR_DEFAULT |  | 0x3*
0 | DATA_STREAMING_PERIODIC_SAMPLE_EN_IQ | DATA_STREAMING_PERIODIC_SAMPLE_IQ_DISABLE | Disable periodical sampling | 0x0*
|  | DATA_STREAMING_PERIODIC_SAMPLE_IQ_ENABLE | Enable periodical sampling | 0x1