### BBIF_COEX_INT_STATUS

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
11 | R | EVENT_IN_PROCESS | EVENT_IN_PROCESS interrupt status flag
10 | R | BLE_IN_PROCESS | BLE_IN_PROCESS interrupt status flag
9 | R | BLE_TX | BLE_TX interrupt status flag
8 | R | BLE_RX | BLE_RX interrupt status flag
3 | W | EVENT_IN_PROCESS_CLEAR | Clear EVENT_IN_PROCESS status flag
2 | W | BLE_IN_PROCESS_CLEAR | Clear BLE_IN_PROCESS status flag
1 | W | BLE_TX_CLEAR | Clear BLE_TX status flag
0 | W | BLE_RX_CLEAR | Clear BLE_RX status flag

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
11 | EVENT_IN_PROCESS | EVENT_IN_PROCESS_NO_INT | No EVENT_IN_PROCESS_EVENT interrupt has been generated | 0x0*
|  | EVENT_IN_PROCESS_INT | A EVENT_IN_PROCESS_EVENT interrupt has been generated | 0x1
10 | BLE_IN_PROCESS | BLE_IN_PROCESS_NO_INT | No BLE_IN_PROCESS_EVENT interrupt has been generated | 0x0*
|  | BLE_IN_PROCESS_INT | A BLE_IN_PROCESS_EVENT interrupt has been generated | 0x1
9 | BLE_TX | BLE_TX_NO_INT | No BLE_TX_EVENT interrupt has been generated | 0x0*
|  | BLE_TX_INT | A BLE_TX_EVENT interrupt has been generated | 0x1
8 | BLE_RX | BLE_RX_NO_INT | No BLE_RX_EVENT interrupt has been generated | 0x0*
|  | BLE_RX_INT | A BLE_RX_EVENT interrupt has been generated | 0x1
3 | EVENT_IN_PROCESS_CLEAR | EVENT_IN_PROCESS_CLEAR |  | 0x1
2 | BLE_IN_PROCESS_CLEAR | BLE_IN_PROCESS_CLEAR |  | 0x1
1 | BLE_TX_CLEAR | BLE_TX_CLEAR |  | 0x1
0 | BLE_RX_CLEAR | BLE_RX_CLEAR |  | 0x1