### LIN_DLBR

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
2:0 | RW | DLBR | Number of data bytes to receive.

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
2:0 | DLBR | RX_1_BYTE | 1 byte will be received | 0x0*
|  | RX_2_BYTES | 2 bytes will be received | 0x1
|  | RX_3_BYTES | 3 bytes will be received | 0x2
|  | RX_4_BYTES | 4 bytes will be received | 0x3
|  | RX_5_BYTES | 5 bytes will be received | 0x4
|  | RX_6_BYTES | 6 bytes will be received | 0x5
|  | RX_7_BYTES | 7 bytes will be received | 0x6
|  | RX_8_BYTES | 8 bytes will be received | 0x7