### BB_SPIPTRCNTL2

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
29:16 | RW | RXLENGTHPTR | Pointer to the received length write sequence address section
13:0 | RW | RSSIPTR | Pointer to the RSSI read sequence address section

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
29:16 | RXLENGTHPTR | RXLENGTHPTR_0 |  | 0x0*
13:0 | RSSIPTR | RSSIPTR_0 |  | 0x0*