### SYSCTRL_CC_DCU_EN1

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
31:16 | R | CC_DCU_EN_OEM_GP | Always On OEM governed dcu_en1 general purpose bits
15:13 | R | CC_DCU_EN_OEM_SEC_RST | Always On OEM governed secure reset enable. If any of these bits are set and the part is in SE state, the cc312_top is reset
12:10 | R | CC_DCU_EN_OEM_SPINDEN | Always On OEM governed CM33 secure non-intrusive debug enable control. Majority of the bits must be set to enable the feature
9:7 | R | CC_DCU_EN_OEM_SPIDEN | Always On OEM governed CM33 secure intrusive debug enable control. Majority of the bits must be set to enable the feature
6:4 | R | CC_DCU_EN_OEM_NIDEN | Always On OEM governed CM33 non-intrusive debug enable control. Majority of the bits must be set to enable the feature
3:1 | R | CC_DCU_EN_OEM_DBGEN | Always On OEM governed CM33 debug enable control. Majority of the bits must be set to enable the feature
0 | R | CC_DCU_EN_OEM_RESERVED | Always On OEM allocated reserved bit (unused)