### BB_ACTFIFOSTAT

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
31:28 | R | SKIP_ET_IDX | Exchange table entry index of the reported skipped event (valid when SKIPACTINTSTAT is set)
27:24 | R | CURRENT_ET_IDX | Exchange table entry index of the reported current event (valid for any set reported interrupt except SKIPACTINTSTAT)
15 | R | ACTFLAG | Forced to 1 in BLE
6 | R | ISORXINTSTAT | Isochronous channel Rx interrupt status
5 | R | ISOTXINTSTAT | Isochronous channel Tx interrupt status
4 | R | RXINTSTAT | Rx interrupt status
3 | R | TXINTSTAT | Tx interrupt status
2 | R | SKIPACTINTSTAT | Skipped event interrupt status
1 | R | ENDACTINTSTAT | End of event interrupt status
0 | R | STARTACTINTSTAT | Start of event interrupt status

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
31:28 | SKIP_ET_IDX | SKIP_ET_IDX_0 |  | 0x0*
27:24 | CURRENT_ET_IDX | CURRENT_ET_IDX_0 |  | 0x0*
15 | ACTFLAG | ACTFLAG_0 |  | 0x0*
|  | ACTFLAG_1 |  | 0x1
6 | ISORXINTSTAT | ISORXINTSTAT_0 | No isochronous channel Rx interrupt | 0x0*
|  | ISORXINTSTAT_1 | An isochronous channel Rx interrupt is pending | 0x1
5 | ISOTXINTSTAT | ISOTXINTSTAT_0 | No isochronous channel Tx interrupt. | 0x0*
|  | ISOTXINTSTAT_1 | An isochronous channel Tx interrupt is pending | 0x1
4 | RXINTSTAT | RXINTSTAT_0 | No Rx interrupt. | 0x0*
|  | RXINTSTAT_1 | An Rx interrupt is pending | 0x1
3 | TXINTSTAT | TXINTSTAT_0 | No Tx interrupt. | 0x0*
|  | TXINTSTAT_1 | A Tx interrupt is pending | 0x1
2 | SKIPACTINTSTAT | SKIPACTINTSTAT_0 | No skipped event interrupt | 0x0*
|  | SKIPACTINTSTAT_1 | A skipped event interrupt is pending | 0x1
1 | ENDACTINTSTAT | ENDACTINTSTAT_0 | No end of event interrupt | 0x0*
|  | ENDACTINTSTAT_1 | An end of event interrupt is pending | 0x1
0 | STARTACTINTSTAT | STARTACTINTSTAT_0 | No start of event interrupt | 0x0*
|  | STARTACTINTSTAT_1 | A start of event interrupt is pending | 0x1