# Transition from EH_STATE to ROT_STATE

## Revoking EH_STATE

Revoking access to the EH_STATE is straightforward and follows a similar process to that outlined for other EH_STATE operations. There are no options specific to this command (though the options common to all commands are still applicable). The revocation action cannot be reversed once it has completed.

Example Usage

c:\Development\RSLSec>rslsec eh revoke --write

This command connects to an RSL15 device and update the EH_STATE configuration to render it invalid. On completion, the device is reset and has transitioned to ROT_STATE in LCS_CM.

NOTE: This action is not reversible.

High level help from 'RSLSec eh revoke --help'

c:\Development\RSLSec>rslsec eh revoke --help

//usage:

RSLSec eh revoke [-h] [--out OUT] [--target TARGET] [--write]

//Revoke LCS_EH, transition to LCS_CM

//optional arguments:

-h, --help show this help message and exit

--out OUT File to which the loadable package is being written

--target TARGET Target connection [RSL15]

--write Update the attached target with the given options