### BB_DEEPSLSTAT

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
31:0 | R | DEEPSLDUR | Actual duration of the last deep sleep phase measured in low_power_clk clock cycle

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
31:0 | DEEPSLDUR | DEEPSLDUR_0 | DEEPSLDUR is set to zero at the beginning of the deep sleep phase, and is incremented at each low_power_clk clock cycle until the end of the deep sleep phase. | 0x0*