## Baseband Interface Function Documentation

### Sys_BBIF_CoexIntConfig

void Sys_BBIF_CoexIntConfig(uint32_t edge, uint32_t types, uint32_t cf_ant_delay, uint32_t cf_powerup)

Configure the coexistence interrupts to monitor for Bluetooth and other RF activity.

Location: bbif.h:66

Parameters

Direction | Name | Description
--- | --- | ---
in | edge | The edge used for all coexistence interrupts; use BLE_[NONE | RISING_EDGE | FALLING_EDGE | TRANSITION]
in | types | The types of coexistence interrupts that are relevant; use BLE_RX_BUSY, BLE_TX_BUSY, BLE_IN_PROCESS, and/or EVENT_IN_PROCESS
in | cf_ant_delay | Correction factor to be applied to account for antenna delays; used to advance the coexistence interrupts by the specified number of uS.
in | cf_powerup | Correction factor to be applied to account for power-up delays on TX, RX; used to advance the coexistence interrupts by the specified number of uS.

Example Code for Sys_BBIF_CoexIntConfig
// Enable co-exsistence interrupts on BLE rising edge events and while // receiving on the BLE communication Sys_BBIF_CoexIntConfig(BLE_RISING_EDGE, BLE_RX_BUSY, 0, 0);